Checking the Network Setting of the Host Machine

| Print out this category

Checking the Network Setting of the Host Machine
Check if the IP address specified in the Host Machine is correct.
1) Select the following: [Additional Functions] > [Configuration] > [Network] > [TCP/IP Setting] > [IPv4 setting] > [IP address setting]; and write down the address in the IP address field.
2) Select the following: [Additional Functions] > [Configuration] > [Network] > [TCP/IP Setting] > [IPv4 setting] > [Ping Command]; and enter the IP address.
The IP address specified in the Host Machine is correct if the message say "Response
from the host".
If the message say "No response from the host", check the following.
NOTE:
When setting the address by manually input, set the Subnet Mask by following the
instruction of the administrator.