OPTION

| Print out this category

OPTION

SORTER>OPTION
BLNK-SW | Set Saddle Finisher fold position margin
Lv.1 | Details | To set the margin width of fold position on Saddle Finisher.
Use case | When changing the margin width of fold position
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 2 0: Normal, 1: Wider, 2: Entire image (no margin)
Default value | 2
MD-SPRTN | Restricted operation at Finisher error
Lv.1 | Details | To set whether to stop the machine when an error occurs at Finisher.
Use case | When preferring to run the machine at Finisher error occurrence
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | When "1" is set, staple operation or alignment operation is not executed. Set "0" normally.
Display/adj/set range | 0 to 1 0: Normal, 1: Restricted operation
Default value | 0
BUFF-SW | Setting Finisher buffer operation:Finisher
Lv.1 | Details | To set ON/OFF of buffer operation in the Finisher. Set 1 in case of misalignment due to charging between papers in staple mode for small size papers.
Use case | When misalignment of paper stack occurs in staple mode for small size papers
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | When the buffer operation is set to OFF, productivity decreases.
Display/adj/set range | 0 to 1 0: ON, 1: OFF
Default value | 0
PRCS-SP1 | Change of paper stack speed for buffered paper: Finisher
Lv.1 | Details | When the value is changed to 1, the paper stack speed becomes fast in the sort or staple mode.
Use case | When the alignment failure occurs in the sort or staple mode. (Paper does not reach to the process tray stopper)
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | When this mode is activated, the productivity goes down.
Display/adj/set range | 0: OFF (600mm/s) 1: ON (700mm/s) * Paper stack speed for buffered paper
Default value | 1
FDPL-SL | Set soil prev for back of Saddle:Finisher

Lv.1

Details

To set ON/OFF of the Feed Plate Engagement Solenoid at the time of Saddle stacking operation.
When 1 is set, the Intermediate Feed Roller is disengaged by turning OFF the Feed Plate Engagement Solenoid at the time of Saddle stacking operation.
Set 1 when the back of paper is soiled by the Intermediate Feed Roller. But the alignment condition of papers at the time of saddle stitching decreases.

Use case | When the back of paper is soiled due to the Intermediate Feed Roller at the time of Saddle stacking operation
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: ON (Engagement), 1: OFF (Disengagement)
Default value | 0
STCR-DWN | Set occasional misalign prev mode:Finisher
Lv.1 | Details | When misalignment in feed direction occurs at approx. every 30 sheets for thin/plain paper (105g/m2 and less), set 1.
Use case | When misalignment in feed direction occurs occasionally for thin/plain paper
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: OFF, 1: ON
Default value | 0
BUFF-INT | Ppr intvl after buffer ppr ejctn: Finisher
Lv.1 | Details | In case of paper with excessive upward curl, paper right after the buffer paper is ejected at the Finisher hits the Stack Delivery Roller, causing Saddle Delivery Sensor stationary jam. When 1 is set, the jam can be avoided since the paper intervals between the present and the following papers after the buffer paper ejection become wider.
Use case | When stationary jam occurs at the Stack Delivery Roller at buffer operation
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: OFF, 1: ON
Default value | 0
PRCS-SP3 | Change of paper stack speed for non-buffer mode: Finisher
Lv.1 | Details | When the value is changed to 1, the paper stack speed becomes slow in the non-buffer mode.
Use case | When the alignment failure occurs with the plain/thin paper. (Paper is spent to the process tray stopper more than required.)
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.

Display/adj/set range

0: 700mm/s
1: 650mm/s
2: 600mm/s
3: 550mm/s
4: 500mm/s
5: 450mm/s
6 to 8: 450mm/s

Unit | 0.49 mm
Default value | 0
NSRT-STC | Set alignment at non-sort delivery: Fin
Lv.1 | Details | To deliver to the Stack Tray after aligning only 2-sided printed paper in the Processing Tray at non-sort delivery. When 2 is set, 1-sided printed paper is also delivered via the Processing Tray, so the stacking performance improves.
Use case | When the paper delivered with non-sort mode is not appropriately stacked
Adj/set/operate method | Enter the setting value, and then press OK key.
Display/adj/set range | 0 to 2 0: Deliver directly to the Stack Tray 1: Deliver only 2-sided printed paper via the Processing Tray 2: Deliver 1-sided/2-sided printed paper via the Processing Tray
| Default value | 1