Operation Check

| Print out this category

Operation Check
Be sure to perform the following procedure for operation check of the Stamp Unit.
1) Connect the power plug of the host machine to the power outlet.
2) Turn ON the main power switch.
3) Press “Finished Stamp” key.
[Scan and Send] or [Fax] > [Other Function] > [Finished Stamp]
4)Put an original in the Feeder, perform a send test, and check that a stamp is printed on the original.