Staple Finisher-G1/Booklet Finisher-G1 + External Hole Puncher-B2

| Print out this category

Staple Finisher-G1/Booklet Finisher-G1 + External Hole Puncher-B2

ACC ID | Jam Code | Type | Sensor ID | Sensor Name/Description
02 | 1001 | DELAY | PI103 | Inlet sensor
02 | 1002 | DELAY | PCB12 | Photosensor PCB
02 | 1004 | DELAY | PI104 | Feed path sensor
02 | 1101 | STNRY | PI103 | Inlet sensor
02 | 1102 | STNRY | PCB12 | Photosensor PCB
02 | 1104 | STNRY | PI104 | Feed path sensor
02 | 1200 | EARLY | PI103 | Inlet sensor
02 | 1300 | POWER ON | PI104 | Feed path sensor
02 | 1400 | DOOR OP | - | Door open jam
02 | 1500 | STP | - | Staple jam
02 | 1604 | PUNCH | PI63 | Punch jam
02 | 1605 | POWER ON | PCB12 | Power on jam
02 | 110F | ERROR | - | Error evasion jam
02 | 1F86 | SDL STP | - | Saddle staple jam
02 | 1F87 | POWER ON | PI1, PI17, PI18, PI19, PI20, PI22 | Power on jam
02 | 1F88 | DOOR OP | - | Door open jam
02 | 1F8F | ERROR*1 | - | Error evasion jam
02 | 1F91 | DELAY | PI18 | No.1 paper sensor
02 | 1F92 | DELAY | PI11 | Delivery sensor
02 | 1F93 | DELAY | PI22 | Saddle inlet sensor
02 | 1FA1 | STNRY | PI18,PI19,PI20 | No.1/2/3 paper sensor
02 | 1FA2 | STNRY | PI11,PI17 | Delivery sensor/Vertical pat paper sensor
02 | 1FA3 | STNRY | PI22 | Saddle inlet sensor

*1: The state is recovered by opening and closing the Door, or turning OFF and then ON the power supply.
If the same jam is detected regardless of the operation above, the error code is displayed.