LASER

| Print out this category

LASER

COPIER>ADJUST>LASER
PVE-OFST | Adj of write start position of laser
Lv.1 | Details | To adjust the image position by changing the laser emitting position. When replacing the DC Controller PCB/clearing RAM data, enter the value of service label. As the value is incremented by 1, the image moves by 0.1mm. +: Toward rear -: Toward front
Adj/set/operate method | Enter the setting value (switch negative/positive by -/+ key) and press OK key.
Caution | Use this only when replacing the DC Controller PCB/Laser Scanner Unit. When adjusting the image write start position, use COPIER> ADJUST> FEED-ADJ> ADJ-C1/C2/C3/C4/MF/DK. If it is not sufficient enough, execute mechanical adjustment.
Display/adj/set range | -512 to 511
Unit | 0.1 mm
Appropriate target value | 0
Default value | 0
LA-OFF | Trailing edge OFF adjustment for the laser
Lv.1 | Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | -128 to 127
Default value | 0
POWER | Adj laser power at no potential control
Lv.1 | Details | To adjust the laser power when the potential control is not performed.
Display/adj/set range | -128 to 127
LDADJ1-K | Magnification between A-B laser (K)
Lv.1 | Details | When replacing the laser scanner unit, enter the value of service label stuck on the laser scanner unit.
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | -512 to 511
Default value | 0
LDADJ2-K | Magnification between A-C laser (K)
Lv.1 | Details | When replacing the laser scanner unit, enter the value of service label stuck on the laser scanner unit.
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | -512 to 511
Default value | 0
LDADJ3-K | Magnification between A-D laser (K)
Lv.1 | Details | When replacing the laser scanner unit, enter the value of service label stuck on the laser scanner unit.
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | -512 to 511
Default value | 0
LDADJ4-K | Phase difference between A-B laser (K)
Lv.1 | Details | When replacing the laser scanner unit, enter the value of service label stuck on the laser scanner unit.
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | -512 to 511
Default value | 0
LDADJ5-K | Phase difference between A-C laser (K)
Lv.1 | Details | When replacing the laser scanner unit, enter the value of service label stuck on the laser scanner unit.
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | -512 to 511
Default value | 0
LDADJ6-K | Phase difference between A-D laser (K)
Lv.1 | Details | When replacing the laser scanner unit, enter the value of service label stuck on the laser scanner unit.
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | -512 to 511
Default value | 0