Connection

| Print out this category

Connection
The following IP address is automatically set for this machine at start-up in Download mode.
IP address:172.16.1.100
Subnet mask:255.255.255.0
When the PC with SST installed is connected to this machine, change the PC network address to the following.
IP address:172.16.1.160
Subnet mask:255.255.255.0
Default gateway: arbitrary
CAUTION:
If the PC has the connection to the network, the settings changed to the above-mentioned may cause network failures due to redundant IP addresses, etc. Ensure that the PC is disconnected from the network when you change the PC network settings. Alternatively use the cross cable to connect the PC to this machine.
Preparation
Requirements
PC with SST Ver. 4.41 or later installed and the system software for this machine is stored
Cross cable
10Base-T: Category 3 or 5
100Base-T: Category 5
1000Base-T: Enhanced Category 5 (CAT5e) or later
CAUTION:
Disconnect USB memory storage device storage devices if connected.
Communication to SST is disabled in this machine if any USB memory storage device storage device is recognized. SST and the USB memory storage device storage device cannot be used concurrently.
Steps
1) Use the cross cable to connect the machine to the PC with SST installed.
2) Turn on the main power switch of this machine.
3) Enter Service mode to start the machine in Download mode.
Select COPIER > FUNCTION > SYSTEM > DOWNLOAD and press [OK].
4) Check the IP address of the PC.
Go to Start menu to select Program > Accessory > Command Prompt.
Type IPCONFIG and press [Return] to see the network settings of the PC.
If any discrepancies from the description in the figure below are found, change the network settings of the PC.
CAUTION:
The network settings are not shown with IPCONFIG if the PC is disconnected from the network. To check the settings, connect the PC to this machine at power-on by the cross cable.