PG

| Print out this category

TEST
PG

COPIER>TEST>PG
TYPE | Test print
Lv.1 | Details | To execute the test print.
Use case | At trouble analysis
Adj/set/operate method | Enter the setting value, and then press Start key. Test print is executed.
Caution | Be sure to return the value to 0 after the test print output.

Display/adj/set range

0 to 50
0: Normal print
1: Grid
2: 17 gradations Tbic rank 2
3: 17 gradations 600dpi (134-line screen or 141-line screen)
4: Solid white
5: Halftone (density: 80H, Tbic rank 2, without image correction)
6: Halftone (density: 80H, 134-line screen or 141-line screen, without image correction)
7: Solid black
8: Horizontal line (4 dots, 27 spaces)
9: Horizontal line (6 dots, 50 spaces)
10: Horizontal line (2 dots, 3 spaces)
11: Halftone (density: 60H, Tbic rank 2, without image correction)
12: Halftone (density: 80H, 134-line screen or 141-line screen, without image correction)
13: Halftone (density: 30H, Tbic rank 2, without image correction)
14: Halftone (density: 30H, 134-line screen or 141-line screen, without image correction)
15-43: For development
44: Fixing cleaning pattern
45-50: For development

Default value | 0
TXPH | [Not used]
PG-PICK | Setting of test print Pickup Cassette
Lv.1 | Details | To set the Pickup Cassette for test print output.
Use case | - At trouble analysis - At test print output
Adj/set/operate method | Select the item, and then press OK key.
Display/adj/set range | 1 to 8 1: Cassette 1, 2: Cassette 2, 3: Cassette 3 (Option Cassette), 4: Cassette 4 (Option Cassette), 5: Paper Deck, 6: Multi-purpose Tray, 7 to 8: Not used
2-SIDE | Setting of PG 2-sided mode
Lv.1 | Details | To set 1-sided/2-sided print for PG output.
Use case | At trouble analysis
Adj/set/operate method | Select the item, and then press OK key.
Display/adj/set range | 0 to 1 0: 1-sided, 1: 2-sided
Default value | 0
PG-QTY | Setting of PG output quantity
Lv.1 | Details | To set the number of sheets for PG output.
Use case | At trouble analysis
Display/adj/set range | 1 to 999
Unit | 1 sheet
Default value | 1
FINISH | Accessory processing function test print
Lv.1 | Details | To execute the test print relating to accessory processing func.
Use case | When checking operation of accessory processing function
Adj/set/operate method | 1) Enter the number of sheets for PG-QTY, and then press OK key. 2) Enter the setting value, and then press OK key. 3) Press Start button. The machine outputs a test print.

Display/adj/set range

0 to 99
0: N/A
1: Staple (front) *1
2: Staple (2 points) *1
3: Staple (rear) *1
4: Booklet (saddle stitch) *1
5: Z-fold (single sleeve) *1
6: 2-fold *1
7 to 10: Not used
11: Punch (Inner Puncher) *3
12: Not used
13: Not used
14 to 99: Spare (for future use)
*1 Finisher, *3 Inner Puncher

Default value | 0
Related service mode | COPIER> TEST> PG> PG-QTY