Restricted function

| Print out this category

Restricted function
The restricted function mode is activated when several specific errors are detected so the surviving functions still can operate.

Item | Copy | ADF Scan | Book Scan | Print | Finisher
Specific error in ADF | Book copy : enabled ADF copy: disabled | Disabled | Enabled | Enabled | Enabled
Specific error in Reader | Disabled | Disabled | Disabled | Enabled | Enabled
Specific error in Host machine | Disabled | Enabled | Enabled | Disabled | Disabled
Specific error in Finisher | Enabled | Enabled | Enabled | Enabled | Enabled*1

*1: Only the straight pass delivery is available. Stapling, aligning, punching are not available.
ADF restriction error code
E413
Reader restriction error code
E202, E225, E227, E248, E280, E400
Printer restriction error code
E000, E001, E002, E003, E004, E010, E014, E020, E024, E025, E110, E261, E800, E805, E806, E840
Finisher restriction error code
Staple/Booklet finisher
E514, E530, E531, E532, E535, E537, E540, E542, E590, E591, E592, E593
*E590 to E593: for the puncher unit (option).
<Related service modes>
Restricted operation at Finisher error (for Staple Finisher-G1/Booklet Finisher-G1)
(Lv.1) SORTER> OPTION> FIXING> MD-SPRTN
0: Normal, 1: Restricted operation
Inner finisher
E505-0002, E531, E551, E590, E5F3, E5F4, E5F6