PANEL

| Print out this category

PANEL

COPIER>FUNCTION>PANEL
LCD-CHK | Check of LCD Panel dot missing
Lv.1 | Details | To check whether there is a missing dot on the LCD Panel of the Control Panel.
Use case | When replacing the LCD Panel
Adj/set/operate method | 1) Select the item, and then press OK key. 2) Check that the LCD Panel lights up in the order of white, black, red, green and blue. 3) Press STOP key to terminate checking.
LED-CHK | Check of Control Panel LED
Lv.1 | Details | To check whether the LED on the Control Panel lights up.
Use case | When replacing the LCD Panel
Adj/set/operate method | 1) Select the item, and then press OK key. 2) Check that the LED lights up in the order. 3) Use LED-OFF to terminate checking.
Related service mode | COPIER> FUNCTION> PANEL> LED-OFF
LED-OFF | End check of Control Panel LED
Lv.1 | Details | To terminate the check of LED on the Control Panel.
Use case | During execution of LED-CHK
Adj/set/operate method | Select the item, and then press OK key.
Related service mode | COPIER> FUNCTION> PANEL> LED-CHK
KEY-CHK | Check of key entry
Lv.1 | Details | To check the key input on the Control Panel.
Use case | When replacing the LCD Panel
Adj/set/operate method | 1) Select the item and press the key on the Control Panel. 2) Check that the input value is displayed. 3) Cancel the selection to terminate checking.
TOUCHCHK | Adj of coordinate pstn of Touch Panel
Lv.1 | Details | To adjust the coordinate position on the Touch Panel of the Control Panel.
Use case | When replacing the LCD Panel
Adj/set/operate method | 1) Select the item, and then press OK key. 2) Press the nine ""+"" keys in sequence.