Reader (R-CON>P001 to P008)

| Print out this category

Reader (R-CON>P001 to P008)

Address | bit | Name | Symbol | Remarks
P001 | 7 | ADF Read Sensor | SR2 | 1: Paper presence
6 | Not used |  |
5 | Not used |  |
4 | Not used |  |
3 | Not used |  |
2 | Not used |  |
1 | Not used |  |
0 | For R&D use |  |
P002 | 7 | Reader Motor Rotatory Direction Change Signal | M14 | 0: CW
6 | Not used |  |
5 | Reader Motor Output Enable Signal | M14 | 1:Output stop
4 | Reader Motor Standby Signal | M14 | 0:Stop
3 | Not used |  |
2 | For R&D use |  |
1 | For R&D use |  |
0 | For R&D use |  |
P003 | 7 | Not used |  |
6 | Not used |  |
5 | Not used |  |
4 | Not used |  |
3 | Not used |  |
2 | Not used |  |
1 | Not used |  |
0 | For R&D use |  |
P004 | 7 | Not used |  |
6 | Not used |  |
5 | Not used |  |
4 | Not used |  |
3 | Not used |  |
2 | Not used |  |
1 | Not used |  |
0 | CCD Unit Flexible Cable Connection Detection Signal |  | 1: Incorrect connection
P005 | 7 | For R&D use |  |
6 | ADF Registration Sensor | SR1 | 1: Paper presence
5 | Not used |  |
4 | Not used |  |
3 | Not used |  |
2 | Not used |  |
1 | Not used |  |
0 | Not used |  |
P006 | 7 | Not used |  |
6 | For R&D use |  |
5 | For R&D use |  |
4 | Not used |  |
3 | Not used |  |
2 | For R&D use |  |
1 | Original Size Sensor | S14/15 | 1: Paper presence
0 | Not used |  |
P007 | 7 | For R&D use |  |
6 | Not used |  |
5 | Not used |  |
4 | Not used |  |
3 | Not used |  |
2 | Not used |  |
1 | Not used |  |
0 | Not used |  |
P008 | 7 | Not used |  |
6 | Not used |  |
5 | Not used |  |
4 | Not used |  |
3 | Not used |  |
2 | Not used |  |
1 | Not used |  |
0 | Not used |  |