E602 to E880

| Print out this category

E602 to E880

E Code | Detail Code | Location | Item | Description
E602 | 0001 | 00 | Title | Hard disk error
Description | HDD detection error. Unable to detect HDD, not become Ready, return an error. When the errors occur, the system of the host machine has not been started normally. Therefore the error code is not recorded in the log.
Remedy | 1. Connection of the HDD cable. 2. Reinstall the system. 3. HDD. 4. Main Controller PCB.
E602 | 0002 | 00 | Title | Hard disk error
Description | There is no startup file. There is no program for main CPU in /BOOTDEV/BOOT/ on HDD. When the errors occur, the system of the host machine has not been started normally. Therefore the error code is not recorded in the log.
Remedy | 1. Reinstall the system. 2. HDD.
E602 | 0003 | 00 | Title | Hard disk error
Description | HDD WriteAbort error. Unable to read /BOOTDEV sector on HDD.
Remedy | 1. Reinstall the system. 2. HDD.
E602 | 0006 | 00 | Title | Hard disk error
Description | There is no SubBootable for the PDL type in /BOOTDEV/BOOT. When the errors occur, the system of the host machine has not been started normally. Therefore the error code is not recorded in the log.
Remedy | 1. Reinstall the system. 2. HDD.
E602 | 0007 | 00 | Title | Hard disk error
Description | No ICC profile corresponding to PDL type exists in /BOOTDEV/PDL
Remedy | 1. Reinstall the system. 2. HDD.
E602 | 0009 | 00 | Title | Hard disk error
Description | There is no FONT file which is required when executing report print, FAX/IFAX transmission and reception, or stamp print in /BOOTDEV/BOOT.
Remedy | 1. Reinstall the system. 2. HDD.
E602 | 0012 | 00 | Title | Hard disk error
Description | The file on HDD in which the Web browser refers to is corrupted or deleted.
Remedy | 1. Reinstall the system. 2. HDD.
E602 | 0100 | 00 | Title | Hard disk error
Description | Error in /FSTDEV.
Remedy | 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0101 | 00 | Title | Hard disk error
Description | Error in /FSTDEV.
Remedy | 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0102 | 00 | Title | Hard disk error
Description | Error in /FSTDEV.
Remedy | 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0103 | 00 | Title | Hard disk error
Description | Error in /FSTDEV.
Remedy | 1. Enter the corresponding CHK-TYPE in the partition to execute HDD-CHECK (duration: several minutes to several dozen minutes); and then turn OFF and then ON the power. 2. If the measures above do not solve the problem, enter the corresponding CHK-TYPE in the partition to execute HDD-CLEAR, and then turn OFF and then ON the main power.
E602 | 0104 | 00 | Title | Hard disk error
Description | Error in /FSTDEV.
Remedy | 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0105 | 00 | Title | Hard disk error
Description | Error in /FSTDEV.
Remedy | 1. Enter the corresponding CHK-TYPE in the partition to execute HDD-CLEAR, and then turn OFF and then ON the power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0110 | 00 | Title | Hard disk error
Description | Error in /FSTDEV.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0111 | 00 | Title | Hard disk error
Description | Error in /FSTDEV.
Remedy | This is the error which usually does not occur in Read/Write level. 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0112 | 00 | Title | Hard disk error
Description | Error in /FSTDEV.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0113 | 00 | Title | Hard disk error
Description | Error in /FSTDEV.

Remedy

The document data (such as Box on the HDD) can be damaged.
1. Enter the corresponding CHK-TYPE in the partition to execute HDD-CHECK (duration: several minutes to several dozen minutes); and then turn OFF and then ON the power.
2. If the measures above do not solve the problem, enter the corresponding CHK-TYPE in the partition to execute HDD-CLEAR, and then turn OFF and then ON the main power.
(Use SST to perform reformat/reinstallation in the case of the following: BOOTDEV, BOOTDEV2 and APL_SEND)
3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.

E602 | 0114 | 00 | Title | Hard disk error
Description | Error in /FSTDEV.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0115 | 00 | Title | Hard disk error
Description | Error in /FSTDEV.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0121 | 00 | Title | Hard disk error
Description | Error in /FSTDEV.
Remedy | This is the error which usually does not occur in Read/Write level. 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0122 | 00 | Title | Hard disk error
Description | Error in /FSTDEV.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0123 | 00 | Title | Hard disk error
Description | Error in /FSTDEV.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0124 | 00 | Title | Hard disk error
Description | Error in /FSTDEV.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0125 | 00 | Title | Hard disk error
Description | Error in /FSTDEV.

Remedy

The document data (such as Box on the HDD) can be damaged.
1. Enter the corresponding CHK-TYPE in the partition to execute HDD-CHECK (duration: several minutes to several dozen minutes); and then turn OFF and then ON the power.
2. If the measures above do not solve the problem, enter the corresponding CHK-TYPE in the partition to execute HDD-CLEAR, and then turn OFF and then ON the main power.
(Use SST to perform reformat/reinstallation in the case of the following: BOOTDEV, BOOTDEV2 and APL_SEND)
3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.

E602 | 0200 | 00 | Title | Hard disk error
Description | Error in /IMG_MNG.
Remedy | 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0201 | 00 | Title | Hard disk error
Description | Error in /IMG_MNG.
Remedy | 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0202 | 00 | Title | Hard disk error
Description | Error in /IMG_MNG.
Remedy | 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0203 | 00 | Title | Hard disk error
Description | Error in /IMG_MNG.
Remedy | 1. Enter the corresponding CHK-TYPE in the partition to execute HDD-CHECK (duration: several minutes to several dozen minutes); and then turn OFF and then ON the power. 2. If the measures above do not solve the problem, enter the corresponding CHK-TYPE in the partition to execute HDD-CLEAR, and then turn OFF and then ON the main power.
E602 | 0204 | 00 | Title | Hard disk error
Description | Error in /IMG_MNG.
Remedy | 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0205 | 00 | Title | Hard disk error
Description | Error in /IMG_MNG.
Remedy | 1. Enter the corresponding CHK-TYPE in the partition to execute HDD-CLEAR, and then turn OFF and then ON the power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0210 | 00 | Title | Hard disk error
Description | Error in /IMG_MNG.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0211 | 00 | Title | Hard disk error
Description | Error in /IMG_MNG.
Remedy | This is the error which usually does not occur in Read/Write level. 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0212 | 00 | Title | Hard disk error
Description | Error in /IMG_MNG.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0213 | 00 | Title | Hard disk error
Description | Error in /IMG_MNG.

Remedy

The document data (such as Box on the HDD) can be damaged.
1. Enter the corresponding CHK-TYPE in the partition to execute HDD-CHECK (duration: several minutes to several dozen minutes); and then turn OFF and then ON the power.
2. If the measures above do not solve the problem, enter the corresponding CHK-TYPE in the partition to execute HDD-CLEAR, and then turn OFF and then ON the main power.
(Use SST to perform reformat/reinstallation in the case of the following: BOOTDEV, BOOTDEV2 and APL_SEND)
3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.

E602 | 0214 | 00 | Title | Hard disk error
Description | Error in /IMG_MNG.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0215 | 00 | Title | Hard disk error
Description | Error in /IMG_MNG.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0221 | 00 | Title | Hard disk error
Description | Error in /IMG_MNG.
Remedy | This is the error which usually does not occur in Read/Write level. 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0222 | 00 | Title | Hard disk error
Description | Error in /IMG_MNG.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0223 | 00 | Title | Hard disk error
Description | Error in /IMG_MNG.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0224 | 00 | Title | Hard disk error
Description | Error in /IMG_MNG.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0225 | 00 | Title | Hard disk error
Description | Error in /IMG_MNG.

Remedy

The document data (such as Box on the HDD) can be damaged.
1. Enter the corresponding CHK-TYPE in the partition to execute HDD-CHECK (duration: several minutes to several dozen minutes); and then turn OFF and then ON the power.
2. If the measures above do not solve the problem, enter the corresponding CHK-TYPE in the partition to execute HDD-CLEAR, and then turn OFF and then ON the main power.
(Use SST to perform reformat/reinstallation in the case of the following: BOOTDEV, BOOTDEV2 and APL_SEND)
3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.

E602 | 0300 | 00 | Title | Hard disk error
Description | Error in /IMG_MNG.
Remedy | 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0301 | 00 | Title | Hard disk error
Description | Error in /FSTCDEV.
Remedy | 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0302 | 00 | Title | Hard disk error
Description | Error in /FSTCDEV.
Remedy | 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0303 | 00 | Title | Hard disk error
Description | Error in /FSTCDEV.
Remedy | 1. Enter the corresponding CHK-TYPE in the partition to execute HDD-CHECK (duration: several minutes to several dozen minutes); and then turn OFF and then ON the power. 2. If the measures above do not solve the problem, enter the corresponding CHK-TYPE in the partition to execute HDD-CLEAR, and then turn OFF and then ON the main power.
E602 | 0304 | 00 | Title | Hard disk error
Description | Error in /FSTCDEV.
Remedy | 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0305 | 00 | Title | Hard disk error
Description | Error in /FSTCDEV.
Remedy | 1. Enter the corresponding CHK-TYPE in the partition to execute HDD-CLEAR, and then turn OFF and then ON the power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0310 | 00 | Title | Hard disk error
Description | Error in /FSTCDEV.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0311 | 00 | Title | Hard disk error
Description | Error in /FSTCDEV.
Remedy | This is the error which usually does not occur in Read/Write level. 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0312 | 00 | Title | Hard disk error
Description | Error in /FSTCDEV.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0313 | 00 | Title | Hard disk error
Description | Error in /FSTCDEV.

Remedy

The document data (such as Box on the HDD) can be damaged.
1. Enter the corresponding CHK-TYPE in the partition to execute HDD-CHECK (duration: several minutes to several dozen minutes); and then turn OFF and then ON the power.
2. If the measures above do not solve the problem, enter the corresponding CHK-TYPE in the partition to execute HDD-CLEAR, and then turn OFF and then ON the main power.
(Use SST to perform reformat/reinstallation in the case of the following: BOOTDEV, BOOTDEV2 and APL_SEND)
3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.

E602 | 0314 | 00 | Title | Hard disk error
Description | Error in /FSTCDEV.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0315 | 00 | Title | Hard disk error
Description | Error in /FSTCDEV.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0321 | 00 | Title | Hard disk error
Description | Error in /FSTCDEV.
Remedy | This is the error which usually does not occur in Read/Write level. 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0322 | 00 | Title | Hard disk error
Description | Error in /FSTCDEV.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0323 | 00 | Title | Hard disk error
Description | Error in /FSTCDEV.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0324 | 00 | Title | Hard disk error
Description | Error in /FSTCDEV.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0325 | 00 | Title | Hard disk error
Description | Error in /FSTCDEV.

Remedy

The document data (such as Box on the HDD) can be damaged.
1. Enter the corresponding CHK-TYPE in the partition to execute HDD-CHECK (duration: several minutes to several dozen minutes); and then turn OFF and then ON the power.
2. If the measures above do not solve the problem, enter the corresponding CHK-TYPE in the partition to execute HDD-CLEAR, and then turn OFF and then ON the main power.
(Use SST to perform reformat/reinstallation in the case of the following: BOOTDEV, BOOTDEV2 and APL_SEND)
3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.

E602 | 0400 | 00 | Title | Hard disk error
Description | Error in /THUMDEV.
Remedy | 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0401 | 00 | Title | Hard disk error
Description | Error in /THUMDEV.
Remedy | 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0402 | 00 | Title | Hard disk error
Description | Error in /THUMDEV.
Remedy | 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0403 | 00 | Title | Hard disk error
Description | Error in /THUMDEV.
Remedy | 1. Enter the corresponding CHK-TYPE in the partition to execute HDD-CHECK (duration: several minutes to several dozen minutes); and then turn OFF and then ON the power. 2. If the measures above do not solve the problem, enter the corresponding CHK-TYPE in the partition to execute HDD-CLEAR, and then turn OFF and then ON the main power.
E602 | 0404 | 00 | Title | Hard disk error
Description | Error in /THUMDEV.
Remedy | 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0405 | 00 | Title | Hard disk error
Description | Error in /THUMDEV.
Remedy | 1. Enter the corresponding CHK-TYPE in the partition to execute HDD-CLEAR, and then turn OFF and then ON the power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0410 | 00 | Title | Hard disk error
Description | Error in /THUMDEV.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0411 | 00 | Title | Hard disk error
Description | Error in /THUMDEV.
Remedy | This is the error which usually does not occur in Read/Write level. 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0412 | 00 | Title | Hard disk error
Description | Error in /THUMDEV.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0413 | 00 | Title | Hard disk error
Description | Error in /THUMDEV.

Remedy

The document data (such as Box on the HDD) can be damaged.
1. Enter the corresponding CHK-TYPE in the partition to execute HDD-CHECK (duration: several minutes to several dozen minutes); and then turn OFF and then ON the power.
2. If the measures above do not solve the problem, enter the corresponding CHK-TYPE in the partition to execute HDD-CLEAR, and then turn OFF and then ON the main power.
(Use SST to perform reformat/reinstallation in the case of the following: BOOTDEV, BOOTDEV2 and APL_SEND)
3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.

E602 | 0414 | 00 | Title | Hard disk error
Description | Error in /THUMDEV.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0415 | 00 | Title | Hard disk error
Description | Error in /THUMDEV.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0421 | 00 | Title | Hard disk error
Description | Error in /THUMDEV.
Remedy | This is the error which usually does not occur in Read/Write level. 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0422 | 00 | Title | Hard disk error
Description | Error in /THUMDEV.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0423 | 00 | Title | Hard disk error
Description | Error in /THUMDEV.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0424 | 00 | Title | Hard disk error
Description | Error in /THUMDEV.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0425 | 00 | Title | Hard disk error
Description | Error in /THUMDEV.

Remedy

The document data (such as Box on the HDD) can be damaged.
1. Enter the corresponding CHK-TYPE in the partition to execute HDD-CHECK (duration: several minutes to several dozen minutes); and then turn OFF and then ON the power.
2. If the measures above do not solve the problem, enter the corresponding CHK-TYPE in the partition to execute HDD-CLEAR, and then turn OFF and then ON the main power.
(Use SST to perform reformat/reinstallation in the case of the following: BOOTDEV, BOOTDEV2 and APL_SEND)
3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.

E602 | 0500 | 00 | Title | Hard disk error
Description | Error in /APL_GEN.
Remedy | 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0501 | 00 | Title | Hard disk error
Description | Error in /APL_GEN.
Remedy | 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0502 | 00 | Title | Hard disk error
Description | Error in /APL_GEN.
Remedy | 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0503 | 00 | Title | Hard disk error
Description | Error in /APL_GEN.
Remedy | 1. Enter the corresponding CHK-TYPE in the partition to execute HDD-CHECK (duration: several minutes to several dozen minutes); and then turn OFF and then ON the power. 2. If the measures above do not solve the problem, enter the corresponding CHK-TYPE in the partition to execute HDD-CLEAR, and then turn OFF and then ON the main power.
E602 | 0504 | 00 | Title | Hard disk error
Description | Error in /APL_GEN.
Remedy | 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0505 | 00 | Title | Hard disk error
Description | Error in /APL_GEN.
Remedy | 1. Enter the corresponding CHK-TYPE in the partition to execute HDD-CLEAR, and then turn OFF and then ON the power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0510 | 00 | Title | Hard disk error
Description | Error in /APL_GEN.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0511 | 00 | Title | Hard disk error
Description | Error in /APL_GEN.
Remedy | This is the error which usually does not occur in Read/Write level. 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0512 | 00 | Title | Hard disk error
Description | Error in /APL_GEN.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0513 | 00 | Title | Hard disk error
Description | Error in /APL_GEN.

Remedy

The document data (such as Box on the HDD) can be damaged.
1. Enter the corresponding CHK-TYPE in the partition to execute HDD-CHECK (duration: several minutes to several dozen minutes); and then turn OFF and then ON the power.
2. If the measures above do not solve the problem, enter the corresponding CHK-TYPE in the partition to execute HDD-CLEAR, and then turn OFF and then ON the main power.
(Use SST to perform reformat/reinstallation in the case of the following: BOOTDEV, BOOTDEV2 and APL_SEND)
3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.

E602 | 0514 | 00 | Title | Hard disk error
Description | Error in /APL_GEN.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0515 | 00 | Title | Hard disk error
Description | Error in /APL_GEN.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0521 | 00 | Title | Hard disk error
Description | Error in /APL_GEN.
Remedy | This is the error which usually does not occur in Read/Write level. 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0522 | 00 | Title | Hard disk error
Description | Error in /APL_GEN.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0523 | 00 | Title | Hard disk error
Description | Error in /APL_GEN.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0524 | 00 | Title | Hard disk error
Description | Error in /APL_GEN.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0525 | 00 | Title | Hard disk error
Description | Error in /APL_GEN.

Remedy

The document data (such as Box on the HDD) can be damaged.
1. Enter the corresponding CHK-TYPE in the partition to execute HDD-CHECK (duration: several minutes to several dozen minutes); and then turn OFF and then ON the power.
2. If the measures above do not solve the problem, enter the corresponding CHK-TYPE in the partition to execute HDD-CLEAR, and then turn OFF and then ON the main power.
(Use SST to perform reformat/reinstallation in the case of the following: BOOTDEV, BOOTDEV2 and APL_SEND)
3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.

E602 | 0600 | 00 | Title | Hard disk error
Description | Error in /TMP_GEN.
Remedy | 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0601 | 00 | Title | Hard disk error
Description | Error in /TMP_GEN.
Remedy | 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0602 | 00 | Title | Hard disk error
Description | Error in /TMP_GEN.
Remedy | 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0603 | 00 | Title | Hard disk error
Description | Error in /TMP_GEN.
Remedy | 1. Enter the corresponding CHK-TYPE in the partition to execute HDD-CHECK (duration: several minutes to several dozen minutes); and then turn OFF and then ON the power. 2. If the measures above do not solve the problem, enter the corresponding CHK-TYPE in the partition to execute HDD-CLEAR, and then turn OFF and then ON the main power.
E602 | 0604 | 00 | Title | Hard disk error
Description | Error in /TMP_GEN.
Remedy | 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0605 | 00 | Title | Hard disk error
Description | Error in /TMP_GEN.
Remedy | 1. Enter the corresponding CHK-TYPE in the partition to execute HDD-CLEAR, and then turn OFF and then ON the power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0610 | 00 | Title | Hard disk error
Description | Error in /TMP_GEN.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0611 | 00 | Title | Hard disk error
Description | Error in /TMP_GEN.
Remedy | This is the error which usually does not occur in Read/Write level. 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0612 | 00 | Title | Hard disk error
Description | Error in /TMP_GEN.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0613 | 00 | Title | Hard disk error
Description | Error in /TMP_GEN.

Remedy

The document data (such as Box on the HDD) can be damaged.
1. Enter the corresponding CHK-TYPE in the partition to execute HDD-CHECK (duration: several minutes to several dozen minutes); and then turn OFF and then ON the power.
2. If the measures above do not solve the problem, enter the corresponding CHK-TYPE in the partition to execute HDD-CLEAR, and then turn OFF and then ON the main power.
(Use SST to perform reformat/reinstallation in the case of the following: BOOTDEV, BOOTDEV2 and APL_SEND)
3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.

E602 | 0614 | 00 | Title | Hard disk error
Description | Error in /TMP_GEN.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0615 | 00 | Title | Hard disk error
Description | Error in /TMP_GEN.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0621 | 00 | Title | Hard disk error
Description | Error in /TMP_GEN.
Remedy | This is the error which usually does not occur in Read/Write level. 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0622 | 00 | Title | Hard disk error
Description | Error in /TMP_GEN.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0623 | 00 | Title | Hard disk error
Description | Error in /TMP_GEN.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0624 | 00 | Title | Hard disk error
Description | Error in /TMP_GEN.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0625 | 00 | Title | Hard disk error
Description | Error in /TMP_GEN.

Remedy

The document data (such as Box on the HDD) can be damaged.
1. Enter the corresponding CHK-TYPE in the partition to execute HDD-CHECK (duration: several minutes to several dozen minutes); and then turn OFF and then ON the power.
2. If the measures above do not solve the problem, enter the corresponding CHK-TYPE in the partition to execute HDD-CLEAR, and then turn OFF and then ON the main power.
(Use SST to perform reformat/reinstallation in the case of the following: BOOTDEV, BOOTDEV2 and APL_SEND)
3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.

E602 | 0700 | 00 | Title | Hard disk error
Description | Error in /TMP_FAX.
Remedy | 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0701 | 00 | Title | Hard disk error
Description | Error in /TMP_FAX.
Remedy | 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0702 0703 | 00 | Title | Hard disk error
Description | Error in /TMP_FAX.
Remedy | 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 00 | Title | Hard disk error
Description | Error in /TMP_FAX.
Remedy | 1. Enter the corresponding CHK-TYPE in the partition to execute HDD-CHECK (duration: several minutes to several dozen minutes); and then turn OFF and then ON the power. 2. If the measures above do not solve the problem, enter the corresponding CHK-TYPE in the partition to execute HDD-CLEAR, and then turn OFF and then ON the main power.
E602 | 0704 | 00 | Title | Hard disk error
Description | Error in /TMP_FAX.
Remedy | 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0705 | 00 | Title | Hard disk error
Description | Error in /TMP_FAX.
Remedy | 1. Enter the corresponding CHK-TYPE in the partition to execute HDD-CLEAR, and then turn OFF and then ON the power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0710 | 00 | Title | Hard disk error
Description | Error in /TMP_FAX.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0711 | 00 | Title | Hard disk error
Description | Error in /TMP_FAX.
Remedy | This is the error which usually does not occur in Read/Write level. 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0712 | 00 | Title | Hard disk error
Description | Error in /TMP_FAX.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0713 | 00 | Title | Hard disk error
Description | Error in /TMP_FAX.

Remedy

The document data (such as Box on the HDD) can be damaged.
1. Enter the corresponding CHK-TYPE in the partition to execute HDD-CHECK (duration: several minutes to several dozen minutes); and then turn OFF and then ON the power.
2. If the measures above do not solve the problem, enter the corresponding CHK-TYPE in the partition to execute HDD-CLEAR, and then turn OFF and then ON the main power.
(Use SST to perform reformat/reinstallation in the case of the following: BOOTDEV, BOOTDEV2 and APL_SEND)
3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.

E602 | 0714 | 00 | Title | Hard disk error
Description | Error in /TMP_FAX.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0715 | 00 | Title | Hard disk error
Description | Error in /TMP_FAX.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0721 | 00 | Title | Hard disk error
Description | Error in /TMP_FAX.
Remedy | This is the error which usually does not occur in Read/Write level. 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0722 | 00 | Title | Hard disk error
Description | Error in /TMP_FAX.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0723 | 00 | Title | Hard disk error
Description | Error in /TMP_FAX.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0724 | 00 | Title | Hard disk error
Description | Error in /TMP_FAX.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0725 | 00 | Title | Hard disk error
Description | Error in /TMP_FAX.

Remedy

The document data (such as Box on the HDD) can be damaged.
1. Enter the corresponding CHK-TYPE in the partition to execute HDD-CHECK (duration: several minutes to several dozen minutes); and then turn OFF and then ON the power.
2. If the measures above do not solve the problem, enter the corresponding CHK-TYPE in the partition to execute HDD-CLEAR, and then turn OFF and then ON the main power.
(Use SST to perform reformat/reinstallation in the case of the following: BOOTDEV, BOOTDEV2 and APL_SEND)
3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.

E602 | 0800 | 00 | Title | Hard disk error
Description | Error in /TMP_PSS.
Remedy | 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0801 | 00 | Title | Hard disk error
Description | Error in /TMP_PSS.
Remedy | 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0802 | 00 | Title | Hard disk error
Description | Error in /TMP_PSS.
Remedy | 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0803 | 00 | Title | Hard disk error
Description | Error in /TMP_PSS.
Remedy | 1. Enter the corresponding CHK-TYPE in the partition to execute HDD-CHECK (duration: several minutes to several dozen minutes); and then turn OFF and then ON the power. 2. If the measures above do not solve the problem, enter the corresponding CHK-TYPE in the partition to execute HDD-CLEAR, and then turn OFF and then ON the main power.
E602 | 0804 | 00 | Title | Hard disk error
Description | Error in /TMP_PSS.
Remedy | 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0805 | 00 | Title | Hard disk error
Description | Error in /TMP_PSS.
Remedy | 1. Enter the corresponding CHK-TYPE in the partition to execute HDD-CLEAR, and then turn OFF and then ON the power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0810 | 00 | Title | Hard disk error
Description | Error in /TMP_PSS.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0811 | 00 | Title | Hard disk error
Description | Error in /TMP_PSS.
Remedy | This is the error which usually does not occur in Read/Write level. 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0812 | 00 | Title | Hard disk error
Description | Error in /TMP_PSS.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0813 | 00 | Title | Hard disk error
Description | Error in /TMP_PSS.

Remedy

The document data (such as Box on the HDD) can be damaged.
1. Enter the corresponding CHK-TYPE in the partition to execute HDD-CHECK (duration: several minutes to several dozen minutes); and then turn OFF and then ON the power.
2. If the measures above do not solve the problem, enter the corresponding CHK-TYPE in the partition to execute HDD-CLEAR, and then turn OFF and then ON the main power.
(Use SST to perform reformat/reinstallation in the case of the following: BOOTDEV, BOOTDEV2 and APL_SEND)
3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.

E602 | 0814 | 00 | Title | Hard disk error
Description | Error in /TMP_PSS.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0815 | 00 | Title | Hard disk error
Description | Error in /TMP_PSS.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0821 | 00 | Title | Hard disk error
Description | Error in /TMP_PSS.
Remedy | This is the error which usually does not occur in Read/Write level. 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0822 | 00 | Title | Hard disk error
Description | Error in /TMP_PSS.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0823 | 00 | Title | Hard disk error
Description | Error in /TMP_PSS.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0824 | 00 | Title | Hard disk error
Description | Error in /TMP_PSS.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0825 | 00 | Title | Hard disk error
Description | Error in /TMP_PSS.

Remedy

The document data (such as Box on the HDD) can be damaged.
1. Enter the corresponding CHK-TYPE in the partition to execute HDD-CHECK (duration: several minutes to several dozen minutes); and then turn OFF and then ON the power.
2. If the measures above do not solve the problem, enter the corresponding CHK-TYPE in the partition to execute HDD-CLEAR, and then turn OFF and then ON the main power.
(Use SST to perform reformat/reinstallation in the case of the following: BOOTDEV, BOOTDEV2 and APL_SEND)
3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.

E602 | 0900 | 00 | Title | Hard disk error
Description | Error in /PDLDEV.
Remedy | 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0901 | 00 | Title | Hard disk error
Description | Error in /PDLDEV.
Remedy | 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0902 | 00 | Title | Hard disk error
Description | Error in /PDLDEV.
Remedy | 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0903 | 00 | Title | Hard disk error
Description | Error in /PDLDEV.
Remedy | Recovery of Boot partition must be executed in Safe Mode using SST. 1. Execute HDD-CHECK (duration: several dozen minutes) with CHK-TYPE = 0, and then turn OFF and then ON the power. 2. If the measures above do not solve the problem, move to the download mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power.
E602 | 0904 | 00 | Title | Hard disk error
Description | Error in /PDLDEV.
Remedy | 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0905 | 00 | Title | Hard disk error
Description | Error in /PDLDEV.
Remedy | Recovery of Boot partition must be executed in Safe Mode using SST. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0910 | 00 | Title | Hard disk error
Description | Error in /PDLDEV.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0911 | 00 | Title | Hard disk error
Description | Error in /PDLDEV.
Remedy | This is the error which usually does not occur in Read/Write level. 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0912 | 00 | Title | Hard disk error
Description | Error in /PDLDEV.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0913 | 00 | Title | Hard disk error
Description | Error in /PDLDEV.

Remedy

The document data (such as Box on the HDD) can be damaged.
1. Enter the corresponding CHK-TYPE in the partition to execute HDD-CHECK (duration: several minutes to several dozen minutes); and then turn OFF and then ON the power.
2. If the measures above do not solve the problem, enter the corresponding CHK-TYPE in the partition to execute HDD-CLEAR, and then turn OFF and then ON the main power.
(Use SST to perform reformat/reinstallation in the case of the following: BOOTDEV, BOOTDEV2 and APL_SEND)
3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.

E602 | 0914 | 00 | Title | Hard disk error
Description | Error in /PDLDEV.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0915 | 00 | Title | Hard disk error
Description | Error in /PDLDEV.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0921 | 00 | Title | Hard disk error
Description | Error in /PDLDEV.
Remedy | This is the error which usually does not occur in Read/Write level. 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0922 | 00 | Title | Hard disk error
Description | Error in /PDLDEV.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0923 | 00 | Title | Hard disk error
Description | Error in /PDLDEV.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0924 | 00 | Title | Hard disk error
Description | Error in /PDLDEV.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 0925 | 00 | Title | Hard disk error
Description | Error in /PDLDEV.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1000 | 00 | Title | Hard disk error
Description | Error in /BOOTDEV.
Remedy | 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1001 | 00 | Title | Hard disk error
Description | Error in /BOOTDEV.
Remedy | 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1002 | 00 | Title | Hard disk error
Description | Error in /BOOTDEV.
Remedy | 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1003 | 00 | Title | Hard disk error
Description | Error in /BOOTDEV.
Remedy | 1. Enter the corresponding CHK-TYPE in the partition to execute HDD-CHECK (duration: several minutes to several dozen minutes); and then turn OFF and then ON the power. 2. If the measures above do not solve the problem, enter the corresponding CHK-TYPE in the partition to execute HDD-CLEAR, and then turn OFF and then ON the main power.
E602 | 1004 | 00 | Title | Hard disk error
Description | Error in /BOOTDEV.
Remedy | 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1005 | 00 | Title | Hard disk error
Description | Error in /BOOTDEV.
Remedy | 1. Enter the corresponding CHK-TYPE in the partition to execute HDD-CLEAR, and then turn OFF and then ON the power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1010 | 00 | Title | Hard disk error
Description | Error in /BOOTDEV.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1011 | 00 | Title | Hard disk error
Description | Error in /BOOTDEV.
Remedy | This is the error which usually does not occur in Read/Write level. 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1012 | 00 | Title | Hard disk error
Description | Error in /BOOTDEV.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1013 | 00 | Title | Hard disk error
Description | Error in /BOOTDEV.

Remedy

The document data (such as Box on the HDD) can be damaged.
1. Enter the corresponding CHK-TYPE in the partition to execute HDD-CHECK (duration: several minutes to several dozen minutes); and then turn OFF and then ON the power.
2. If the measures above do not solve the problem, enter the corresponding CHK-TYPE in the partition to execute HDD-CLEAR, and then turn OFF and then ON the main power.
(Use SST to perform reformat/reinstallation in the case of the following: BOOTDEV, BOOTDEV2 and APL_SEND)
3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.

E602 | 1014 | 00 | Title | Hard disk error
Description | Error in /BOOTDEV.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1015 | 00 | Title | Hard disk error
Description | Error in /BOOTDEV.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1021 | 00 | Title | Hard disk error
Description | Error in /BOOTDEV.
Remedy | This is the error which usually does not occur in Read/Write level. 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1022 | 00 | Title | Hard disk error
Description | Error in /BOOTDEV.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1023 | 00 | Title | Hard disk error
Description | Error in /BOOTDEV.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1024 | 00 | Title | Hard disk error
Description | Error in /BOOTDEV.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1025 | 00 | Title | Hard disk error
Description | Error in /BOOTDEV.

Remedy

The document data (such as Box on the HDD) can be damaged.
1. Enter the corresponding CHK-TYPE in the partition to execute HDD-CHECK (duration: several minutes to several dozen minutes); and then turn OFF and then ON the power.
2. If the measures above do not solve the problem, enter the corresponding CHK-TYPE in the partition to execute HDD-CLEAR, and then turn OFF and then ON the main power.
(Use SST to perform reformat/reinstallation in the case of the following: BOOTDEV, BOOTDEV2 and APL_SEND)
3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.

E602 | 1100 | 00 | Title | Hard disk error
Description | Error in /APL_MEAP.
Remedy | 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1101 | 00 | Title | Hard disk error
Description | Error in /APL_MEAP.
Remedy | 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1102 | 00 | Title | Hard disk error
Description | Error in /APL_MEAP.
Remedy | 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1103 | 00 | Title | Hard disk error
Description | Error in /APL_MEAP.

Remedy

1. If possible, ask the customer to retrieve the data in the Address Book from the remote UI.
2. Enter the corresponding CHK-TYPE in the partition to execute HDD-CHECK (duration: several minutes to several dozen minutes); and then turn OFF and then ON the power.
3. If the measures above do not solve the problem, move to the download mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power.

E602 | 1104 | 00 | Title | Hard disk error
Description | Error in /APL_MEAP.
Remedy | 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1105 | 00 | Title | Hard disk error
Description | Error in /APL_MEAP.
Remedy | 1. Enter the corresponding CHK-TYPE in the partition to execute HDD-CLEAR, and then turn OFF and then ON the power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1110 | 00 | Title | Hard disk error
Description | Error in /APL_MEAP.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1111 | 00 | Title | Hard disk error
Description | Error in /APL_MEAP.
Remedy | This is the error which usually does not occur in Read/Write level. 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1112 | 00 | Title | Hard disk error
Description | Error in /APL_MEAP.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1113 | 00 | Title | Hard disk error
Description | Error in /APL_MEAP.

Remedy

The document data (such as Box on the HDD) can be damaged.
1. Enter the corresponding CHK-TYPE in the partition to execute HDD-CHECK (duration: several minutes to several dozen minutes); and then turn OFF and then ON the power.
2. If the measures above do not solve the problem, enter the corresponding CHK-TYPE in the partition to execute HDD-CLEAR, and then turn OFF and then ON the main power.
(Use SST to perform reformat/reinstallation in the case of the following: BOOTDEV, BOOTDEV2 and APL_SEND)
3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.

E602 | 1114 | 00 | Title | Hard disk error
Description | Error in /APL_MEAP.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1115 | 00 | Title | Hard disk error
Description | Error in /APL_MEAP.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1121 | 00 | Title | Hard disk error
Description | Error in /APL_MEAP.
Remedy | This is the error which usually does not occur in Read/Write level. 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1122 | 00 | Title | Hard disk error
Description | Error in /APL_MEAP.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1123 | 00 | Title | Hard disk error
Description | Error in /APL_MEAP.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1124 | 00 | Title | Hard disk error
Description | Error in /APL_MEAP.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1125 | 00 | Title | Hard disk error
Description | Error in /APL_MEAP.

Remedy

The document data (such as Box on the HDD) can be damaged.
1. Enter the corresponding CHK-TYPE in the partition to execute HDD-CHECK (duration: several minutes to several dozen minutes); and then turn OFF and then ON the power.
2. If the measures above do not solve the problem, enter the corresponding CHK-TYPE in the partition to execute HDD-CLEAR, and then turn OFF and then ON the main power.
(Use SST to perform reformat/reinstallation in the case of the following: BOOTDEV, BOOTDEV2 and APL_SEND)
3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.

E602 | 1200 | 00 | Title | Hard disk error
Description | Error in /APL_SEND.
Remedy | 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1201 | 00 | Title | Hard disk error
Description | Error in /APL_SEND.
Remedy | 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1202 | 00 | Title | Hard disk error
Description | Error in /APL_SEND.
Remedy | 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1203 | 00 | Title | Hard disk error
Description | Error in /APL_SEND.
Remedy | Recovery of Boot partition must be executed in Safe Mode using SST. 1. Execute HDD-CHECK (duration: several dozen minutes) with CHK-TYPE = 0, and then turn OFF and then ON the power. 2. If the measures above do not solve the problem, move to the download mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power.
E602 | 1204 | 00 | Title | Hard disk error
Description | Error in /APL_SEND.
Remedy | 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1205 | 00 | Title | Hard disk error
Description | Error in /APL_SEND.
Remedy | Recovery of Boot partition must be executed in Safe Mode using SST. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1210 | 00 | Title | Hard disk error
Description | Error in /APL_SEND.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1211 | 00 | Title | Hard disk error
Description | Error in /APL_SEND.
Remedy | This is the error which usually does not occur in Read/Write level. 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1212 | 00 | Title | Hard disk error
Description | Error in /APL_SEND.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1213 | 00 | Title | Hard disk error
Description | Error in /APL_SEND.

Remedy

The document data (such as Box on the HDD) can be damaged.
1. Enter the corresponding CHK-TYPE in the partition to execute HDD-CHECK (duration: several minutes to several dozen minutes); and then turn OFF and then ON the power.
2. If the measures above do not solve the problem, enter the corresponding CHK-TYPE in the partition to execute HDD-CLEAR, and then turn OFF and then ON the main power.
(Use SST to perform reformat/reinstallation in the case of the following: BOOTDEV, BOOTDEV2 and APL_SEND)
3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.

E602 | 1214 | 00 | Title | Hard disk error
Description | Error in /APL_SEND.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1215 | 00 | Title | Hard disk error
Description | Error in /APL_SEND.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1221 | 00 | Title | Hard disk error
Description | Error in /APL_SEND.
Remedy | This is the error which usually does not occur in Read/Write level. 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1222 | 00 | Title | Hard disk error
Description | Error in /APL_SEND.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1223 | 00 | Title | Hard disk error
Description | Error in /APL_SEND.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1224 | 00 | Title | Hard disk error
Description | Error in /APL_SEND.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1225 | 00 | Title | Hard disk error
Description | Error in /APL_SEND.

Remedy

The document data (such as Box on the HDD) can be damaged.
1. Enter the corresponding CHK-TYPE in the partition to execute HDD-CHECK (duration: several minutes to several dozen minutes); and then turn OFF and then ON the power.
2. If the measures above do not solve the problem, enter the corresponding CHK-TYPE in the partition to execute HDD-CLEAR, and then turn OFF and then ON the main power.
(Use SST to perform reformat/reinstallation in the case of the following: BOOTDEV, BOOTDEV2 and APL_SEND)
3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.

E602 | 1300 | 00 | Title | Hard disk error
Description | Error in /APL_KEEP.
Remedy | 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1301 | 00 | Title | Hard disk error
Description | Error in /APL_KEEP.
Remedy | 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1302 | 00 | Title | Hard disk error
Description | Error in /APL_KEEP.
Remedy | 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1303 | 00 | Title | Hard disk error
Description | Error in /APL_KEEP.
Remedy | 1. Enter the corresponding CHK-TYPE in the partition to execute HDD-CHECK (duration: several minutes to several dozen minutes); and then turn OFF and then ON the power. 2. If the measures above do not solve the problem, enter the corresponding CHK-TYPE in the partition to execute HDD-CLEAR, and then turn OFF and then ON the main power.
E602 | 1304 | 00 | Title | Hard disk error
Description | Error in /APL_KEEP.
Remedy | 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1305 | 00 | Title | Hard disk error
Description | Error in /APL_KEEP.
Remedy | 1. Enter the corresponding CHK-TYPE in the partition to execute HDD-CLEAR, and then turn OFF and then ON the power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1310 | 00 | Title | Hard disk error
Description | Error in /APL_KEEP.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1311 | 00 | Title | Hard disk error
Description | Error in /APL_KEEP.
Remedy | This is the error which usually does not occur in Read/Write level. 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1312 | 00 | Title | Hard disk error
Description | Error in /APL_KEEP.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1313 | 00 | Title | Hard disk error
Description | Error in /APL_KEEP.

Remedy

The document data (such as Box on the HDD) can be damaged.
1. Enter the corresponding CHK-TYPE in the partition to execute HDD-CHECK (duration: several minutes to several dozen minutes); and then turn OFF and then ON the power.
2. If the measures above do not solve the problem, enter the corresponding CHK-TYPE in the partition to execute HDD-CLEAR, and then turn OFF and then ON the main power.
(Use SST to perform reformat/reinstallation in the case of the following: BOOTDEV, BOOTDEV2 and APL_SEND)
3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.

E602 | 1314 | 00 | Title | Hard disk error
Description | Error in /APL_KEEP.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1315 | 00 | Title | Hard disk error
Description | Error in /APL_KEEP.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1321 | 00 | Title | Hard disk error
Description | Error in /APL_KEEP.
Remedy | This is the error which usually does not occur in Read/Write level. 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1322 | 00 | Title | Hard disk error
Description | Error in /APL_KEEP.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1323 | 00 | Title | Hard disk error
Description | Error in /APL_KEEP.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1324 | 00 | Title | Hard disk error
Description | Error in /APL_KEEP.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1325 | 00 | Title | Hard disk error
Description | Error in /APL_KEEP.

Remedy

The document data (such as Box on the HDD) can be damaged.
1. Enter the corresponding CHK-TYPE in the partition to execute HDD-CHECK (duration: several minutes to several dozen minutes); and then turn OFF and then ON the power.
2. If the measures above do not solve the problem, enter the corresponding CHK-TYPE in the partition to execute HDD-CLEAR, and then turn OFF and then ON the main power.
(Use SST to perform reformat/reinstallation in the case of the following: BOOTDEV, BOOTDEV2 and APL_SEND)
3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.

E602 | 1400 | 00 | Title | Hard disk error
Description | Error in /APL_LOG.
Remedy | 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1401 | 00 | Title | Hard disk error
Description | Error in /APL_LOG.
Remedy | 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1402 | 00 | Title | Hard disk error
Description | Error in /APL_LOG.
Remedy | 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1403 | 00 | Title | Hard disk error
Description | Error in /APL_LOG.
Remedy | 1. Enter the corresponding CHK-TYPE in the partition to execute HDD-CHECK (duration: several minutes to several dozen minutes); and then turn OFF and then ON the power. 2. If the measures above do not solve the problem, enter the corresponding CHK-TYPE in the partition to execute HDD-CLEAR, and then turn OFF and then ON the main power.
E602 | 1404 | 00 | Title | Hard disk error
Description | Error in /APL_LOG.
Remedy | 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1405 | 00 | Title | Hard disk error
Description | Error in /APL_LOG.
Remedy | 1. Enter the corresponding CHK-TYPE in the partition to execute HDD-CLEAR, and then turn OFF and then ON the power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1410 | 00 | Title | Hard disk error
Description | Error in /APL_LOG.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1411 | 00 | Title | Hard disk error
Description | Error in /APL_LOG.
Remedy | This is the error which usually does not occur in Read/Write level. 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1412 | 00 | Title | Hard disk error
Description | Error in /APL_LOG.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1413 | 00 | Title | Hard disk error
Description | Error in /APL_LOG.

Remedy

The document data (such as Box on the HDD) can be damaged.
1. Enter the corresponding CHK-TYPE in the partition to execute HDD-CHECK (duration: several minutes to several dozen minutes); and then turn OFF and then ON the power.
2. If the measures above do not solve the problem, enter the corresponding CHK-TYPE in the partition to execute HDD-CLEAR, and then turn OFF and then ON the main power.
(Use SST to perform reformat/reinstallation in the case of the following: BOOTDEV, BOOTDEV2 and APL_SEND)
3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.

E602 | 1414 | 00 | Title | Hard disk error
Description | Error in /APL_LOG.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1415 | 00 | Title | Hard disk error
Description | Error in /APL_LOG.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1421 | 00 | Title | Hard disk error
Description | Error in /APL_LOG.
Remedy | This is the error which usually does not occur in Read/Write level. 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1422 | 00 | Title | Hard disk error
Description | Error in /APL_LOG.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1423 | 00 | Title | Hard disk error
Description | Error in /APL_LOG.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1424 | 00 | Title | Hard disk error
Description | Error in /APL_LOG.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1425 | 00 | Title | Hard disk error
Description | Error in /APL_LOG.

Remedy

The document data (such as Box on the HDD) can be damaged.
1. Enter the corresponding CHK-TYPE in the partition to execute HDD-CHECK (duration: several minutes to several dozen minutes); and then turn OFF and then ON the power.
2. If the measures above do not solve the problem, enter the corresponding CHK-TYPE in the partition to execute HDD-CLEAR, and then turn OFF and then ON the main power.
(Use SST to perform reformat/reinstallation in the case of the following: BOOTDEV, BOOTDEV2 and APL_SEND)
3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.

E602 | 1500 | 00 | Title | Hard disk error
Description | Error in /CRBDEV.
Remedy | 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1501 | 00 | Title | Hard disk error
Description | Error in /CRBDEV.
Remedy | 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1502 | 00 | Title | Hard disk error
Description | Error in /CRBDEV.
Remedy | 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1503 | 00 | Title | Hard disk error
Description | Error in /CRBDEV.
Remedy | 1. Enter the corresponding CHK-TYPE in the partition to execute HDD-CHECK (duration: several minutes to several dozen minutes); and then turn OFF and then ON the power. 2. If the measures above do not solve the problem, enter the corresponding CHK-TYPE in the partition to execute HDD-CLEAR, and then turn OFF and then ON the main power.
E602 | 1504 | 00 | Title | Hard disk error
Description | Error in /CRBDEV.
Remedy | 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1505 | 00 | Title | Hard disk error
Description | Error in /CRBDEV.
Remedy | 1. Enter the corresponding CHK-TYPE in the partition to execute HDD-CLEAR, and then turn OFF and then ON the power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1510 | 00 | Title | Hard disk error
Description | Error in /CRBDEV.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1511 | 00 | Title | Hard disk error
Description | Error in /CRBDEV.
Remedy | This is the error which usually does not occur in Read/Write level. 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1512 | 00 | Title | Hard disk error
Description | Error in /CRBDEV.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1513 | 00 | Title | Hard disk error
Description | Error in /CRBDEV.

Remedy

The document data (such as Box on the HDD) can be damaged.
1. Enter the corresponding CHK-TYPE in the partition to execute HDD-CHECK (duration: several minutes to several dozen minutes); and then turn OFF and then ON the power.
2. If the measures above do not solve the problem, enter the corresponding CHK-TYPE in the partition to execute HDD-CLEAR, and then turn OFF and then ON the main power.
(Use SST to perform reformat/reinstallation in the case of the following: BOOTDEV, BOOTDEV2 and APL_SEND)
3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.

E602 | 1514 | 00 | Title | Hard disk error
Description | Error in /CRBDEV.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1515 | 00 | Title | Hard disk error
Description | Error in /CRBDEV.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1521 | 00 | Title | Hard disk error
Description | Error in /CRBDEV.
Remedy | This is the error which usually does not occur in Read/Write level. 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1522 | 00 | Title | Hard disk error
Description | Error in /CRBDEV.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1523 | 00 | Title | Hard disk error
Description | Error in /CRBDEV.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1524 | 00 | Title | Hard disk error
Description | Error in /CRBDEV.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1525 | 00 | Title | Hard disk error
Description | Error in /CRBDEV.

Remedy

The document data (such as Box on the HDD) can be damaged.
1. Enter the corresponding CHK-TYPE in the partition to execute HDD-CHECK (duration: several minutes to several dozen minutes); and then turn OFF and then ON the power.
2. If the measures above do not solve the problem, enter the corresponding CHK-TYPE in the partition to execute HDD-CLEAR, and then turn OFF and then ON the main power.
(Use SST to perform reformat/reinstallation in the case of the following: BOOTDEV, BOOTDEV2 and APL_SEND)
3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.

E602 | 1600 | 00 | Title | Hard disk error
Description | Error in /APL_CDS.
Remedy | 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1601 | 00 | Title | Hard disk error
Description | Error in /APL_CDS.
Remedy | 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1602 | 00 | Title | Hard disk error
Description | Error in /APL_CDS.
Remedy | 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1603 | 00 | Title | Hard disk error
Description | Error in /APL_CDS.
Remedy | 1. Enter the corresponding CHK-TYPE in the partition to execute HDD-CHECK (duration: several minutes to several dozen minutes); and then turn OFF and then ON the power. 2. If the measures above do not solve the problem, enter the corresponding CHK-TYPE in the partition to execute HDD-CLEAR, and then turn OFF and then ON the main power.
E602 | 1604 | 00 | Title | Hard disk error
Description | Error in /APL_CDS.
Remedy | 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1605 | 00 | Title | Hard disk error
Description | Error in /APL_CDS.
Remedy | 1. Enter the corresponding CHK-TYPE in the partition to execute HDD-CLEAR, and then turn OFF and then ON the power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1610 | 00 | Title | Hard disk error
Description | Error in /APL_CDS.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1611 | 00 | Title | Hard disk error
Description | Error in /APL_CDS.
Remedy | This is the error which usually does not occur in Read/Write level. 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1612 | 00 | Title | Hard disk error
Description | Error in /APL_CDS.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 3. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1613 | 00 | Title | Hard disk error
Description | Error in /APL_CDS.

Remedy

The document data (such as Box on the HDD) can be damaged.
1. Enter the corresponding CHK-TYPE in the partition to execute HDD-CHECK (duration: several minutes to several dozen minutes); and then turn OFF and then ON the power.
2. If the measures above do not solve the problem, enter the corresponding CHK-TYPE in the partition to execute HDD-CLEAR, and then turn OFF and then ON the main power.
(Use SST to perform reformat/reinstallation in the case of the following: BOOTDEV, BOOTDEV2 and APL_SEND)
3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.

E602 | 1614 | 00 | Title | Hard disk error
Description | Error in /APL_CDS.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 3. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1615 | 00 | Title | Hard disk error
Description | Error in /APL_CDS.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 3. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1621 | 00 | Title | Hard disk error
Description | Error in /APL_CDS.
Remedy | This is the error which usually does not occur in Read/Write level. 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1622 | 00 | Title | Hard disk error
Description | Error in /APL_CDS.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1623 | 00 | Title | Hard disk error
Description | Error in /APL_CDS.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1624 | 00 | Title | Hard disk error
Description | Error in /APL_CDS.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | 1625 | 00 | Title | Hard disk error
Description | Error in /APL_CDS.

Remedy

The document data (such as Box on the HDD) can be damaged.
1. Enter the corresponding CHK-TYPE in the partition to execute HDD-CHECK (duration: several minutes to several dozen minutes); and then turn OFF and then ON the power.
2. If the measures above do not solve the problem, enter the corresponding CHK-TYPE in the partition to execute HDD-CLEAR, and then turn OFF and then ON the main power.
(Use SST to perform reformat/reinstallation in the case of the following: BOOTDEV, BOOTDEV2 and APL_SEND)
3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.

E602 | 2000 | 00 | Title | Authentication error between Host Machine and Encryption Board
Description | Authentication error between Host Machine and Encryption Board.
Remedy | 1. Connection error between the Encryption Board and the Main Controller PCB (turn OFF and then ON the power). 2. Execute the key clear of the Encryption Board using SST (at this time, HDD becomes unformatted; thus, it is necessary to execute HDD format and system reinstallation).
E602 | 2001 | 00 | Title | Discrepancy in the Encryption Board operation
Description | Although the Host Machine does not have the authentication information of the Encryption Board, the authenticated Encryption Board is installed.
Remedy | Although the Host Machine does not have the authentication information of the Encryption Board, the authenticated Encryption Board is installed.
E602 | 2002 | 00 | Title | Failure of Encryption Board, others
Description | Failure of Encryption Board, others.

Remedy

1. Connection error between the Encryption Board and the Main Controller PCB (turn Off and then ON the power).
2. Execute the key clear of the Encryption Board using SST (at this time, HDD becomes unformatted; thus, it is necessary to execute HDD format and system reinstallation).
3. After replacing the Encryption Board, execute HDD format and system reinstallation using SST.
4. Main Controller PCB.

E602 | 4000 | 00 | Title | OS startup error
Description | Unable to install OS. When the errors occur, the system of the host machine has not been started normally. Therefore the error code is not recorded in the log.
Remedy | 1. Cable connection error. 2. After HDD All Format, reinstall the system software. 3. HDD.
E602 | 4001 | 00 | Title | OS startup error
Description | No OS startup script. When the errors occur, the system of the host machine has not been started normally. Therefore the error code is not recorded in the log.
Remedy | 1. Cable connection error. 2. After HDD All Format, reinstall the system software. 3. HDD.
E602 | FF00 | 00 | Title | Hard disk error
Description | Unidentified partition error.
Remedy | 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | FF01 | 00 | Title | Hard disk error
Description | Unidentified partition error.
Remedy | 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | FF02 | 00 | Title | Hard disk error
Description | Unidentified partition error.
Remedy | 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | FF03 | 00 | Title | Hard disk error
Description | Unidentified partition error.
Remedy | 1. Execute HDD-CHECK (duration: several dozen minutes) with CHK-TYPE = 0, and then turn OFF and then ON the power. 2. If the measures above do not solve the problem, execute HDD-CLEAR with CHK-TYPE = 1, 2, 3, 5, and then turn OFF and then ON the power.
E602 | FF04 | 00 | Title | Hard disk error
Description | Unidentified partition error.
Remedy | 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | FF05 | 00 | Title | Hard disk error
Description | Unidentified partition error.
Remedy | This is the error which does not occur usually. 1. Execute HDD-CLEAR with CHK-TYPE = 1, 2, 3, 5, and then turn OFF and then ON the power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | FF10 | 00 | Title | Hard disk error
Description | Unidentified partition error.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | FF11 | 00 | Title | Hard disk error
Description | Unidentified partition error.
Remedy | This is the error which usually does not occur in Read/Write level. 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | FF12 | 00 | Title | Hard disk error
Description | Unidentified partition error.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | FF13 | 00 | Title | Hard disk error
Description | Unidentified partition error.

Remedy

The document data (such as Box on the HDD) can be damaged.
1. Enter the corresponding CHK-TYPE in the partition to execute HDD-CHECK (duration: several minutes to several dozen minutes); and then turn OFF and then ON the power.
2. If the measures above do not solve the problem, enter the corresponding CHK-TYPE in the partition to execute HDD-CLEAR, and then turn OFF and then ON the main power.
(Use SST to perform reformat/reinstallation in the case of the following: BOOTDEV, BOOTDEV2 and APL_SEND)
3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.

E602 | FF14 | 00 | Title | Hard disk error
Description | Unidentified partition error.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | FF15 | 00 | Title | Hard disk error
Description | Unidentified partition error.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | FF21 | 00 | Title | Hard disk error
Description | Unidentified partition error.
Remedy | This is the error which usually does not occur in Read/Write level. 1. Check the Cable and Power Connector. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | FF22 | 00 | Title | Hard disk error
Description | Unidentified partition error.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | FF23 | 00 | Title | Hard disk error
Description | Unidentified partition error.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | FF24 | 00 | Title | Hard disk error
Description | Unidentified partition error.
Remedy | Error due to data corruption or software bug. 1. Start up in Safe Mode to perform All Format using SST and reinstall the system (SYSTEM, LANGUAGE, RUI), and then turn OFF and then ON the main power. 2. If the measures above do not solve the problem, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system.
E602 | FF25 | 00 | Title | Hard disk error
Description | Unidentified partition error.

Remedy

"The document data (such as Box on the HDD) can be damaged.
1. Enter the corresponding CHK-TYPE in the partition to execute HDD-CHECK (duration: several minutes to several dozen minutes); and then turn OFF and then ON the power.
2. If the measures above do not solve the problem, enter the corresponding CHK-TYPE in the partition to execute HDD-CLEAR, and then turn OFF and then ON the main power.
(Use SST to perform reformat/reinstallation in the case of the following: BOOTDEV, BOOTDEV2 and APL_SEND)
3. If the error still remains, it can be caused by HDD failure; therefore, replace the HDD and reinstall the system."

E604 | 0000 | 00 | Title | Insufficient memory
Description | Insufficient memory (require 1024 MB).
Remedy | DDR2-SDRAM
E609 | 0008 | 00 | Title | Insufficient memory
Description | Temperature of the HDD does not rise to the specified temperature within the specified period of time at the time of startup.
Remedy | HDD.
E609 | 0009 | 00 | Title | Hard disk error
Description | At the time of recovery from sleep, it does not reach to the specified temperature.
Remedy | HDD.
E610 | 0001 | 00 | Title | Failure of the HDD encryption key (hardware configuration error/initialization error/encryption key error/encryption processing error)
Description | The Encryption Board does not exist.
Remedy | Check the hardware configuration.
E610 | 0002 | 00 | Title | Failure of the HDD encryption key (hardware configuration error/initialization error/encryption key error/encryption processing error)
Description | Not meeting the memory configuration to execute encryption operation.
Remedy | Check the hardware configuration.
E610 | 0101 | 00 | Title | Failure of the HDD encryption key (hardware configuration error/initialization error/encryption key error/encryption processing error)
Description | Failed to initialize the memory of key storage area.
Remedy | Turn OFF and then ON the power.
E610 | 0102 | 00 | Title | Failure of the HDD encryption key (hardware configuration error/initialization error/encryption key error/encryption processing error)
Description | Failed to initialize the encryption processing part.
Remedy | Turn OFF and then ON the power.
E610 | 0201 | 00 | Title | Failure of the HDD encryption key (hardware configuration error/initialization error/encryption key error/encryption processing error)
Description | Error in the encryption processing part.
Remedy | Turn OFF and then ON the power.
E610 | 0202 | 00 | Title | Failure of the HDD encryption key (hardware configuration error/initialization error/encryption key error/encryption processing error)
Description | Error in the encryption processing part.
Remedy | Turn OFF and then ON the power.
E610 | 0301 | 00 | Title | Failure of the HDD encryption key (hardware configuration error/initialization error/encryption key error/encryption processing error)
Description | Failed to create the encryption key.
Remedy | Turn OFF and then ON the power.
E610 | 0302 | 00 | Title | Failure of the HDD encryption key (hardware configuration error/initialization error/encryption key error/encryption processing error)
Description | Failure of the encryption key is detected.
Remedy | Turn OFF and then ON the power. Due to this error, HDD content is initialized.
E610 | 0303 | 00 | Title | Failure of the HDD encryption key (hardware configuration error/initialization error/encryption key error/encryption processing error)
Description | Failure of the encryption key is detected.
Remedy | Turn OFF and then ON the power. Due to this error, HDD content is initialized.
E610 | 0401 | 00 | Title | Failure of the HDD encryption key (hardware configuration error/initialization error/encryption key error/encryption processing error)
Description | Error is detected during encryption.
Remedy | Turn OFF and then ON the power.
E610 | 0402 | 00 | Title | Failure of the HDD encryption key (hardware configuration error/initialization error/encryption key error/encryption processing error)
Description | Error is detected during decryption.
Remedy | Turn OFF and then ON the power.
E610 | 0501 | 00 | Title | Failure of the HDD encryption key (hardware configuration error/initialization error/encryption key error/encryption processing error)
Description | Error in document management information on /FSTDEV.
Remedy | Turn OFF and then ON the power.
E611 | 0000 | 00 | Title | Rebooting due to SRAM corruption when executing a transmission job that secures disconnection of the power
Description | In the case that reboot is repeated at recovery from power down because SRAM information is corrupted and the job information saved on SRAM cannot be read, the phenomenon that the communication is repeated occurs.
Remedy | Clear SRAM to erase the job that secures disconnection of the power.
E615 | 0001 | 00 | Title | Self test error of encryption module
Description | A self test of the Ipsec Board was conducted, and an error was detected. The encryption module is broken.
Remedy | Upgrade the system after HDD format. When this error occurs, normal network communication cannot be guaranteed.
E674 | 0001 | 00 | Title | FAX error
Description | Communication error with the FAX PCB.
Remedy | Check the cable connection, replace the FAX PCB, replace the Main Controller PCB.
E674 | 0004 | 00 | Title | FAX error
Description | Error in access of the modem IC.
Remedy | Check the cable connection, replace the FAX PCB, replace the Main Controller PCB.
E674 | 0008 | 00 | Title | FAX error
Description | Error in access of the port IC.
Remedy | Check the cable connection, replace the FAX PCB, replace the Main Controller PCB.
E674 | 0010 | 00 | Title | FAX error
Description | FAX error
Remedy | Replace the Main Controller PCB.
E674 | 0011 | 00 | Title | FAX error
Description | FAX error
Remedy | Replace the Main Controller PCB.
E674 | 0030 | 00 | Title | FAX error
Description | Checksum error.
Remedy | Download the system software for 2-line FAX.
E674 | 0100 | 00 | Title | FAX error
Description | Logging is failed after completion of FAX communication, and unable to read.
Remedy | Turn OFF and then ON the power.
E674 | 0200 | 00 | Title | HDD access error
Description | An error occurred when accessing the HDD.
Remedy | 1. Turn OFF/ON the main power switch. 2. Reinstall all the formats and the system. 3. Replace the HDD. 4. Replace the Main Controller PCB 1.
E674 | 000C | 00 | Title | FAX error
Description | Error in access of the modem IC/port IC.
Remedy | Check the cable connection, replace the FAX PCB, replace the Main Controller PCB.
E677 | 0001 | 00 | Title | Print server error
Description | Exhaust Fan operation error on the print server is detected.
Remedy | 1. Check power supply to the Exhaust Fan. 2. Replace the Exhaust Fan.
E677 | 0003 | 00 | Title | Print server error
Description | Error is detected at the configuration check performed at startup.
Remedy | Check the cable connection, reinstallation.
E677 | 0004 | 00 | Title | Print server error
Description | CPU Fan operation error on the print server is detected.
Remedy | 1. Check power supply to the CPU Fan. 2. Replace the CPU Fan.
E677 | 0010 | 00 | Title | Print server error
Description | Not proper print server is connected.
Remedy | Replace the print server with the proper one.
E677 | 0080 | 00 | Title | Print server error
Description | Communication error at startup.
Remedy | Check the cable connection, reinstallation.
E710 | 0001 | 00 | Title | Printer IPC error
Description | Error is detected by IPC communication IC of the printer engine at power ON.
Remedy | Disconnection of cable.
E711 | 0001 | 05 | Title | UFDI communication error
Description | Communication system error (reception time out error/checksum error etc.)
Remedy | 1. Check the cable. 2. Replace the DC Controller PCB (UN2). 3. Replace the Finisher Controller PCB.
E711 | 0002 | 05 | Title | IPC communication error
Description | Communication system error (packet error occurs without the request of initialization)
Remedy | 1. Check the cable. 2. Replace the DC Controller PCB (UN2). 3. Replace the Finisher Controller PCB.
E713 | 0000 | 05 | Title | Erroneous communication with finisher (retry error)
Description | The communication does not restart by the error retry after the communication failure with the finisher.
Remedy | 1. Check the cable. 2. Replace the DC Controller PCB (UN2). 3. Replace the Finisher Controller PCB.
E713 | 0001 | 05 | Title | Erroneous communication with finisher (transmission retry error)
Description | The communication does not restart by the error retry after the communication failure with the finisher.
Remedy | 1. Check the cable. 2. Replace the DC Controller PCB (UN2). 3. Replace the Finisher Controller PCB.
E713 | 0002 | 05 | Title | Erroneous communication with finisher (transmission data error)
Description | The communication does not restart by the error retry after the communication failure with the finisher.
Remedy | 1. Check the cable. 2. Replace the DC Controller PCB (UN2). 3. Replace the Finisher Controller PCB.
E713 | 0004 | 05 | Title | Erroneous communication with finisher (reception error)
Description | The communication does not restart by the error retry after the communication failure with the finisher.
Remedy | 1. Check the cable. 2. Replace the DC Controller PCB (UN2). 3. Replace the Finisher Controller PCB.
E713 | 0010 | 05 | Title | Erroneous communication with finisher (reception error)
Description | The communication does not restart by the error retry after the communication failure with the finisher.
Remedy | 1. Check the cable. 2. Replace the DC Controller PCB (UN2). 3. Replace the Finisher Controller PCB.
E713 | 0011 | 05 | Title | Erroneous communication with finisher (reception error)
Description | The communication does not restart by the error retry after the communication failure with the finisher.
Remedy | 1. Check the cable. 2. Replace the DC Controller PCB (UN2). 3. Replace the Finisher Controller PCB.
E713 | 0020 | 05 | Title | Erroneous communication with finisher (reception data error)
Description | The communication does not restart by the error retry after the communication failure with the finisher.
Remedy | 1. Check the cable. 2. Replace the DC Controller PCB (UN2). 3. Replace the Finisher Controller PCB.
E713 | 0021 | 05 | Title | Erroneous communication with finisher (reception time out error)
Description | The communication does not restart by the error retry after the communication failure with the finisher.
Remedy | 1. Check the cable. 2. Replace the DC Controller PCB (UN2). 3. Replace the Finisher Controller PCB.
E713 | 0022 | 05 | Title | Erroneous communication with finisher (reception data error)
Description | The communication does not restart by the error retry after the communication failure with the finisher.
Remedy | 1. Check the cable. 2. Replace the DC Controller PCB (UN2). 3. Replace the Finisher Controller PCB.
E716 | 0000 | 05 | Title | Erroneous communication with cassette pedestal
Description | After the presence of a cassette pedestal has been detected, the communication fails to be normal for 5 sec.
Remedy | 1. Check the cable. 2. Replace the DC Controller PCB (UN2). 3. Replace the Cassette Pedestal Driver PCB.
E717 | 0001 | 00 | Title | Communication error with the NE Controller
Description | Error when the NE Controller is started. The NE Controller which was connected before turning OFF the power is not connected at power-on.
Remedy | Check the cable, and then go through the following to clear the error: Service Mode > COPIER > FUNCTION > CLEAR > ERR.
E717 | 0002 | 00 | Title | Communication error with the NE Controller
Description | IPC error at NE Controller operation. Open circuit of IPC, unable to recover the IPC communication.
Remedy | Check the cable, and then go through the following to clear the error: Service Mode > COPIER > FUNCTION > CLEAR > ERR.
E719 | 0001 | 00 | Title | Error in coin manager
Description | Error when the coin manager is started. The coin manager which was connected before turning OFF the power is not connected at power-on.
Remedy | Check the cable, and then go through the following to clear the error: Service Mode > COPIER > FUNCTION > CLEAR > ERR.
E719 | 0002 | 00 | Title | Error in coin manager
Description | IPC error at coin manager operation. Open circuit of IPC, unable to recover the IPC communication. When open circuit of the pickup/delivery signal cable is detected. Invalid connection is detected.
Remedy | Check the cable, and then go through the following to clear the error: Service Mode > COPIER > FUNCTION > CLEAR > ERR.
E719 | 0003 | 00 | Title | Error in coin manager
Description | Communication error with the coin manager occurs during unit price acquisition at startup.
Remedy | Check the cable, and then go through the following to clear the error: Service Mode > COPIER > FUNCTION > CLEAR > ERR.
E719 | 0011 | 00 | Title | Error when the Card Reader is started
Description | The Card Reader which was connected before turning OFF the power is not connected at power-on.
Remedy | Check the cable, and then go through the following to clear the error: Service Mode > COPIER > FUNCTION > CLEAR > ERR.
E719 | 0012 | 00 | Title | IPC error at Card Reader operation
Description | Open circuit of IPC, unable to recover the IPC communication.
Remedy | Check the cable, and then go through the following to clear the error: Service Mode > COPIER > FUNCTION > CLEAR > ERR.
E719 | 0031 | 00 | Title | Communication error when the Card Reader (serial) is started
Description | Unable to start communication with the Card Reader at startup.

Remedy

1. Check the cable connection of the Card Reader (connector connection error, open circuit), and then go through the following to clear the error: Service Mode > COPIER > FUNCTION > CLEAR > ERR.
2. After removing the Card Reader, execute the following service mode, and then reinstall the Card Reader.
COPIER>FUNCTION>CLEAR>CARD
COPIER>FUNCTION>CLEAR>ERR"

E719 | 0032 | 00 | Title | Communication error after the Card Reader (serial) is started
Description | Although communication with the Card Reader was possible at startup, it became unavailable in the middle of it.
Remedy | Check the cable connection of the Card Reader (connector connection error, open circuit), and then go through the following to clear the error: Service Mode > COPIER > FUNCTION > CLEAR > ERR.
E730 | 1001 | 00 | Title | PDL software error
Description | Systematic fatal error, such as initialization failure, occurs.
Remedy | 1. PDL reset processing. 2. Turn OFF and then ON the power.
E730 | 9004 | 00 | Title | Third party PDL communication error
Description | Communication error with the print server.
Remedy | 1. Turn OFF and then ON the power. 2. Check the cable connection. 3. Replace the Open I/F PCB, F Link PCB (Main/Sub). 4. Replace the Main Controller PCB.
E730 | 9005 | 00 | Title | Third party PDL communication error
Description | Error in video cable connection with the print server.
Remedy | 1. Turn OFF and then ON the power. 2. Check the cable connection. 3. Replace the Open I/F PCB, F Link PCB (Main/Sub). 4. Replace the Main Controller PCB.
E730 | 100A | 00 | Title | PDL software error
Description | Systematic fatal error, such as initialization failure, occurs.
Remedy | 1. PDL reset processing. 2. Turn OFF and then ON the power.
E730 | A006 | 00 | Title | PDL communication error
Description | No reply from PDL. Due to failure of Subbootable, or no existence, there is no reply from PDL.
Remedy | 1. PDL reset processing. 2. Turn OFF and then ON the power. 3. Check the connection of the Main Controller PCB. 4. Reinstall the firmware. 5. Replace the Main Controller PCB.
E730 | A007 | 00 | Title | Mismatched PDL version
Description | Version of the host machine control software and version of PDL control software are different.
Remedy | 1. PDL reset processing. 2. Turn OFF and then ON the power. 3. System All Format and installation.
E730 | B013 | 00 | Title | PDL embedded font error
Description | Font data is corrupted.
Remedy | 1. Turn OFF and then ON the power. 2. Reinstall the system. 3. System All Format and installation.
E732 | 0000 | 00 | Title | Reader communication error
Description | Negotiation failure.
Remedy | 1. Check the connection of the Connector with the Reader. 2. Check the power of the Reader (check if the initialization operation is executed at startup). 3. Replace the Reader Controller PCB and the Main Controller PCB.
E732 | 0001 | 00 | Title | Reader communication error
Description | Communication error.
Remedy | 1. Check the connection of the Connector with the Reader. 2. Check the power of the Reader (check if the initialization operation is executed at startup). 3. Replace the Reader Controller PCB and the Main Controller PCB.
E732 | 0010 | 00 | Title | Reader communication error
Description | Unable to detect Vsync from the Reader Controller although 2 minutes have passed after the completion of register setting of the Main Controller.
Remedy | 1. Check the connection of the Connector with the Reader. 2. Check the power of the Reader (check if the initialization operation is executed at startup). 3. Replace the Reader Controller PCB and the Main Controller PCB.
E732 | 0021 | 04 | Title | Reader communication error
Description | Communication error
Remedy | 1. Check the connection of the Connector with the Reader. 2. Check the power of the Reader (check if the initialization operation is executed at startup). 3. Replace the Reader Controller PCB and the Main Controller PCB.
E732 | 8888 | 00 | Title | Error in the reader type
Description | When a scanner for the different model is detected during the communication with the reader.
Remedy | Replace to the proper reader.
E732 | 9999 | 00 | Title | Detection of Reader
Description | The Reader is detected for the first time with the printer model. (On the user screen, only the message "Turn OFF and then ON the power again", instead of an error code, is displayed. It is recorded as an error log in Service Mode > DISPLAY > ERR.)
Remedy | ---
E733 | 0000 | 00 | Title | Printer communication error
Description | Unable to communicate with printer at startup.
Remedy | 1. Check the connection of the Connector with the printer. 2. Check the power of the printer (check if the initialization operation is executed at startup). 3. Replace the DC Controller or the Main Controller PCB.
E733 | 0001 | 00 | Title | Printer communication error
Description | Communication error between the Main Controller and the DC Controller.
Remedy | 1. Check the connection between the DC controller PCB (J210) and the main controller PCB2 (I8112). 2. Check the power of the printer (check if the initialization operation is executed at startup). 3. Replace the DC Controller or the Main Controller PCB 2.
E733 | 0002 | 00 | Title | Printer communication error
Description | Communication error between the Main Controller and the DC Controller.
Remedy | 1. Check the connection between the DC controller PCB (J210) and the main controller PCB2 (I8112). 2. Check the power of the printer (check if the initialization operation is executed at startup). 3. Replace the DC Controller or the Main Controller PCB 2.
E733 | 0010 | 00 | Title | Printer communication error
Description | Error to detect printer vertical synchronous signal.
Remedy | 1. Check the connection between the DC controller PCB (J210) and the main controller PCB2 (I8112). 2. Check the power of the printer (check if the initialization operation is executed at startup). 3. Replace the DC Controller or the Main Controller PCB 2.
E740 | 0002 | 00 | Title | Network Controller error
Description | Invalid MAC address.
Remedy | 1. Check the connection of the LAN Connector. 2. Check the connection of the Main Controller PCB 1. 3. Replacement of the Main Controller PCB 1.
E743 | 0000 | 05 | Title | DDI communication error
Description | The Reader Controller PCB detected the communication error between the Main Controller PCB and the Reader Controller PCB.
Remedy | 1. Connection error between the Main Controller PCB and the Reader Controller PCB. 2. Failure of the Reader Controller PCB (PCB1). 3. Failure of the Main Controller PCB.
E744 | 0001 | 00 | Title | Error in language file/BootROM
Description | Version of language in HDD and version of Bootable are different.
Remedy | Download the correct version of the language file.
E744 | 0002 | 00 | Title | Error in language file/BootROM
Description | Size of the language in HDD is too big.
Remedy | Download the correct version of the language file.
E744 | 0003 | 00 | Title | Error in language file/BootROM
Description | Unable to find the language to be switched to that is described in the Config.txt in HDD.
Remedy | Download the correct version of the language file.
E744 | 0004 | 00 | Title | Error in language file/BootROM
Description | Unable to switch to the language in HDD.
Remedy | Download the correct version of the language file.
E744 | 1000 | 00 | Title | Error in language file/BootROM
Description | The Boot ROM for the different model is installed.
Remedy | Replace the Boot ROM with the one for the correct model.
E744 | 2000 | 00 | Title | Error in language file/BootROM
Description | When the engine ID described in Soft ID is invalid.
Remedy | Replace the Soft ID with the one for the correct model.
E744 | 4000 | 05 | Title | Engine ID error
Description | The Main Controller PCB model and the DC Controller PCB (UN2) model are not matched.
Remedy | Replace the DC Controller PCB (UN2) or redownload.
E746 | 0003 | 00 | Title | Different Image Analysis PCB model
Description | Different Image Analysis PCB model.
Remedy | 1. Check the connection of the Image Analysis PCB. 2. Replace the Image Analysis PCB.
E746 | 0021 | 00 | Title | Image Analysis PCB self-check error detection
Description | Image Analysis PCB self-check error detection.
Remedy | 1. Check the connection of the Image Analysis PCB. 2. Replace the Image Analysis PCB.
E746 | 0022 | 00 | Title | Invalid Image Analysis PCB version
Description | Invalid Image Analysis PCB version.
Remedy | 1. Upgrade the Image Analysis PCB software. 2. Replace the Image Analysis PCB.
E746 | 0023 | 00 | Title | No reply from Image Analysis PCB
Description | No reply from Image Analysis PCB.
Remedy | 1. Check the connection of the Image Analysis PCB. 2. Replace the Image Analysis PCB.
E746 | 0024 | 00 | Title | Image Analysis PCB operation error
Description | Image Analysis PCB operation error
Remedy | 1. Check the connection of the Image Analysis PCB. 2. Replace the Image Analysis PCB.
E746 | 0031 | 00 | Title | Hardware error (TPM)
Description | Hardware error (TPM).
Remedy | The TPM PCB is not installed, the TPM PCB for other model is installed, or failure of TPM Chip.
E746 | 0032 | 00 | Title | Error in engine ID of SoftID
Description | Mismatched data in TPM

Remedy

Format the system.
Format the HDD using SST or USB memory, and download the system software. For details, see "Chapter 6: Upgrading". For your reference, the method using USB memory is described below.
1. Prepare the USB memory which system software was registered.
2. Execute the following service mode: COPIER>FUNCTION>SYSTEM>DOWNLOAD to enter the download mode.
3. Insert the USB memory to the equipment.
4. Execute [4]: Format HDD in the main menu.
After formatting is completed, the machine reboots automatically and starts with the download mode.
5. Execute [1]: Upgrade (Auto) in the main menu.
System software is downloaded and the machine restarts automatically.

E746 | 0033 | 00 | Title | Error in engine ID of SoftID
Description | Error that can be recovered

Remedy

When the TPM key was backed up, it can be restored.
1. Connect the USB memory which stores the TPM key.
2. Go to Management Settings > Data Management > TPM Settings, and then click "Restore TPM Key".
3. Enter the password set at backup operation.
4. When the restoration completion screen is displayed, click "OK". Remove the USB memory, and turn OFF and then ON the main power.
When the TPM key was not backed up, formatting the system is required.
Format the HDD using SST or USB memory, and download the system software. For details, see "Chapter 6: Upgrading". For your reference, the method using USB memory is described below.
1. Prepare the USB memory which system software was registered.
2. Execute the following service mode: COPIER>FUNCTION>SYSTEM>DOWNLOAD to enter the download mode.
3. Insert the USB memory to the equipment.
4. Execute [4]: Format HDD in the main menu.
After formatting is completed, the machine reboots automatically and starts with the download mode.
5. Execute [1]: Upgrade (Auto) in the main menu.
System software is downloaded and the machine restarts automatically.

E746 | 0034 | 00 | Title | Error occurs, but auto recovery of system is possible (TPM)
Description | Error occurs, but auto recovery of system is possible (TPM).
Remedy | Mismatch of key occurs. However, recovery by restart is possible. Turn OFF and then ON the power.
E748 | 2000 | 00 | Title | Main Controller PCB access error
Description | Main Controller PCB Chip access error.
Remedy | Replace the Main Controller PCB 1/2.
E748 | 2001 | 00 | Title | Main Controller PCB access error
Description | Main Controller PCB memory access error.
Remedy | 1. Remove and then reinstall the DDR2-SDRAM(M0/M1/P). 2. Replace the Main Controller PCB 1/2.
E748 | 2010 | 00 | Title | Flash board error
Description | IPL (Initial Program Loader) is not found
Remedy | Flash board replacement
E748 | 2011 | 00 | Title | Flash board error
Description | OS is not found
Remedy | Flash board replacement
E748 | 2012 | 00 | Title | Flash board error
Description | Cannot mount the OS in safe mode startup or No OS startup script
Remedy | Flash board replacement
E748 | 2021 | 00 | Title | Main controller board 2 access errors
Description | Main controller board 2 access errors
Remedy | Main controller board 1/2 removing and inserting, replacement
E748 | 2023 | 00 | Title | Main controller board 2 access errors
Description | Main controller board 2 access errors
Remedy | DDR2-SDRAM (M0/M1/P) removing and inserting, replacement
E748 | 2024 | 00 | Title | Main controller board 2 access errors
Description | Main controller board 2 access errors
Remedy | Main controller board 1/2 removing and inserting, replacement
E748 | 4910 | 00 | Title | Main controller board 2 access errors
Description | Main controller board 2 access errors
Remedy | Replace the Main Controller PCB 2.
E748 | 9000 | 00 | Title | System error
Description | ---
Remedy | Contact to the sales companies
E753 | 0001 | 05 | Title | Download error
Description | System Software Update Error Error occurs when updating system software of uninstalled options

Remedy

Check the log to find where the download error has been occurred.
FIN_G1 Staple Finisher-G1/Booklet Finisher-G1
IFN_D1 Inner Finisher-D1
G3CCB Super G3 FAX Board-AK1/Super G3 2nd Line Fax Board-AK1/Super G3 3rd/4th Line Fax Board-AK1
G3CCM Super G3 FAX Board-AK1/Super G3 2nd Line Fax Board-AK1/Super G3 3rd/4th Line Fax Board-AK1
When any of the above system software is displayed, check if the target option has been installed.
When the target option has not been installed:
Turn OFF and then ON the main power supply to restore (since there is no system software to be updated.).
When the target option has been installed:
Check if the accessory is correctly installed and if the target system software to be downloaded is for the installed option. Then download the appropriate system software again.

E760 | 0001 | 00 | Title | Main Controller PCB 2 internal error

Description

1. Turn OFF and then ON the main power.
2. Remove and then install the DDR2-SDRAM (J201) on the Main Controller PCB 2.
3. Replace the DDR2-SDRAM on the Main Controller PCB 2.
4. Replace the Main Controller PCB 2.
NOTE:
If the error occurs periodically or it occurs with specific jobs although it can be solved by turning OFF and then ON the power, upgrade the system software to the latest version.

Remedy | Error was detected in the Image Processing Chip on the Main Controller PCB 2.
E800 | 0000 | 05 | Title | Power condition unmatched error between Main Controller PCB and DC Controller PCB
Description | The power of DC controller PCB still keep ON even if it reaches 90 sec after detecting the power OFF by the main controller PCB.
Remedy | 1. Wait till the power is turned off. 2. Turn the main power switch ON.
E804 | 0000 | 05 | Title | Failure of the Power Supply Cooling Fan
Description | When lock signal is detected for 5 sec while the Power Supply Cooling Fan (FM5) is stopped. * The same condition is detected after the error retry is performed.
Remedy | 1. Disconnect and then connect the connector (J205) on the DC Controller PCB (UN2). 2. Replace the Power Supply Cooling Fan (FAN6). 3. Replace the DC Controller PCB (UN2).
E804 | 0001 | 05 | Title | Unstable rotation of the Power Supply Cooling Fan (FAN6)
Description | The fan stop signal is detected for 5 minutes or more and the retry operation fails 4 times continuously after generating the ON signal of the Power Supply Cooling Fan (FAN5).
Remedy | 1. Check connection of the Connectors (J2003/J119). 2. Replace the Power Supply Cooling Fan (FM5).
E805 | 0000 | 05 | Title | Failure of the Exhaust Fan (Rear) (FM3)
Description | When lock signal is detected for 15 sec while the Exhaust Fan (Rear) (FM3) is stopped. * The same condition is detected after the error retry is performed.
Remedy | 1. Check connection of the Connectors (J2010/J2501/J206). 2. Replace the Exhaust Fan (Rear) (FM3). 3. Replace the DC Controller PCB (UN2).
E805 | 0001 | 05 | Title | Unstable rotation of the Exhaust Fan (Rear) (FM3)
Description | When lock signal failed to be detected for 15 sec while the Exhaust Fan (Rear) (FM3) is driven. * The same condition is detected after the error retry is performed.
Remedy | 1. Check connection of the Connectors (J2010/J2501/J206). 2. Replace the Exhaust Fan (Rear) (FM3). 3. Replace the DC Controller PCB (UN2).
E805 | 0002 | 05 | Title | Failure of the Exhaust Fan (Front) (FM4)
Description | When lock signal is detected for 15 sec while the Exhaust Fan (Front) (FM4) is stopped. * The same condition is detected after the error retry is performed.
Remedy | 1. Check connection of the Connectors (J2009/J2501/J206). 2. Replace the Exhaust Fan (Front) (FM4). 3. Replace the DC Controller PCB (UN2).
E805 | 0003 | 05 | Title | Unstable rotation of the Exhaust Fan (Front) (FM4)
Description | When lock signal failed to be detected for 15 sec while the Exhaust Fan (Front) (FM4) is driven. * The same condition is detected after the error retry is performed.
Remedy | 1. Check connection of the Connectors (J2009/J2501/J206). 2. Replace the Exhaust Fan (Front) (FAN4). 3. Replace the DC Controller PCB (UN2).
E806 | 0000 | 05 | Title | Failure of the Main Body Cooling Fan (FM6)
Description | When lock signal is detected for 5 sec while the Main Body Cooling Fan (FM6) is stopped. *The same condition is detected after the error retry is performed.
Remedy | 1. Check connection of the Connectors (J2210/J222). 2. Replace the Main Body Cooling Fan (FM6). 3. Replace the DC Controller PCB (UN2).
E806 | 0001 | 05 | Title | Unstable rotation of the Main Body Cooling Fan (FM6)
Description | When lock signal failed to be detected for 15 sec while the Main Body Cooling Fan (FM6) is driven. * The same condition is detected after the error retry is performed.
Remedy | 1. Check connection of the Connectors (J2210/J222). 2. Replace the Main Body Cooling Fan (FM6). 3. Replace the DC Controller PCB (UN2).
E806 | 0002 | 05 | Title | Failure of the Paper Cooling Fan (FM7)
Description | When lock signal is detected for 15 sec while the Paper Cooling Fan (FM7) is stopped. *The same condition is detected after the error retry is performed.
Remedy | 1. Check connection of the Connectors (J2209/J2509/J206). 2. Replace the Paper Cooling Fan (FM7). 3. Replace the DC Controller PCB (UN2).
E806 | 0003 | 05 | Title | Unstable rotation of the Paper Cooling Fan (FM7)
Description | When lock signal failed to be detected for 15 sec while the Paper Cooling Fan (FM7) is driven. * The same condition is detected after the error retry is performed.
Remedy | 1. Check connection of the Connectors (J2209/J2509/J206). 2. Replace the Paper Cooling Fan (FM7). 3. Replace the DC Controller PCB (UN2).
E840 | 0000 | 05 | Title | Edge Shutter Home Position error
Description | When the home position of the shutter is not detected
Remedy | 1. Check connection of the Connectors (J2039/J2037/J2507/J215). 2. Replace the fixing film edge shutter HP sensor (S10). 3. Replace the fixing film edge shutter motor (M8). 4. Replace the DC controller PCB (UN2).
E840 | 0001 | 05 | Title | Failure of Fixing Film Edge Cooling Fan (Rear) (FM1)
Description | When the lock signal is detected for 15 sec while the fixing film edge cooling fan (rear) stops. * The same status is detected again after the retry operation.
Remedy | 1. Check connection of the Connectors (J2036/J215). 2. Replace the fixing film edge cooling fan (rear) (FM1) 3. Replace the DC controller PCB (UN2).
E840 | 0002 | 05 | Title | Rotation error of Fixing Film Edge Cooling Fan (Rear) (FM1)
Description | When the lock signal is detected for 15 sec while the fixing film cooling fan (rear) operates. * The same status is detected again after the retry operation.
Remedy | 1. Check connection of the Connectors (J2036/J215). 2. Replace the fixing film edge cooling fan (rear) (FM1) 3. Replace the DC controller PCB (UN2).
E840 | 0003 | 05 | Title | Failure of Fixing Film Edge Cooling Fan (Front) (FM2)
Description | When the lock signal is detected for 15 sec while the fixing film edge cooling fan (front) stops. * The same status is detected again after the retry operation.
Remedy | 1. Check connection of the Connectors (J2035/J215). 2. Replace the fixing film edge Cooling fan (front) (FM2) 3. Replace the DC controller PCB (UN2).
E840 | 0004 | 05 | Title | Rotation error of Fixing Film Edge Cooling Fan (Front) (FM2)
Description | When the lock signal is detected for 15 sec while the fixing film edge cooling fan (front) operates. * The same status is detected again after the retry operation.
Remedy | 1. Check connection of the Connectors (J2035/J215). 2. Replace the fixing film edge cooling fan (front) (FM2). 3. Replace the DC controller PCB (UN2).
E880 | 0001 | 00 | Title | Controller Cooling Fan error
Description | The failure of the controller cooling fan (FM12) is detected.
Remedy | 1. Check the connector (J1015). 2. Replace the controller cooling fan (FM12). 3. Replace the main controller PCB 1 (UN25).
E880 | 0005 | 00 | Title | Controller Cooling Fan error
Description | 1. Check the connector (J1015). 2. Replace the controller cooling fan (FM12). 3. Replace the main controller PCB 1 (UN25).
Remedy | Controller Cooling Fan (FM12) is detected.