Handling of Laser System﻿

| Print out this category

Handling of Laser System﻿
When servicing the area around the laser assembly, be sure to turn off the main power.
If you must servicr while the power is turned on, be sure to keep the followings:
- Do not use a screwdriver or tools that have a high level of reflectance in the laser path.
- Remove watches and rings before starting the work. (They can reflect the laser beam, possibly hitting the eye.)
The machine's covers that can reflect laser light are identified by means of a warning label (Figure). If you must detach a cover showing the label, be sure to take
extra caution during the work.
The following warnings are given to comply with Safety Standard (EN60950-1).
This product is certificated as a Class 1 laser product under IEC60825-1:2007.