Unpacking the Machine and Removing the Packaging Materials

| Print out this category

﻿Unpacking and Installation Procedure
Unpacking the Machine and Removing the Packaging Materials
1) Unpack the machine and remove the vinyl cover.
NOTE:
When installing the host machine and the options at the same time, install the options first by following the procedure below for better workability.
1. Installing the Cassette Pedestal (Refer to Installation Procedure for the Cassette Pedestal.)
2. Installing the DADF (if it is an option) (Refer to Installation Procedure for the DADF.)
3. Installing the host machine
2) While holding four handles on the left and right sides of the machine, lift the machine to take it down from the palette.
CAUTION:
The maximum weight of the machine is approx. 78.9 kg (FAX standard model). Be sure to perform the work in accordance with the standard to handle a heavy load in each country. In addition, be sure to keep the machine leveled when lifting it.
3) Remove the tapes on the exterior of the host machine.
CAUTION:
Remove the following in later step.
Cassette inside (wire of the cassette intermediate plate)
Reader assembly (two optical system fixing screws)
Front cover inside (fixing tape of the waste toner container mount)
Right cover inside (fixing pressure release material)
4) Open the ADF, and remove the cushioning material.
5) Close the ADF.
6) Remove two optical system fixing screws on the left side of the reader. (Keep the removed screws because they may be used later for machine relocation.)
7) Press the cassette release button to draw out the cassette forward.
8) Remove the wire that secures the intermediate plate of the cassette 1/2 and the fixing tape.
9) Insert the cassette 1/2.
10) Remove the fixing pressure release material.
11) Remove the fixing pressure release material.
12) Close the right cover.