﻿Removing the Developing Cylinder

| Print out this category

Removing the Developing Cylinder
<Procedure>
Caution:
Take note of the following points when removing the developing cylinder from the developing assembly:
Lots of self-tapping screws are used. Be careful not to damage the screw holes by tightening the self-tapping screws.
Do not touch nor give a shock to the developing cylinder.
1) Remove the developing assembly. (Reference)
2) Remove the top cover.
4 screws
3) Remove the ring, the gear, the parallel pin and the gear.
4) Remove the gear unit.
3 screws
5) Remove the holder.
2 screws
1 pushing wheel
6) Remove the bearing.
7) Remove the holder.
2 screws
8) Remove the developing contact spring.
9) Remove the holder.
2 screws
1 pushing wheel
10) Remove the bearing.
11) Remove the blade unit.
2 screws
CAUTION:
Remove the Developing Cylinder after removing the Developing Blade on a blade unit basis.
12) Remove the developing cylinder.