Setting the Cassettes

| Print out this category

Setting the Cassettes
1) Press the cassette release button to draw out the cassette forward.
2) Confirm the type of paper used by the customer.
3) While nipping the trailing edge guide lever, slide the trailing edge guide to the position corresponding to the prescribed paper size.
4) While nipping the side guide lever, slide the side guide to the position corresponding to the prescribed paper size.
5) Set paper and open the cover at the insertion area of the size plate.
6) Cut the 2 points of the cassette size label with nippers.
7) Following the paper size, set the cassette size label (unused size plates should be put together).
8) Close the cover at the insertion area of the cassette size label and push in the cassette.
9) Set another cassette as well.