Left Edge Margin Adjustment (1st side)

| Print out this category

Image Position Adjustment
Left Edge Margin Adjustment (1st side)
Adjustment of Cassette/Manual feed pickup tray
Print from each cassette/Manual feed pickup tray, and check that the left edge margin of the image (L1) is within 2.5 +/- 1.5mm.
If it is not within the range, execute adjustment by following the procedure below.
1) Adjust the image position in service mode.
Cassette 1: Service mode (Level 2) > COPIER > ADJUST > MISC > C1-ADJ-Y
Cassette 2: Service mode (Level 2) > COPIER > ADJUST > MISC > C2-ADJ-Y
Cassette 3: Service mode (Level 2) > COPIER > ADJUST > MISC > C3-ADJ-Y
Cassette 4: Service mode (Level 2) > COPIER > ADJUST > MISC > C4-ADJ-Y
Manual feed pickup tray: Service mode (Level 2) > COPIER > ADJUST > MISC > MF-ADJ-Y
NOTE:
<Setting Range>
-128 to 127 (0.1mm per unit)
As the value is incremented by 1, the left edge margin is increased by 0.1mm.
2) Print from the cassette/manual feed pickup tray, and check that the left edge margin of the image is within 2.5 +/- 1.5mm.
3) When the setting value was changed in step 1), write down the new numerical value in the service label.
4) Exit from the service mode.