Required Options/Conditions

| Print out this category

Required Options/Conditions
Pickup System Options

Product name | Required options, conditions, etc.
Paper Deck Unit-B2 | Pickup capacity:2,700 sheets (80 g/m2), 3,000 sheets (64 g/m2) Paper size: A4, LTR Paper weight: 60 to 128 g/m2 Paper type: plain paper 1 (60 to 63 g/m2), plain paper 2 (64 to 90 g/m2), recycled paper, color paper, heavy paper 1 (91 to 105 g/m2) ,heavy paper 2 (106 to 128 g/m2), pre-punched paper
Paper Deck Heater Unit-C1 | Option for Paper Deck Unit-B2 Use it to suppress the moisture absorption of the paper in the paper deck.
Cassette Feeding Unit-AF1 | Pickup capacity:550 sheets (80 g/m2), 680 sheets (64 g/m2) Paper size: Standard (universal) A3, B4, A4, B5, 279mmX432mm(11"X17"), LGL, LTR, A4R, B5R, LTRR, A5R, STMTR, 8K, 16K, 16KR, EXEC Paper weight: 64 to 128 g/m2 Paper type: plain paper 1 (60 to 63 g/m2), plain paper 2 (64 to 90 g/m2), recycled paper, color paper, heavy paper 1 (91 to 105 g/m2) ,heavy paper 2 (106 to 128 g/m2), pre-punched paper
Cassette Heater Unit-37 | Option for cassette of main body and Cassette Feeding Unit-AF1 Use it to suppress the moisture absorption of the paper in the cassette. Heater Kit-K1 is required.
FL Cassette-AM1 | Option for 2nd cassette of the main body
FL Cassette-AQ1 | Option for 1st cassette of the main body
Envelope Feeder Attachment-D1 | Option for 2nd cassette of the main body

Delivery System Options

Product name | Required options, conditions, etc.
Inner Finisher Additional Tray-A1 | Option for Inner Finisher-D1 Stacking capacity Non-collate/collate/group mode:100 sheets (12.5 mm or less in height) Staple mode:60 sheets (8.1 mm or less in height)
Inner Finisher-D1 | Stacking capacity: 1,000 sheets (81.4 g/m2; A4, B5, A5R, LTR, STMTR, EXEC, 16K) Paper weight: 52 to 220 g/m2 Stapling capacity: 50 sheets (81.4 g/m2; A4, B5, A5R, LTR, STMTR, EXEC, 16K)
Inner 2 Hole Puncher-A1 Inner 2/3 Hole Puncher-A1 Inner 2/4 Hole Puncher-A1 Inner 4 Hole Puncher-A1 | Option for Inner Finisher-D1. Hole type: 2 holes (AB), 2 holes/3 holes (Inch), FRN, 2 holes /4 holes, SWE/4 holes Paper size: A3, B4, A4, A4R, B5, B5R, 279mmX432mm(11"X17"), LGL, LTR, LTRR Paper weight: 52 to 220 g/m2
Inner Finisher-D1 with 2/3 Hole Puncher-A1 | US only Refer to Inner Finisher-D1 and Inner 2/3 Hole Puncher-A1.
Buffer Pass Unit-H1 | Staple Finisher-G1 or Booklet Finisher-G1 is required.

Inner 2Way Tray-H1

Tray capacity:
Tray A:
A4, B5, LTR: 250 sheets (80 g/m2)
A3, B4, 279mmX432mm(11"X17"), LGL: 100 sheets (80 g/m2)
Tray B:
A4, B5, LTR: 100 sheets (80 g/m2)
A3, B4, 279mmX432mm(11"X17"), LGL: 50 sheets (80 g/m2)

External 2 Hole Puncher-B2 External 2/3 Hole Puncher-B2 External 2/4 Hole Puncher-B2 External 4 Hole Puncher-B2 | Option for Staple Finisher-G1/Booklet Finisher-G1. Hole type: 2 holes (AB), 2 holes/3 holes (Inch), FRN, 2 holes /4 holes, SWE/4 holes Paper size: A3, B4, A4, A4R, B5, B5R, 279mmX432mm(11"X17"), LGL, LTR, LTRR, EXEC Paper weight: 52 to 220 g/m2
Staple Finisher-G1 | Using with Booklet Finisher-G1 is not available. Paper weight: 52 to 220 g/m2 Maximum stacking capacity: 4,000 sheets (A4, B5, A5R, LTR, STMTR, EXEC, 16K) Stapling capacity: 50 sheets (81.4 g/m2; A4, B5, LTR, EXEC)
Booklet Finisher-G1 | Using with Staple Finisher-G1 is not available. Paper weight: 52 to 220 g/m2 Maximum stacking capacity: 4000 sheets (A4, B5, A5R, LTR, STMTR, EXEC, 16K) Stapling capacity: 50 sheets (81.4 g/m2; A4, B5, LTR, EXEC) Saddle capacity: 16 sheets (81.4 g/m2; A3, B4, A4R, 279mmX432mm(11"X17"), LGL, LTRR)