DADF-AG1 FEEDER > P001 to P009

| Print out this category

DADF-AG1 FEEDER > P001 to P009

Address | bit | Name | Symbol | Remarks
P001 | 7 | Not used |  |
6 | Not used |  |
5 | Not used |  |
4 | Not used |  |
3 | Not used |  |
2 | Not used |  |
1 | For R&D use |  |
0 | For R&D use |  |
P002 | 7 | Registration Clutch Drive | CL2 | 1: ON
6 | Pick up Clutch Drive | CL1 | 1: ON
5 | Not used |  |
4 | Not used |  |
3 | Not used |  |
2 | Stamp Solenoid Drive | SL2 | 1: ON
1 | ADF Fan Motor Drive | FM1 | 1: ON
0 | Document Detection LED | PCB3 | 1: ON
P003 | 7 | Not used |  |
6 | Not used |  |
5 | Not used |  |
4 | Not used |  |
3 | For R&D use |  |
2 | For R&D use |  |
1 | For R&D use |  |
0 | For R&D use |  |
P004 | 7 | Not used |  |
6 | Timing sensor | SR4 | 1: Paper presence
5 | Not used |  |
4 | Delivery reversal Sensor | SR3 | 1: Paper presence
3 | ADF Fan Motor Lock Siganal | FM1 | 1: Lock
2 | Not used |  |
1 | Model Port 1 | PCB1 | 1: DF Non-support
0 | Model Port 0 | PCB1 | 1: DF Non-support
P005 | 7 | Not used |  |
6 | A4R/LTRR Sensor | SR8 | 1: A4R
5 | Empty Sensor | SR5 | 0: Paper presence
4 | Not used |  |
3 | Cover Open/Closed Sensor | SR6 | 0: Open
2 | Release Motor HP Sensor | SR11 | 1: HP
1 | Document Length Sensor 2 | SR10 | 1: Paper presence
0 | Document Length Sensor 1 | SR7 | 1: Paper presence
P006 | 0to7 | For R&D use |  |
P007 | 0to15 | For R&D use |  |
P008 | 0to15 | For R&D use |  |
P009 | 0to15 | For R&D use |  |