﻿Removing the Pressure Roller

| Print out this category

Removing the Pressure Roller
1)Remove the fixing film unit. (Reference)
2)Remove the cable holder.
1 screw
3) Remove the fixing entrance guide.
1 claw
4) Insert the 5 to 6 sheets of plain paper between the fixing entrance guide and the pressure roller so that all ribs of the exit guide are covered with the paper.
CAUTION:
If the pressure roller is removed without inserting paper, the pressure roller will contact with the ribs on the exit guide so that the surface of the pressure roller is damaged. Surely insert the 5 to 6 sheets of paper between the fixing entrance guide and the pressure roller before removing the pressure roller.
5)Remove the pressure roller.
6)Remove the E ring, pressure roller gear, bushings and bearings.
CAUTION:
When the pressure roller is installed, set the pressure roller after covering the whole surface of the roller with 5 to 6 sheets of plain paper.
Pull out the paper by turning the pressure roller gear with a hand.