VERSION

| Print out this category

﻿COPIER
DISPLAY
VERSION

COPIER>DISPLAY>VERSION
DC-CON | Display of DCON firmware version
Lv.1 | Details | To display the firmware version of DC Controller PCB.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
R-CON | Display of RCON firmware version
Lv.1 | Details | To display the firmware version of Reader Controller PCB.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
PANEL | Dis of Control Panel CPU PCB ROM version
Lv.1 | Details | To display the ROM version of Control Panel CPU PCB.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
FEEDER | Display of DADF Driver PCB ROM version
Lv.1 | Details | To display the firmware version of DADF Driver PCB.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
SORTER | Display of FIN-CONT firmware version
Lv.1 | Details | To display the firmware version of Finisher Controller PCB.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
NIB | Display of network software version
Lv.1 | Details | To display the version of the network software.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
PS/PCL | Dis of UFR Board (PS/PCL func) version
Lv.1 | Details | To display the version of UFR Board (PS/PCL function).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
SDL-STCH | Dis of Saddle Sttch Ctrollr PCB ROM version
Lv.1 | Details | To display the ROM version of the Saddle Stitcher Controller PCB.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
MN-CONT | Display of MNCON firmware version
Lv.1 | Details | To display the firmware version of Main Controller PCB.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
DIAG-DVC | Dis of self diagnosis device ROM version
Lv.1 | Details | To display the ROM version of self diagnosis device.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
RUI | Display of remote UI version
Lv.1 | Details | To display the version of remote UI.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
PUNCH | Display of Finisher Inner Punch Unit
Lv.1 | Details | To display the version of Finisher Inner Punch Unit.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
LANG-EN | Display of English language file version
Lv.1 | Details | To display the version of English language file.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
LANG-FR | Display of French language file version
Lv.1 | Details | To display the version of French language file.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
LANG-DE | Display of German language file version
Lv.1 | Details | To display the version of German language file.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
LANG-IT | Display of Italian language file version
Lv.1 | Details | To display the version of Italian language file.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
LANG-JP | Display of Japanese language file version
Lv.1 | Details | To display the version of Japanese language file.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
LANG-CS | Display of Czech language file version
Lv.2 | Details | To display the version of Czech language file.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
LANG-DA | Display of Danish language file version
Lv.2 | Details | To display the version of Danish language file.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
LANG-EL | Display of Greek language file version
Lv.2 | Details | To display the version of Greek language file.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
LANG-ES | Display of Spanish language file version
Lv.2 | Details | To display the version of Spanish language file.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
LANG-ET | Display of Estonian language file version
Lv.2 | Details | To display the version of Estonian language file.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
LANG-FI | Display of Finnish language file version
Lv.2 | Details | To display the version of Finnish language file.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
LANG-HU | Display of Hungarian language file version
Lv.2 | Details | To display the version of Hungarian language file.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
LANG-KO | Display of Korean language file version
Lv.2 | Details | To display the version of Korean language file.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
LANG-NL | Display of Dutch language file version
Lv.2 | Details | To display the version of Dutch language file.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
LANG-NO | Display of Norwegian language file version
Lv.2 | Details | To display the version of Norwegian language file.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
LANG-PL | Display of Polish language file version
Lv.2 | Details | To display the version of Polish language file.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
LANG-PT | Display of Portuguese language file version
Lv.2 | Details | To display the version of Portuguese language file.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
LANG-RU | Display of Russian language file version
Lv.2 | Details | To display the version of Russian language file.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
LANG-SL | Display of Slovenian language file version
Lv.2 | Details | To display the version of Slovenian language file.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
LANG-SV | Display of Swedish language file version
Lv.2 | Details | To display the version of Swedish language file.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
LANG-TW | Display of Chinese language file version: traditional
Lv.2 | Details | To display the version of Chinese language file (traditional).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
LANG-ZH | Display of Chinese language file version: smple
Lv.2 | Details | To display the version of Chinese language file (simplified).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
LANG-BU | Display of Bulgarian language file version
Lv.2 | Details | To display the version of Bulgarian language file.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
LANG-CR | Display of Croatian language file version
Lv.2 | Details | To display the version of Croatian language file.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
LANG-RM | Display of Romanian language file version
Lv.2 | Details | To display the version of Romanian language file.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
LANG-SK | Display of Slovak language file version
Lv.2 | Details | To display the version of Slovak language file.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
LANG-TK | Display of Turkish language file version
Lv.2 | Details | To display the version of Turkish language file.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
MEAP | Display of MEAP contents version
Lv.2 | Details | To display the version of MEAP contents in HDD.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
OCR-CN | Display of Chinese OCR version : simplified
Lv.2 | Details | "To display the version of Chinese OCR (simplified). ""--.--"" is displayed when no file is found."
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
OCR-JP | Display of Japanese OCR version
Lv.1 | Details | "To display the version of Japanese OCR. ""--.--"" is displayed when no file is found."
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
OCR-KR | Display of Korean OCR version
Lv.1 | Details | To display the version of Korean OCR. ""--.--"" is displayed when no file is found.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
OCR-TW | Display of Chinese OCR version : traditional
Lv.1 | Details | To display the version of Chinese OCR (traditional). ""--.--"" is displayed when no file is found.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
TTS-JA | Dis of Japanese voice dictionary version
Lv.1 | Details | To display the version of Japanese voice dictionary. ""--.--"" is displayed when no file is found.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
TTS-EN | Dis of English voice dictionary version
Lv.1 | Details | To display the version of English voice dictionary. ""--.--"" is displayed when no file is found.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
TTS-IT | Dis of Italian voice dictionary version
Lv.1 | Details | To display the version of Italian voice dictionary. ""--.--"" is displayed when no file is found.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
TTS-FR | Dis of French voice dictionary version
Lv.1 | Details | To display the version of French voice dictionary. ""--.--"" is displayed when no file is found.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
TTS-ES | Dis of Spanish voice dictionary version
Lv.1 | Details | To display the version of Spanish voice dictionary. ""--.--"" is displayed when no file is found.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
TTS-DE | Dis of German voice dictionary version
Lv.1 | Details | "To display the version of German voice dictionary. ""--.--"" is displayed when no file is found."
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
WEB-BRWS | Display of Web browser version
Lv.1 | Details | "To display the version of Web browser. ""--.--"" is displayed when no file is found."
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
HELP | Display of easy NAVI version
Lv.1 | Details | To display the version of "EASY NAVI" file.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
LANG-CA | Display of Catalan language file version
Lv.2 | Details | To display the version of Catalan language file.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
WEBDAV | Display of WebDAV version
Lv.1 | Details | "To display the version of ""WebDAV"" file. ""--.--"" is displayed when no file is found."
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
TIMESTMP | Display of timestamp version
Lv.1 | Details | "To display the version of ""Time Stamp"" file. ""--.--"" is displayed when no file is found."
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
ASR-JA | Display of Japanese ASR dictionary version
Lv.1 | Details | "To display the version of Japanese automatic speech recognition dictionary. ""--.--"" is displayed when no file is found."
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
ASR-EN | Dis of English ASR dictionary version
Lv.1 | Details | To display the version of English automatic speech recognition dictionary. ""--.--"" is displayed when no file is found.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
MEDIA-JA | Display of Japanese media information version
Lv.2 | Details | To display the version of Japanese media information.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
MEDIA-EN | Display of English media information version
Lv.2 | Details | To display the version of English media information.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
MEDIA-DE | Display of German media information version
Lv.2 | Details | To display the version of German media information.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
MEDIA-IT | Display of Italian media information version
Lv.2 | Details | To display the version of Italian media information.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
MEDIA-FR | Dis of French media information version
Lv.2 | Details | To display the version of French media information.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
MEDIA-ZH | Display of Chinese media info version : smple
Lv.2 | Details | To display the version of Chinese media information (simplified).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
MEDIA-SK | Display of Slovak media information version
Lv.2 | Details | To display the version of Slovak media information.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
MEDIA-TK | Display of Turkish media information version
Lv.2 | Details | To display the version of Turkish media information.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
MEDIA-CS | Display of Czech media information version
Lv.2 | Details | To display the version of Czech media information.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
MEDIA-EL | Display of Greek media information version
Lv.2 | Details | To display the version of Greek media information.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
MEDIA-ES | Display of Spanish media information version
Lv.2 | Details | To display the version of Spanish media information.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
MEDIA-ET | Display of Estonian media information version
Lv.2 | Details | To display the version of Estonian media information.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
MEDIA-FI | Display of Finnish media information version
Lv.2 | Details | To display the version of Finnish media information.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
MEDIA-HU | Display of Hungarian media information version
Lv.2 | Details | To display the version of Hungarian media information.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
MEDIA-KO | Display of Korean media information version
Lv.2 | Details | To display the version of Korean media information.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
MEDIA-NL | Display of Dutch media information version
Lv.2 | Details | To display the version of Dutch media information.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
MEDIA-NO | Display of Norwegian media information version
Lv.2 | Details | To display the version of Norwegian media information.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
MEDIA-PL | Display of Polish media information version
Lv.2 | Details | To display the version of Polish media information.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
MEDIA-PT | Display of Portuguese media information version
Lv.2 | Details | To display the version of Portuguese media information.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
MEDIA-RU | Display of Russian media information version
Lv.2 | Details | To display the version of Russian media information.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
MEDIA-SL | Display of Slovenian media information version
Lv.2 | Details | To display the version of Slovenian media information.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
MEDIA-SV | Display of Swedish media information version
Lv.2 | Details | To display the version of Swedish media information.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
MEDIA-TW | Display of Chinese media info version:traditional
Lv.2 | Details | To display the version of Chinese media information (traditional).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
MEDIA-BU | Display of Bulgarian media information version
Lv.2 | Details | To display the version of Bulgarian media information.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
MEDIA-CR | Display of Croatian media information version
Lv.2 | Details | To display the version of Croatian media information.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
MEDIA-RM | Display of Romanian media information version
Lv.2 | Details | To display the version of Romanian media information.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
MEDIA-CA | Display of Catalan media information version
Lv.2 | Details | To display the version of Catalan media information.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
FAX1 | Display of 1-line FAX PCB ROM version
Lv.2 | Details | "To display the ROM version of 1-line FAX PCB. ""NULL"" is displayed if the PCB is not connected."
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | ASCII character string (21 digits)
FAX2/3/4 | Display of 2/3/4-line FAX PCB ROM version
Lv.2 | Details | "To display the ROM version of 2/3/4-line FAX PCB. ""NULL"" is displayed if the PCB is not connected."
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | ASCII character string (21 digits)
IOCS | Display of BIOS version
Lv.2 | Details | To display the BIOS version.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
SYSTEM | Display of Linux kernel/tool/driver/file version
Lv.2 | Details | To display the version of Linux kernel/tool/driver/file.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
ROOT | Display of ROOT version
Lv.2 | Details | To display the ROOT version.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
S-LNG-JP | Display of service mode Japanese file version
Lv.1 | Details | To display the version of Japanese language file in service mode.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
S-LNG-EN | Display of service mode English file version
Lv.1 | Details | To display the version of English language file in service mode.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
S-LNG-FR | Display of service mode French file version
Lv.1 | Details | To display the version of French language file in service mode.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
S-LNG-IT | Display of service mode Italian file version
Lv.1 | Details | To display the version of Italian language file in service mode.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
S-LNG-GR | Display of service mode German file version
Lv.1 | Details | To display the version of German language file in service mode.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
S-LNG-SP | Display of service mode Spanish file version
Lv.1 | Details | To display the version of Spanish language file in service mode.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
UI-RES | Display of UI resource file version
Lv.1 | Details | "To display the UIRES version. UIRES consists of the resource file which is necessary to display the native screen (top screen and software keyboard screen) of UI."
Use case | When checking the version at the time of downloading UIRES to MFP
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
COPY-AP | Display of COPY (JAVA UI) version
Lv.1 | Details | To display the version of COPY application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
SEND-AP | Display of SEND (JAVA UI) version
Lv.1 | Details | To display the version of SEND application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
BOX-AP | Display of BOX (JAVA UI) version
Lv.1 | Details | To display the version of BOX application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
MOBPR-AP | Display of mobile print(JAVA UI) version
Lv.1 | Details | To display the version of the mobile print application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
RPTL-AP | Display of RUI portal version
Lv.1 | Details | To display the RUI portal version.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
INTRO-AP | Dis of useful func introduce appli ver
Lv.1 | Details | To display the version of Introduction to Useful Features application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
TSP-JLK | Display of PCAM Option Board version
Lv.1 | Details | To display the version of the PCAM Option Board.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
COPY-FR | Display of COPY appli French file version
Lv.1 | Details | To display the French language file version of COPY application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
COPY-IT | Display of COPY appli Italian file version
Lv.1 | Details | To display the Italian language file version of COPY application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
COPY-DE | Display of COPY appli German file version
Lv.1 | Details | To display the German language file version of COPY application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
COPY-ES | Display of COPY appli Spanish file version
Lv.1 | Details | To display the Spanish language file version of COPY application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
COPY-ZH | Display COPY appli Chinese file version: simple
Lv.2 | Details | To display the simplified Chinese language file version of COPY application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
COPY-TW | Display of COPY appli Chinese file ver:traditional
Lv.2 | Details | To display the traditional Chinese language file version of COPY application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
COPY-KO | Display of COPY appli Korean file version
Lv.2 | Details | To display the Korean language file version of COPY application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
COPY-CS | Dis of COPY appli Czech file version
Lv.2 | Details | To display the Czech language file version of COPY application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
COPY-DA | Display of COPY appli Danish file version
Lv.2 | Details | To display the Danish language file version of COPY application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
COPY-EL | Display of COPY appli Greek file version
Lv.2 | Details | To display the Greek language file version of COPY application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
COPY-ET | Display of COPY appli Estonian file version
Lv.2 | Details | To display the Estonian language file version of COPY application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
COPY-FI | Display of COPY appli Finnish file version
Lv.2 | Details | To display the Finnish language file version of COPY application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
COPY-HU | Display of COPY appli Hungarian file version
Lv.2 | Details | To display the Hungarian language file version of COPY application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
COPY-NL | Display of COPY appli Dutch file version
Lv.2 | Details | To display the Dutch language file version of COPY application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
COPY-NO | Display of COPY appli Norwegian file version
Lv.2 | Details | To display the Norwegian language file version of COPY application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
COPY-PL | Display of COPY appli Polish file version
Lv.2 | Details | To display the Polish language file version of COPY application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
COPY-PT | Display of COPY appli Portuguese file version
Lv.2 | Details | To display the Portuguese language file version of COPY application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
COPY-RU | Display of COPY appli Russian file version
Lv.2 | Details | To display the Russian language file version of COPY application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
COPY-SL | Display of COPY appli Slovenian file version
Lv.2 | Details | To display the Slovenian language file version of COPY application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
COPY-SV | Display of COPY appli Swedish file version
Lv.2 | Details | To display the Swedish language file version of COPY application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
COPY-ID | Display of COPY appli Indonesian file version
Lv.2 | Details | To display the Indonesian language file version of COPY application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
COPY-BU | Display of COPY appli Bulgarian file version
Lv.2 | Details | To display the Bulgarian language file version of COPY application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
COPY-CR | Display of COPY appli Croatian file version
Lv.2 | Details | To display the Croatian language file version of COPY application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
COPY-RM | Display of COPY appli Romanian file version
Lv.2 | Details | To display the Romanian language file version of COPY application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
COPY-SK | Display of COPY appli Slovak file version
Lv.2 | Details | To display the Slovak language file version of COPY application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
COPY-TK | Display of COPY appli Turkish file version
Lv.2 | Details | To display the Turkish language file version of COPY application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
COPY-CA | Display of COPY appli Catalan file version
Lv.2 | Details | To display the Catalan language file version of COPY application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
COPY-TH | Display of COPY appli Thai file version
Lv.2 | Details | To display the Thai language file version of COPY application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
COPY-VN | Dis of COPY appli Vietnamese file ver
Lv.2 | Details | To display the Vietnamese language file version of COPY application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
SEND-FR | Display of SEND appli French file version
Lv.2 | Details | To display the French language file version of SEND application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
SEND-IT | Display of SEND appli Italian file version
Lv.2 | Details | To display the Italian language file version of SEND application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
SEND-DE | Display of SEND appli German file version
Lv.2 | Details | To display the German language file version of SEND application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
SEND-ES | Display of SEND appli Spanish file version
Lv.2 | Details | To display the Spanish language file version of SEND application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
SEND-ZH | Display SEND appli Chinese file version: simple
Lv.2 | Details | To display the simplified Chinese language file version of SEND application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
SEND-TW | Display of SEND appli Chinese file ver:traditional
Lv.2 | Details | To display the traditional Chinese language file version of SEND application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
SEND-KO | Display of SEND appli Korean file version
Lv.2 | Details | To display the Korean language file version of SEND application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
SEND-CS | Display of SEND appli Czech file version
Lv.2 | Details | To display the Czech language file version of SEND application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
SEND-DA | Display of SEND appli Danish file version
Lv.2 | Details | To display the Danish language file version of SEND application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
SEND-EL | Display of SEND appli Greek file version
Lv.2 | Details | To display the Greek language file version of the SEND application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
SEND-ET | Display of SEND appli Estonian file version
Lv.2 | Details | To display the Estonian language file version of SEND application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
SEND-FI | Display of SEND appli Finnish file version
Lv.2 | Details | To display the Finnish language file version of SEND application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
SEND-HU | Display of SEND appli Hungarian file version
Lv.2 | Details | To display the Hungarian language file version of SEND application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
SEND-NL | Display of SEND appli Dutch file version
Lv.2 | Details | To display the Dutch language file version of SEND application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
SEND-NO | Display of SEND appli Norwegian file version
Lv.2 | Details | To display the Norwegian language file version of SEND application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
SEND-PL | Display of SEND appli Polish file version
Lv.2 | Details | To display the Polish language file version of SEND application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
SEND-PT | Display of SEND appli Portuguese file version
Lv.2 | Details | To display the Portuguese language file version of SEND application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
SEND-RU | Display of SEND appli Russian file version
Lv.2 | Details | To display the Russian language file version of SEND application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
SEND-SL | Display of SEND appli Slovenian file version
Lv.2 | Details | To display the Slovenian language file version of SEND application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
SEND-SV | Display of SEND appli Swedish file version
Lv.2 | Details | To display the Swedish language file version of SEND application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
SEND-ID | Display of SEND appli Indonesian file version
Lv.2 | Details | To display the Indonesian language file version of SEND application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
SEND-BU | Display of SEND appli Bulgarian file version
Lv.2 | Details | To display the Bulgarian language file version of SEND application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
SEND-CR | Display of SEND appli Croatian file version
Lv.2 | Details | To display the Croatian language file version of SEND application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
SEND-RM | Display of SEND appli Romanian file version
Lv.2 | Details | To display the Romanian language file version of SEND application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
SEND-SK | Display of SEND appli Slovak file version
Lv.2 | Details | To display the Slovak language file version of SEND application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
SEND-TK | Display of SEND appli Turkish file version
Lv.2 | Details | To display the Turkish language file version of SEND application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
SEND-CA | Display of SEND appli Catalan file version
Lv.2 | Details | To display the Catalan language file version of SEND application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
SEND-TH | Display of SEND appli Thai file version
Lv.2 | Details | To display the Thai language file version of SEND application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
SEND-VN | Dis of SEND appli Vietnamese file ver
Lv.2 | Details | To display the Vietnamese language file version of SEND application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
INTRO-FR | Display of useful func intro French file version
Lv.2 | Details | To display the version of French language file of Introduction to Useful Features application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
INTRO-IT | Display of useful func intro Italian file version
Lv.2 | Details | To display the version of Italian language file of Introduction to Useful Features application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
INTRO-DE | Display of useful func intro German file version
Lv.2 | Details | To display the version of German language file of Introduction to Useful Features application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
INTRO-ES | Display of useful func intro Spanish file version
Lv.2 | Details | To display the version of Spanish language file of Introduction to Useful Features application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
INTRO-ZH | Display of useful func intro Chinese file version: simple
Lv.2 | Details | To display the version of simplified Chinese language file of Introduction to Useful Features application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
INTRO-TW | Display of useful func intro Chinese file version: traditional
Lv.2 | Details | To display the version of traditional Chinese language file of Introduction to Useful Features application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
INTRO-KO | Display of dis of useful func intro Korean file version
Lv.2 | Details | To display the version of Korean language file of Introduction to Useful Features application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
INTRO-CS | Display of useful func intro Czech file version
Lv.2 | Details | To display the version of Czech language file of Introduction to Useful Features application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
INTRO-DA | Display of useful func intro Danish file version
Lv.2 | Details | To display the version of Danish language file of Introduction to Useful Features application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
INTRO-EL | Display of useful func intro Greek file version
Lv.2 | Details | To display the version of Greek language file of Introduction to Useful Features application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
INTRO-ET | Display useful func intro Estonian file version
Lv.2 | Details | To display the version of Estonian language file of Introduction to Useful Features application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
INTRO-FI | Display useful func intro Finnish file version
Lv.2 | Details | To display the version of Finnish language file of Introduction to Useful Features application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
INTRO-HU | Display useful func intro Hungarian file version
Lv.2 | Details | To display the version of Hungarian language file of Introduction to Useful Features application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
INTRO-NL | Display of useful func intro Dutch file version
Lv.2 | Details | To display the version of Dutch language file of Introduction to Useful Features application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
INTRO-NO | Display useful func intro Norwegian file version
Lv.2 | Details | To display the version of Norwegian language file of Introduction to Useful Features application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
INTRO-PL | Display of useful func intro Polish file version
Lv.2 | Details | To display the version of Polish language file of Introduction to Useful Features application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
INTRO-PT | Display useful func intro Portuguese file version
Lv.2 | Details | To display the version of Portuguese language file of Introduction to Useful Features application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
INTRO-RU | Display useful func intro Russian file version
Lv.2 | Details | To display the version of Russian language file of Introduction to Useful Features application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
INTRO-SL | Display useful func intro Slovenian file version
Lv.2 | Details | To display the version of Slovenian language file of Introduction to Useful Features application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
INTRO-SV | Display of useful func intro Swedish file version
Lv.2 | Details | To display the version of Swedish language file of Introduction to Useful Features application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
INTRO-ID | Display of useful func intro Indonesian file version
Lv.2 | Details | To display the version of Indonesian language file of Introduction to Useful Features application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
INTRO-BU | Display useful func intro Bulgarian file version
Lv.2 | Details | To display the version of Bulgarian language file of Introduction to Useful Features application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
INTRO-CR | Display useful func intro Croatian file version
Lv.2 | Details | To display the version of Croatian language file of Introduction to Useful Features application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
INTRO-RM | Display useful func intro Romanian file version
Lv.2 | Details | To display the version of Romanian language file of Introduction to Useful Features application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
INTRO-SK | Display of useful func intro Slovak file version
Lv.2 | Details | To display the version of Slovak language file of Introduction to Useful Features application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
INTRO-TK | Display useful func intro Turkish file version
Lv.2 | Details | To display the version of Turkish language file of Introduction to Useful Features application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
INTRO-CA | Display useful func intro Catalan file version
Lv.2 | Details | To display the version of Catalan language file of Introduction to Useful Features application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
INTRO-TH | Display useful func intro Thai file ver
Lv.2 | Details | To display the version of Thai language file of Introduction to Useful Features application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
INTRO-VN | Dis usful func intro Vietnamese file ver
Lv.2 | Details | To display the version of Vietnamese language file of Introduction to Useful Features application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
CSTMN-FR | Display of custom menu French file version
Lv.2 | Details | To display the version of French language file for custom menu application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
CSTMN-IT | Display of custom menu Italian file version
Lv.2 | Details | To display the version of Italian language file for custom menu application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
CSTMN-DE | Display of custom menu German file version
Lv.2 | Details | To display the version of German language file for custom menu application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
CSTMN-ES | Display of custom menu Spanish file version
Lv.2 | Details | To display the version of Spanish language file for custom menu application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
CSTMN-ZH | Display of custom menu Chinese file ver: simple
Lv.2 | Details | To display the version of simplified Chinese language file for custom menu application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
CSTMN-TW | Dis of custom menu Chinese file ver:trad
Lv.2 | Details | To display the version of traditional Chinese language file for custom menu application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
CSTMN-KO | Display of custom menu Korean file version
Lv.2 | Details | To display the version of Korean language file for custom menu application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
CSTMN-CS | Display of custom menu Czech file version
Lv.2 | Details | To display the version of Czech language file for custom menu application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
CSTMN-DA | Display of custom menu Danish file version
Lv.2 | Details | To display the version of Danish language file for custom menu application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
CSTMN-EL | Display of custom menu Greek file version
Lv.2 | Details | To display the version of Greek language file for custom menu application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
CSTMN-ET | Display of custom menu Estonian file version
Lv.2 | Details | To display the version of Estonian language file for custom menu application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
CSTMN-FI | Display of custom menu Finnish file version
Lv.2 | Details | To display the version of Finnish language file for custom menu application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
CSTMN-HU | Display of custom menu Dutch file version
Lv.2 | Details | To display the version of Dutch language file for custom menu application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
CSTMN-NL | Display of custom menu Dutch file ver
Lv.2 | Details | To display the version of Dutch language file for custom menu application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
CSTMN-NO | Display of custom menu Norwegian file ver
Lv.2 | Details | To display the version of Norwegian language file for custom menu application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
CSTMN-PL | Display of custom menu Polish file version
Lv.2 | Details | To display the version of Polish language file for custom menu application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
CSTMN-PT | Display of custom menu Portuguese file version
Lv.2 | Details | To display the version of Portuguese language file for custom menu application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
CSTMN-RU | Display of custom menu Russian file version
Lv.2 | Details | To display the version of Russian language file for custom menu application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
CSTMN-SL | Display of custom menu Slovenian file version
Lv.2 | Details | To display the version of Slovenian language file for custom menu application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
CSTMN-SV | Display of custom menu Swedish file version
Lv.2 | Details | To display the version of Swedish language file for custom menu application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
CSTMN-ID | Display of custom menu Indonesian file version
Lv.2 | Details | To display the version of Indonesian language file for custom menu application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
CSTMN-BU | Dis of custom menu Bulgarian file version
Lv.2 | Details | To display the version of Bulgarian language file for custom menu application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
CSTMN-CR | Dis of custom menu Croatian file version
Lv.2 | Details | To display the version of Croatian language file for custom menu application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
CSTMN-RM | Dis of custom menu Rumanian file version
Lv.2 | Details | To display the version of Rumanian language file for custom menu application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
CSTMN-SK | Display of custom menu Slovak file version
Lv.2 | Details | To display the version of Slovak language file for custom menu application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
CSTMN-TK | Display of custom menu Turkish file version
Lv.2 | Details | To display the version of Turkish language file for custom menu application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
CSTMN-CA | Display of custom menu Catalan file version
Lv.2 | Details | To display the version of Catalan language file for custom menu application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
CSTMN-TH | Display of custom menu Thai file version
Lv.2 | Details | To display the version of Thai language file for custom menu application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
CSTMN-VN | Dis of custom menu Vietnamese file ver
Lv.2 | Details | To display the version of Vietnamese language file for custom menu application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
ACSBT-FR | Display of accessibility French file version
Lv.2 | Details | To display the version of French language file for Accessibility application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
ACSBT-IT | Display of accessibility Italian file version
Lv.2 | Details | To display the version of Italian language file for Accessibility application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
ACSBT-DE | Display of accessibility German file version
Lv.2 | Details | To display the version of German language file for Accessibility application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
ACSBT-ES | Display of accessibility Spanish file version
Lv.2 | Details | To display the version of Spanish language file for Accessibility application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
ACSBT-ZH | Display Accessibility Chinese file version: simple
Lv.2 | Details | To display the version of simplified Chinese language file for Accessibility application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
ACSBT-TW | Display accessibility Chinese file version:traditional
Lv.2 | Details | To display the version of traditional Chinese language file for Accessibility application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
ACSBT-KO | Display of accessibility Korean file version
Lv.2 | Details | To display the version of Korean language file for Accessibility application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
ACSBT-CS | Display of accessibility Czech file version
Lv.2 | Details | To display the version of Czech language file for Accessibility application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
ACSBT-DA | Display of accessibility Danish file version
Lv.2 | Details | To display the version of Danish language file for Accessibility application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
ACSBT-EL | Display of accessibility Greek file version
Lv.2 | Details | To display the version of Greek language file for Accessibility application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
ACSBT-ET | Display of accessibility Estonian file version
Lv.2 | Details | To display the version of Estonian language file for Accessibility application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
ACSBT-FI | Display of accessibility Finnish file version
Lv.2 | Details | To display the version of Finnish language file for Accessibility application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
ACSBT-HU | Display of accessibility Hungarian file version
Lv.2 | Details | To display the version of Hungarian language file for Accessibility application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
ACSBT-NL | Display of accessibility Dutch file version
Lv.2 | Details | To display the version of Dutch language file for Accessibility application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
ACSBT-NO | Display of accessibility Norwegian file version
Lv.2 | Details | To display the version of Norwegian language file for Accessibility application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
ACSBT-PL | Display of accessibility Polish file version
Lv.2 | Details | To display the version of Polish language file for Accessibility application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
ACSBT-PT | Display of accessibility Portuguese file version
Lv.2 | Details | To display the version of Portuguese language file for Accessibility application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
ACSBT-RU | Display of accessibility Russian file version
Lv.2 | Details | To display the version of Russian language file for Accessibility application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
ACSBT-SL | Display of accessibility Slovenian file version
Lv.2 | Details | To display the version of Slovenian language file for Accessibility application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
ACSBT-SV | Display of accessibility Swedish file version
Lv.2 | Details | To display the version of Swedish language file for Accessibility application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
ACSBT-ID | Display of accessibility Indonesian file version
Lv.2 | Details | To display the version of Indonesian language file for Accessibility application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
ACSBT-BU | Display of accessibility Bulgarian file version
Lv.2 | Details | To display the version of Bulgarian language file for Accessibility application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
ACSBT-CR | Display of accessibility Croatian file version
Lv.2 | Details | To display the version of Croatian language file for Accessibility application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
ACSBT-RM | Display of accessibility Romanian file version
Lv.2 | Details | To display the version of Romanian language file for Accessibility application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
ACSBT-SK | Display of accessibility Slovak file version
Lv.2 | Details | To display the version of Slovak language file for Accessibility application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
ACSBT-TK | Display of accessibility Turkish file version
Lv.2 | Details | To display the version of Turkish language file for Accessibility application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
ACSBT-CA | Display of accessibility Catalan file version
Lv.2 | Details | To display the version of Catalan language file for Accessibility application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
ACSBT-TH | Display of accessibility Thai file ver
Lv.2 | Details | To display the version of Thai language file for Accessibility application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
ACSBT-VN | Dis of accessibility Vietnamese file ver
Lv.2 | Details | To display the version of Vietnamese language file for Accessibility application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
ERS-FR | Display of ERS French file version
Lv.2 | Details | To display the version of French language file for ERS application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
ERS-IT | Display of ERS Italian file version
Lv.2 | Details | To display the version of Italian language file for ERS application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
ERS-DE | Display of ERS German file version
Lv.2 | Details | To display the version of German language file for ERS application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
ERS-ES | Display of ERS Spanish file version
Lv.2 | Details | To display the version of Spanish language file for ERS application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
ERS-ZH | Display of ERS Chinese file version:simple
Lv.2 | Details | To display the version of simplified Chinese language file for ERS application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
ERS-TW | Display of ERS Chinese file version:traditional
Lv.2 | Details | To display the version of traditional Chinese language file for ERS application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
ERS-KO | Display of ERS Korean file version
Lv.2 | Details | To display the version of Korean language file for ERS application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
ERS-CS | Display of ERS Czech file version
Lv.2 | Details | To display the version of Czech language file for ERS application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
ERS-DA | Display of ERS Danish file version
Lv.2 | Details | To display the version of Danish language file for ERS application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
ERS-EL | Display of ERS Greek file version
Lv.2 | Details | To display the version of Greek language file for ERS application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
ERS-ET | Display of ERS Estonian file version
Lv.2 | Details | To display the version of Estonian language file for ERS application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
ERS-FI | Display of ERS Finnish file version
Lv.2 | Details | To display the version of Finnish language file for ERS application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
ERS-HU | Display of ERS Hungarian file version
Lv.2 | Details | To display the version of Hungarian language file for ERS application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
ERS-NL | Display of ERS Dutch file version
Lv.2 | Details | To display the version of Dutch language file for ERS application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
ERS-NO | Display of ERS Norwegian file version
Lv.2 | Details | To display the version of Norwegian language file for ERS application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
ERS-PL | Display of ERS Polish file version
Lv.2 | Details | To display the version of Polish language file for ERS application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
ERS-PT | Display of ERS Portuguese file version
Lv.2 | Details | To display the version of Portuguese language file for ERS application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
ERS-RU | Display of ERS Russian file version
Lv.2 | Details | To display the version of Russian language file for ERS application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
ERS-SL | Display of ERS Slovenian file version
Lv.2 | Details | To display the version of Slovenian language file for ERS application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
ERS-SV | Display of ERS Swedish file version
Lv.2 | Details | To display the version of Swedish language file for ERS application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
ERS-ID | Display of ERS Indonesian file version
Lv.2 | Details | To display the version of Indonesian language file for ERS application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
ERS-BU | Display of ERS Bulgarian file version
Lv.2 | Details | To display the version of Bulgarian language file for ERS application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
ERS-CR | Display of ERS Croatian file version
Lv.2 | Details | To display the version of Croatian language file for ERS application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
ERS-RM | Display of ERS Romanian file version
Lv.2 | Details | To display the version of Romanian language file for ERS application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
ERS-SK | Display of ERS Slovak file version
Lv.2 | Details | To display the version of Slovak language file for ERS application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
ERS-TK | Display of ERS Turkish file version
Lv.2 | Details | To display the version of Turkish language file for ERS application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
ERS-CA | Display of ERS Catalan file version
Lv.2 | Details | To display the version of Catalan language file for ERS application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
ERS-TH | Display of ERS Thai file version
Lv.2 | Details | To display the version of Thai language file for ERS application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
ERS-VN | Display of ERS Vietnamese file version
Lv.2 | Details | To display the version of Vietnamese language file for ERS application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
NLS-FR | Display of UAC French file version
Lv.1 | Details | To display the version of French language file for UAC application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
NLS-IT | Display of UAC Italian file version
Lv.1 | Details | To display the version of Italian language file for UAC application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
NLS-DE | Display of UAC German file version
Lv.1 | Details | To display the version of German language file for UAC application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
NLS-ES | Display of UAC Spanish file version
Lv.1 | Details | To display the version of Spanish language file for UAC application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
NLS-ZH | Display of UAC Chinese file version:simple
Lv.2 | Details | To display the version of simplified Chinese language file for UAC application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
NLS-TW | Display of UAC Chinese file version:traditional
Lv.2 | Details | To display the version of traditional Chinese language file for UAC application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
NLS-KO | Display of UAC Korean file version
Lv.2 | Details | To display the version of Korean language file for UAC application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
NLS-CS | Display of UAC Czech file version
Lv.2 | Details | To display the version of Czech language file for UAC application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
NLS-DA | Display of UAC Danish file version
Lv.2 | Details | To display the version of Danish language file for UAC application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
NLS-EL | Display of UAC Greek file version
Lv.2 | Details | To display the version of Greek language file for UAC application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
NLS-ET | Display of UAC Estonian file version
Lv.2 | Details | To display the version of Estonian language file for UAC application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
NLS-FI | Display of UAC Finnish file version
Lv.2 | Details | To display the version of Finnish language file for UAC application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
NLS-HU | Display of UAC Hungarian file version
Lv.2 | Details | To display the version of Hungarian language file for UAC application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
NLS-NL | Display of UAC Dutch file version
Lv.2 | Details | To display the version of Dutch language file for UAC application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
NLS-NO | Display of UAC Norwegian file version
Lv.2 | Details | To display the version of Norwegian language file for UAC application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
NLS-PL | Display of UAC Polish file version
Lv.2 | Details | To display the version of Polish language file for UAC application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
NLS-PT | Display of UAC Portuguese file version
Lv.2 | Details | To display the version of Portuguese language file for UAC application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
NLS-RU | Display of UAC Russian file version
Lv.2 | Details | To display the version of Russian language file for UAC application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
NLS-SL | Display of UAC Slovenian file version
Lv.2 | Details | To display the version of Slovenian language file for UAC application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
NLS-SV | Display of UAC Swedish file version
Lv.2 | Details | To display the version of Swedish language file for UAC application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
NLS-ID | Display of UAC Indonesian file version
Lv.2 | Details | To display the version of Indonesian language file for UAC application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
NLS-BU | Display of UAC Bulgarian file version
Lv.2 | Details | To display the version of Bulgarian language file for UAC application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
NLS-CR | Display of UAC Croatian file version
Lv.2 | Details | To display the version of Croatian language file for UAC application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
NLS-RM | Display of UAC Romanian file version
Lv.2 | Details | To display the version of Romanian language file for UAC application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
NLS-SK | Display of UAC Slovak file version
Lv.2 | Details | To display the version of Slovak language file for UAC application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
NLS-TK | Display of UAC Turkish file version
Lv.2 | Details | To display the version of Turkish language file for UAC application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
NLS-CA | Display of UAC Catalan file version
Lv.2 | Details | To display the version of Catalan language file for UAC application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
BCT | Display of self diagnosis tool version
Lv.2 | Details | To display the version of self diagnosis tool.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
ASR-ES | Display of Spanish voice dictionary version
Lv.2 | Details | To display the version of Spanish voice dictionary.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
ASR-FR | Display of French voice dictionary version
Lv.2 | Details | To display the version of French voice dictionary.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
ASR-IT | Display of Italian voice dictionary version
Lv.2 | Details | To display the version of Italian voice dictionary.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
ASR-DE | Display of German voice dictionary version
Lv.2 | Details | To display the version of German voice dictionary.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
LANG-TH | Display of Thai language file version
Lv.2 | Details | To display the version of Thai language file.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
LANG-VN | Display of Vietnamese language file ver
Lv.2 | Details | To display the version of Vietnamese language file.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
BOX-FR | Display of BOX appli French file version
Lv.2 | Details | To display the version of French language file for BOX application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
BOX-IT | Display of BOX appli Italian file version
Lv.2 | Details | To display the version of Italian language file for BOX application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
BOX-DE | Display of BOX appli German file version
Lv.2 | Details | To display the version of German language file for BOX application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
BOX-ES | Display of BOX appli Spanish file version
Lv.2 | Details | To display the version of Spanish language file for BOX application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
BOX-ZH | Display of BOX appli Chinese file version:simple
Lv.2 | Details | To display the version of simplified Chinese language file for BOX application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
BOX-TW | Display of BOX appli Chinese file version:traditional
Lv.2 | Details | To display the version of traditional Chinese language file for BOX application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
BOX-KO | Display of BOX appli Korean file version
Lv.2 | Details | To display the version of Korean language file for BOX application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
BOX-CS | Display of BOX appli Czech file version
Lv.2 | Details | To display the version of Czech language file for BOX application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
BOX-DA | Display of BOX appli Danish file version
Lv.2 | Details | To display the version of Danish language file for BOX application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
BOX-EL | Display of BOX appli Greek file version
Lv.2 | Details | To display the version of Greek language file for BOX application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
BOX-ET | Dis of BOX appli Estonian file version
Lv.2 | Details | To display the version of Estonian language file for BOX application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
BOX-FI | Dis of BOX appli Finnish file version
Lv.2 | Details | To display the version of Finnish language file for BOX application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
BOX-HU | Display of BOX appli Hungarian file version
Lv.2 | Details | To display the version of Hungarian language file for BOX application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
BOX-NL | Display of BOX appli Dutch file version
Lv.2 | Details | To display the version of Dutch language file for BOX application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
BOX-NO | Display of BOX appli Norwegian file version
Lv.2 | Details | To display the version of Norwegian language file for BOX application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
BOX-PL | Display of BOX appli Polish file version
Lv.2 | Details | To display the version of Polish language file for BOX application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
BOX-PT | Display of BOX appli Portuguese file version
Lv.2 | Details | To display the version of Portuguese language file for BOX application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
BOX-RU | Display of BOX appli Russian file version
Lv.2 | Details | To display the version of Russian language file for BOX application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
BOX-SL | Display of BOX appli Slovenian file version
Lv.2 | Details | To display the version of Slovenian language file for BOX application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
BOX-SV | Display of BOX appli Swedish file version
Lv.2 | Details | To display the version of Swedish language file for BOX application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
BOX-ID | Display of BOX appli Indonesian file version
Lv.2 | Details | To display the version of Indonesian language file for BOX application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
BOX-BU | Display of BOX appli Bulgarian file version
Lv.2 | Details | To display the version of Bulgarian language file for BOX application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
BOX-CR | Display of BOX appli Croatian file version
Lv.2 | Details | To display the version of Croatian language file for BOX application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
BOX-RM | Display of BOX appli Romanian file version
Lv.2 | Details | To display the version of Romanian language file for BOX application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
BOX-SK | Display of BOX appli Slovak file version
Lv.2 | Details | To display the version of Slovak language file for BOX application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
BOX-TK | Display of BOX appli Turkish file version
Lv.2 | Details | To display the version of Turkish language file for BOX application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
BOX-CA | Display of BOX appli Catalan file version
Lv.2 | Details | To display the version of Catalan language file for BOX application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
BOX-TH | Display of BOX appli Thai file version
Lv.2 | Details | To display the version of Thai language file for BOX application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
BOX-VN | Dis of BOX appli Vietnamese file ver
Lv.2 | Details | To display the version of Vietnamese language file for BOX application (JAVA UI).
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
NLS-TH | Display of UAC Thai file version
Lv.2 | Details | To display the version of Thai language file for UAC application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
Supplement/memo | UAC: User Access Control
NLS-VN | Display of UAC Vietnamese file version
Lv.2 | Details | To display the version of Vietnamese language file for UAC application.
Use case | When upgrading the firmware
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 00.01 to 99.99
Supplement/memo | UAC: User Access Control