Function Supporting Deep Sleep Mode

| Print out this category

Function Supporting Deep Sleep Mode
Once the device shifted to the deep sleep mode, the USB device could not be controlled after recovery from the deep sleep mode. For this reason, it was necessary to control the application not to shift to the deep sleep mode.
With this function, the USB device control is enabled after recovery from the deep sleep mode as in the case when the USB device is inserted and removed (occurrence of disconnection/connection event) at recovery from the deep sleep mode.
In addition, this function enables the USB device control after shifting to the deep sleep mode, so the application needs to perform reconnection processing.
This function can be used with the device which MEAP Specifications Ver.54 is supported.