USB Device report print

| Print out this category

USB Device report print
To check the vendor IDs (idVendor) and the product IDs (idProduct) registered in this device by means of declaration in Manifest file of MEAP applications, output the USB Device repot report print.
Steps to output the USB Device report print
1) Start [ SERVICE MODE ] in Level 1.
2) Press [ COPIER ] > [ Function ] > [ MISC-P ].
3) Press or button for several times until [ USBH-PRT ] is shown. Press [ USBH-PRT ].
4) When pressing [ OK ] button, [ ACTIVE ] blinks on the status field.
5) When [ OK ] is shown on the status field, the status print is output. Check the contents of the print.
Example of output result
USB device information Content
Display the information of the USB device, which the device recognized.
If not displayed, there may be some fault occurred.
Some of standard optional devices are not displayed on a report.
The details of each item are as follows.
T : Topology
Internal hierarchical structure, which a USB device is connected, is shown. The number of a connected bus, the hierarchical structure and connection speed can be indicated.
D : Device
Information of USB devices is shown.
P : Product
Product information of USB devices is shown. Vendor ID and Product ID can be recognized here.
S : String
The character string embedded in a USB device is shown. A manufacture name and a product name can be recognized here.
C : Configure
The configuration information of a USB device is shown. * mark is to know whether it is active.
I : Interface
The interface information of a USB device is shown. Interface class and the driver to handle can be recognized.
The value and the content of Driver are as follows.

Labeling | Content
usbhid | It is displayed when the USB system driver is assigned to the input device connected.
usb-storage | It is displayed when storage devices (USB memory storage etc.) are connected.
irda-usb IrDA | It is displayed when the dongle is connected.
hub | It is displayed when HUB is connected.
gpusb | It is displayed when the USB driver only for MEAP application is assigned to the input device connected.
gpusbex | It is displayed when a USB device, which specific vendor ID/ Product ID are preferentially registered using a manifest and MEAP API, is connected and the USB driver only for MEAP application is assigned.

E:Endpoint
The Endpoint information of a USB device is shown.
Right or wrong of report output

Connecting device | User installation | Report printing
HID | Available | Yes
Storage | Available | Yes
FAX | Not available | No
USB Device Port | IrDA | Not available | Yes
Multimedia Card Reader | Not available | Yes
IC Card Reader | Not available | Yes
Image Data Analyzer Board-A1 | Not available | No
Hub | Internal Hub* | Not available | No
External Hub | Available | Yes

* USB Device Port-B1 Hub for device ports installed at the introduction
The content of MEAP preferred device information
Display the information of the application or a USB device, which preferentially registered with MEAP application.
By seeing this information, it can check which Application ID of the MEAP application is in the status using a specific USB device.
AppID : Application ID
VID : Vendor ID
PID : Product ID