Specifications

| Print out this category

Specifications

Item | Function/method
Fixing method | On-demand fixing
Fixing speed | Process Speed H | 233mm/sec (1/1-high speed: 1.4% speed-up)
233mm/sec (1/1-end speed: 0.9% speed-up)
230mm/sec (1/1-speed)
224mm/sec (1/1-slow speed: 4.5% speed-down)
Process Speed L | 139mm/sec (1/1-high speed: 1.4% speed-up)
139mm/sec (1/1-end speed: 0.9% speed-up)
137mm/sec (1/1-speed)
131mm/sec (1/1-slow speed: 4.5% speed-down)
Fixing heater | Ceramic heater
Control temperature | 215 deg C (Process speed H, plain paper 1, single sided) *1
Temperature detection | By the main thermistors and the sub thermistors (front) and (rear)
Cleaning control | Cleaning sequence control
Edge heat rising prevention control | Paper edge cooling fans (front)/(rear) and sequence control
Fixing loop control | Loop sensor
Protective Function | "Main thermistor and Sub thermistors (front)/(rear) Thermo Switch (operating temperature: 250 deg C)"

*1. Target temperature is specified depending on the process speed, the fixing mode and the fixing temperature at the start of warm-up control.