﻿Removing the Reader Assembly

| Print out this category

﻿Removing the Reader Assembly
<Procedure>
1) Disconnect the ADF cable.
2) Remove the reader left cover. (Reference)
3) Remove the reader right cover. (Reference)
4) Remove the reader rear cover. (Reference)
5) Remove the rear cover. (Reference)
6) Remove the controller cover.
7) Remove the reader front cover. (Reference)
8)Remove the operation panel. (Reference)
9) Release the cables from the wire saddle.
10) Remove the operation panel fixing plate .
8 Screws
11) Disconnect the connector of the reader.
12) Connect the flexible cable.
13) Attach the grounding plate (L/R).
5 Screws
14) Remove the 5 screws from the left side of the host machine.
15) Remove the 2 screws from the right side of the host machine.
16) Remove the reader assembly.