Login by RLS Authentication

| Print out this category

Login by RLS Authentication
Login without using the SMS login window but by entering the user ID and password for authentication in the RLS (Remote Login Service) window. The user information (user name and password) used is the information for domain authentication or local device authentication. The login procedures are as follows.
1) Access SMS by RLS Authentication from the PC browser on the same network as the MEAP device.
URL: https://<IP address of MEAP device>:8443/sms/rls/
Ex.) https://172.16.188.240:8443/sms/rls/
Note:
To encrypt the password information input when logging in, SSL of the login screen was made effective. However, it is redirected to new URL (effective SSL) even when accessing with URL (non-SSL) before.
Note:
When the device authentication method used is domain authentication, enter the user name, password and login destination registered with Active Directory and then click ‘Log In’.
If the authentication method used is local device authentication, enter the user name, password and login destination registered in the device and click ‘Log In’. - When using SDL as the login service, enter the user information registered in the device, as per local device authentication.
The user information is set as below for local device authentication by default. Both are case sensitive.
- User Name: Administrator
- Password: password
Note:
Only the following users may us SMS via RLS.
- In the case of domain authentication, users belonging to the Canon Peripheral Admins Group.
- For local device authentication, users with Administrator or Device Admin authority.
SMS Access can be gained also from Remote UI.
Access Remote UI and click on SMS shortcut shown on the lower right of the screen to gain access to SMS.
When only the password authentication is enabled, the password authentication screen is shown.
When only the RLS authentication is enabled, no further authentication is needed to access SMS. This is because users have already authorized upon accessing to Remote UI.
CAUTION:
In case that the login method to a device is set to SSO-H, if you log in SMS with RLS authentication, no selection is displayed although it is the screen to change the login method.
This is the specification to prevent the inconsistent setting which enables to stop SMS Installer Service (Password Authentication) by changing the login method to Default Authentication.
When you want to change the login method to a device, log in the SMS with the password authentication.