ADJ-XY

| Print out this category

ADJ-XY

COPIER>ADJUST>ADJ-XY
ADJ-X | Adj of img pstn in book mode: vert scan

Lv.1

Details

To adjust the image reading start position (image leading edge position) in vertical scanning direction.
When replacing the CCD unit (CCD PCB)/clearing RAM data, enter the value of service label.
When the non-image width is larger than the standard value, set the smaller value.
When out of original area is copied, set the larger value.
As the value is incremented by 1, the image position moves to the trailing edge side by 0.1mm.

Use case | When replacing the CCD unit (CCD PCB)/clearing RAM data
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | Do not use this at the normal service.
Display/adj/set range | 1 to 100
Unit | 0.1 mm
Default value | 29
ADJ-Y | Adj of img pstn in book mode: horz scan

Lv.1

Details

To adjust the image reading start position in horizontal scanning direction.
When replacing the CCD unit (CCD PCB)/clearing RAM data, enter the value of service label.
When the non-image width is larger than the standard value, set the smaller value.
When out of original area is copied, set the larger value.
As the value is incremented by 1, the image position moves to the rear side by 0.1mm.

Use case | When replacing the CCD unit (CCD PCB)/clearing RAM data
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | 45 to 254
Unit | 0.1 mm
Default value | 78
ADJ-S | Adj of reading start pstn for CCD: horz scan
Lv.1 | Details | To adjust the image reading start position for CCD in horizontal scanning direction. When replacing the CCD unit (CCD PCB)/clearing RAM data, enter the value of service label.
Use case | When replacing the CCD unit (CCD PCB)/clearing RAM data
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | 20 to 500
Unit | 0.1 mm
Default value | 121
ADJ-Y-DF | Adj img pstn in DADF mode:horz scan[Frt]
Lv.1 | Details | To adjust the image reading start position in horizontal scanning direction at DADF reading. When replacing the CCD unit (CCD PCB)/clearing RAM data, enter the value of service label. As the value is incremented by 1, the image position moves to the rear side by 0.1mm.
Use case | When replacing the CCD unit (CCD PCB)/clearing RAM data
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | 2 to 202
Unit | 0.1 mm
Default value | 78
STRD-POS | Adj read pstn in DADF mode: front side
Lv.1 | Details | To adjust the reading position at DADF reading (front side). When replacing the CCD unit (CCD PCB)/clearing RAM data, enter the value of service label.
Use case | When replacing the CCD unit (CCD PCB)/clearing RAM data
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | 1 to 200
Unit | 0.1 mm
Default value | 0
Related service mode | COPIER> FUNCTION> INSTALL> STRD-POS
ADJ-X-MG | Adj img ratio in book mod:vert scan[Frt]

Lv.1

Details

To make a fine adjustment of image magnification in vertical scanning direction at copyboard reading.
When replacing the CCD unit (CCD PCB)/clearing RAM data, enter the value of service label.
As the value is incremented by 1, the image magnification changes by 0.01%.
+: Enlarge
-: Reduce

Use case | When replacing the CCD unit (CCD PCB)/clearing RAM data
Adj/set/operate method | 1) Enter the setting value (switch negative/positive by -/+ key) and press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | -50 to 50
Unit | 0.01%
Default value | 0