﻿Removing the Fixing Film Unit

| Print out this category

Removing the Fixing Film Unit
1)Remove the Fixing Main Unit.(Reference)
2) Remove the support plate.
1 screw
CAUTION:
When installing the support plate, install it to engage the teeth with the locking lever at the position shown in the figure.
3)Remove the drawer connector and the earth wire, and then release the fixing harness from the cable guide.
3 screws
4)Remove the cable guide by pressing the embossment.
5)Remove the fixing film cover.
2 screws
6)Turn the pressure release arm to pressurize the fixing film.
7)Remove the 2 screws retaining the pressure plate units (front/rear).
CAUTION:
Never turn the screws pressurizing the fixing film unit. Turning the screws causes to change the pressure of the fixing film unit and results in the replacement of the fixing unit because the pressure adjustment cannot be performed in the field.
8)Release the pressure plate units (front/rear) to the arrow direction.
CAUTION:
Release the pressure plate units while pressing the upper part of them, because the units are pressurized.
9)Turn the pressure plate units and separate them from the fixing film.
10)Remove the terminal cover.
1 claw
11)Remove the 1 screw retaining the terminal.
12)Releasing the claw, take out the terminal plate to the arrow direction.
13)Press the both sides of the connector holder with the condition that the connector is attached, and then remove the connect holder.
14)Disconnect the connector from the drawer connector.
15)Take out the fixing film unit.