In case of Host Machine

| Print out this category

Installation Procedure
In case of Host Machine
1) Remove the Power Cord Clamp. (120V only)
1 Screw
1 Hook
2) Remove the Power Cord.
3) Remove the Connector Cover.
1 Screw
4) When the Cassette Pedestal is installed, remove the 3 connectors.
5) Remove the Lower Rear Cover.
4 Screws
3 Claws
6) Remove the ACC Sheet. (The removed ACC Sheet will not be used.)
7) Remove the cassette.
8) Remove the screw. (The removed screw will not be used.)
9) Install the wire saddle to Heater Connector Cover.
10) Put the connector of the heater through the Wire Saddle and install the Heater Connector Cover.
1 Screw (P tight; M3x8)
11) After putting the connector through the square hole and fitting the 3 claws on the Cassette Heater Unit into the holes on the Base Plate, and then move it toward the front.
CAIUTION:
Be sure that the claws are fit into the holes of the Base Plate properly.
12) Secure the Cassette Heater Unit using a stubby screwdriver.
1 Screw (W Sems Round End; M3x6)
NOTE:
Connect the connector of the Cassette Heater Unit when installing the Heater Kit. (Refer to Installation Procedure of Heater Kit-K1.)
13) Install the removed Cassettes.
14) Return the removed covers to their original positions.
NOTE:
When installing the Hear Kit at the same time, it is efficient to install covers when installing the Hear Kit.
Lower Rear Cover (4 Screws)
3 Connectors (When the Cassette Pedestal is installed.)
Connector Cover (1 Screw)
Power Cord
Power Cord Clamp (1 Screw)
15) Turn ON the Environment Heater Switch.