NETWORK

| Print out this category

NETWORK

COPIER>TEST>NETWORK
PING | Network connection check
Lv.1 | Details | To check connection between this machine and TCP/IP network.
Use case | - When checking network connection at the time of installation - At network connection failure

Adj/set/operate method

1) Turn OFF the main power switch.
2) Connect the network cable to this machine, and then turn ON the main power switch.
3) Inform the system administrator at user's site that installation of this machine is complete, and ask for network setting.
4) Ask the system administrator to check the network connection, and check the remote host address of PING transmission target.
5) Select the item and enter the remote host address, and then press OK key and Start key.
OK: Connection is normal. Checking procedure is complete.
NG: Connection failed. Go to step 6) if the cable connection is OK. In case of cable connection failure, connect again and then go to step 5).
6) Select the item and enter loopback address, and then press OK key and Start key.
OK: TCP/IP setting of this machine is normal. Go to step 7) to check NIC.
NG: TCP/IP setting of this machine has failure. Go to step 3) to check the setting again.
7) Select the item and enter the local host address, and then press OK key.
OK: Network setting of this machine and NIC are normal. Inform the system administrator that the trouble is due to network environment and ask for countermeasure.
NG: Connection failure/fault with NIC. Check connection of NIC/ replace NIC.

Display/adj/set range | 0.0.0.0 to 255.255.255.255 At normal state: OK At failure occurrence: NG
Supplement/memo | - Remote host address: IP address of PC terminal in network. - Loopback address: 127.0.0.1. Checking TCP/IP of this machine is available because the signal is returned before NIC. - NIC: Network interface board - Local host address: IP address of this machine
IPV6-ADR | Setting of PING send address (IPv6)
Lv.1 | Details | To set the IPv6 address to send PING. When PING is sent to this address by COPIER> TEST> NETWORK> PING-IP6, the network connection condition in the IPv6 environment can be checked.
Caution | - Enter a consistent character string as an address of IPv6. - Enter an address within 39 characters including hexadecimal numbers (0-9, a-f) and a separator (:).
Related service mode | COPIER> TEST> NETWORK> PING-IP6
PING-IP6 | PING transmission to IPv6 address
Lv.1 | Details | To send PING to the address specified by IPV6-ADR. The network connection condition in the IPv6 environment can be checked.
Adj/set/operate method | Select the item, and then press OK key.
Related service mode | COPIER> TEST> NETWORK> IPV6-ADR