Staple Finisher-G1/Booklet Finisher-G1 SORTER > P001 to P031

| Print out this category

Staple Finisher-G1/Booklet Finisher-G1 SORTER > P001 to P031

Address | bit | Name | Symbol | Remarks
PORT1 | 7 | Tray 2 Paper Surface Sensor 2 | PI120 | 0:Paper present
6 | Not used |  |
5 | For R&D use |  |
4 | For R&D use |  |
3 | Front Cover Open/Close Sensor | PI102 | 1:Open
2 | Saddle Unit Detection |  | 0: Present
1 | For R&D use |  |
0 | For R&D use |  |
PORT2 | 7 | For R&D use |  |
6 | For R&D use |  |
5 | For R&D use |  |
4 | For R&D use |  |
3 | Not used |  |
2 | For R&D use |  |
1 | Not used |  |
0 | For R&D use |  |
PORT3 | 7 | For R&D use |  |
6 | For R&D use |  |
5 | For R&D use |  |
4 | For R&D use |  |
3 | For R&D use |  |
2 | For R&D use |  |
1 | For R&D use |  |
0 | For R&D use |  |
PORT4 | 7 | For R&D use |  |
6 | For R&D use |  |
5 | For R&D use |  |
4 | For R&D use |  |
3 | For R&D use |  |
2 | For R&D use |  |
1 | For R&D use |  |
0 | Punch Paper Detection(Rear) |  | 1: Detection
PORT5 | 7 | Not used |  |
6 | Not used |  |
5 | Punch Unit Connect Signal |  | 0: Connect
4 | For R&D use |  |
3 | For R&D use |  |
2 | For R&D use |  |
1 | For R&D use |  |
0 | For R&D use |  |
PORT6 | 7 | Not used |  |
6 | Not used |  |
5 | For R&D use |  |
4 | For R&D use |  |
3 | For R&D use |  |
2 | For R&D use |  |
1 | For R&D use |  |
0 | For R&D use |  |
PORT7 | 7 | Not used |  |
6 | Not used |  |
5 | Not used |  |
4 | Not used |  |
3 | Tray 1 Shift Motor Lock Signal | M107 | 1: Lock
2 | Tray 1 switch | MSW103 | 1: ON
1 | For R&D use |  |
0 | Front Cover Open/Close Sensor | PI102 | 1:Open
PORT8 | 7 | Tray2 Shift Area Sensor 1 | PCB5 | 0: ON
6 | Tray2 Shift Area Sensor 2 | PCB5 | 0: ON
5 | Tray2 Shift Area Sensor 3 | PCB5 | 0: ON
4 | Inlet sensor | PI103 | 0:Paper present
3 | Swing Guide HP Sensor | PI105 | 1: HP
2 | For R&D use |  |
1 | Not used |  |
0 | Not used |  |
PORT9 | 7 | Tray 1 Paper Sensor | PI111 | 0:Paper present
6 | For R&D use |  |
5 | For R&D use |  |
4 | Tray1 Shift Area Sensor 1 | PCB4 | 0: ON
3 | Tray1 Shift Area Sensor 2 | PCB4 | 0: ON
2 | Tray1 Shift Area Sensor 3 | PCB4 | 0: ON
1 | Tray 2 Shift Motor Lock Signal | M108 | 1: Lock
0 | Tray 2 Paper Sensor | PI112 | 0:Paper present
PORT10 | 7 | For R&D use |  |
6 | For R&D use |  |
5 | For R&D use |  |
4 | For R&D use |  |
3 | For R&D use |  |
2 | For R&D use |  |
1 | For R&D use |  |
0 | For R&D use |  |
PORT11 | 7 | For R&D use |  |
6 | For R&D use |  |
5 | For R&D use |  |
4 | Not used |  |
3 | Not used |  |
2 | Not used |  |
1 | Not used |  |
0 | Not used |  |
PORT12 | 7 | Swing Height Sensor | PI123 | 1:Open
6 | Not used |  |
5 | Upper Cover Sensor | PI101 | 1:Open
4 | Rear End Assist HP Sensor | PI109 | 0: HP
3 | Processing Tray Sensor | PI108 | 0:Paper present
2 | Rear Aligning Plate HP Sensor | PI107 | 0: HP
1 | Front Aligning Plate HP Sensor | PI106 | 0: HP
0 | For R&D use |  |
PORT13 | 7 | Tray 2 Shift Motor ON | M108 | 1: ON
6 | Tray 2 Shift Motor Direction Change Signal | M108 | 0: CW 1: CCW
5 | Feed Roller Separation Solenoid | SL101 | 1: ON
4 | Punch Motor Standby |  | 0: Standby
3 | For R&D use |  |
2 | For R&D use |  |
1 | For R&D use |  |
0 | For R&D use |  |
PORT14 | 7 | For R&D use |  |
6 | Tray 1 Shift Motor Direction Change Signal | M107 | 0: CW 1: CCW
5 | Tray 1 Shift Motor ON | M107 | 1: ON
4 | For R&D use |  |
3 | For R&D use |  |
2 | For R&D use |  |
1 | Rear End Assist Motor Direction Change Signal | M109 | 0: CW 1: CCW
0 | Not used |  |
PORT15 | 7 | Staple Motor Direction Change Signal (CW) | M111 | 0: ON
6 | Staple Motor Direction Change Signal (CCW) | M111 | 0: ON
5 | For R&D use |  |
4 | For R&D use |  |
3 | For R&D use |  |
2 | Stack Ejection Motor Direction Change Signal | M102 | 0: CW 1: CCW
1 | For R&D use |  |
0 | Swing Motor Direction Change Signal | M106 | 0: CW 1: CCW
PORT16 | 7 | Not used |  |
6 | Eaer Aligning Plate Motor Direction Change Signal | M104 | 0: CW 1: CCW
5 | For R&D use |  |
4 | For R&D use |  |
3 | Not used |  |
2 | For R&D use |  |
1 | Front aligning plate motor Direction Change Signal | M103 | 0: CW 1: CCW
0 | For R&D use |  |
PORT17 | 7 | Tray 2 Paper Surface Sensor 1 | PI115 | 0:Paper present
6 | Tray 1 Paper Surface Sensor | PI114 | 0:Paper present
5 | Shutter HP Sensor | PI113 | 0: HP
4 | Stapler Shift HP Sensor | PI110 | 0: HP
3 | Stapler Alignment Interference Sensor | PI116 | 0:Interference
2 | Staple Existence |  | 0:Staple present
1 | Staple READY |  | 0: Standby
0 | Staple HP Detection |  | 1: HP
PORT18 | 7 | Stapler Shift Motor Direction Change Signal | M105 | 0: CCW 1: CW
6 | Buffer Roller Separation Solenoid | SL102 | 1: ON
5 | Shutter Clutch | CL101 | 1: ON
4 | Stack Ejection Lower Roller Clutch | CL102 | 1: ON
3 | Buffer Rear End Holding Solenoid | SL104 | 1: ON
2 | 1st Delivery Roller Separation Solenoid | SL103 | 1: ON
1 | For R&D use |  |
0 | For R&D use |  |
PORT19 | 7 | Not used |  |
6 | Feed Path Sensor | PI104 | 0:Paper present
5 | Swing Guide Lock Signal | MSW32 | 1: Lock
4 | Staple Lock Signal | MSW104 | 1: Lock
3 | Not used |  |
2 | Not used |  |
1 | Not used |  |
0 | For R&D use |  |
PORT20 | 7 | Alignment Plate HP Sensor | PI5 | 1: HP
6 | Not used |  |
5 | Not used |  |
4 | Not used |  |
3 | Saddle Stapl Unit Connect Detection |  | 0: Connect
2 | Vertical Path Paper Sensor | PI17 | 1:Paper present
1 | Not used |  |
0 | Not used |  |
PORT21 | 7 | Not used |  |
6 | For R&D use |  |
5 | For R&D use |  |
4 | For R&D use |  |
3 | Stitcher HP Sensor (Rear) | SW5 | 1: HP
2 | Stitcher HP Sensor (Front) | SW7 | 1: HP
1 | Paper Pushing Plate Top Position Sensor | PI15 | 0: ON
0 | Paper Pushing Plate HP Sensor | PI14 | 1: HP
PORT22 | 7 | For R&D use |  |
6 | For R&D use |  |
5 | For R&D use |  |
4 | For R&D use |  |
3 | Not used |  |
2 | For R&D use |  |
1 | For R&D use |  |
0 | Feed Motor Direction Change Signal | M1 | 0: CCW 1: CW
PORT23 | 7 | For R&D use |  |
6 | For R&D use |  |
5 | Not used |  |
4 | Not used |  |
3 | For R&D use |  |
2 | For R&D use |  |
1 | For R&D use |  |
0 | Not used |  |
PORT24 | 7 | Not used |  |
6 | Not used |  |
5 | No.2 Paper Deflecting Solenoid | SL2 | 1: ON
4 | No.1 Paper Deflecting Solenoid | SL1 | 1: ON
3 | Saddle Inlet Solenoid | SL5 | 1: ON
2 | Paper Folding HP Sensor | PI21 | 1: ON
1 | For R&D use |  |
0 | For R&D use |  |
PORT25 | 7 | Not used |  |
6 | For R&D use |  |
5 | Not used |  |
4 | For R&D use |  |
3 | For R&D use |  |
2 | For R&D use |  |
1 | For R&D use |  |
0 | For R&D use |  |
PORT26 | 7 | Not used |  |
6 | Not used |  |
5 | Not used |  |
4 | Not used |  |
3 | Stitcher Motor (Rear) Direction Change Signal (CW) | M6 | 0: ON
2 | Not used |  |
1 | Staple Sensor (Rear) | SW4 | 1:Staple present
0 | 24V Detection |  | 0: ON
PORT27 | 7 | Not used |  |
6 | Feed Plate Contact Solenoid | SL4 | 1: ON
5 | Paper Folding Motor RV | M2 | 1: ON
4 | For R&D use |  |
3 | For R&D use |  |
2 | Paper Positioning Plate Paper Sensor | PI8 | 0:Paper present
1 | Paper Positioning Plate HP Sensor | PI7 | 0: HP
0 | Tray Paper Sensor | PI6 | 0:Paper present
PORT28 | 7 | Paper Pushing Plate Motor EN | M8 | 0: ON
6 | Paper Pushing Plate Motor FWD | M8 | 1: ON
5 | Paper Pushing Plate Motor RV | M8 | 1: ON
4 | Paper Folding Motor FWD | M2 | 1: ON
3 | Not used |  |
2 | For R&D use |  |
1 | For R&D use |  |
0 | For R&D use |  |
PORT29 | 7 | Stitcher Motor (Rear) Direction Change Signal CCW | M6 | 0: ON
6 | For R&D use |  |
5 | For R&D use |  |
4 | Stitcher Motor (Front) Direction Change Signal CW | M7 | 0: ON
3 | Stitcher Motor (Front) Direction Change Signal CCW | M7 | 0: ON
2 | Staple Sensor (Front) | SW6 | 1:Staple present
1 | Not used |  |
0 | Not used |  |
PORT30 | 7 | For R&D use |  |
6 | For R&D use |  |
5 | For R&D use |  |
4 | For R&D use |  |
3 | For R&D use |  |
2 | For R&D use |  |
1 | For R&D use |  |
0 | For R&D use |  |
PORT31 | 7 | Saddle Inlet Sensor | PI22 | 1:Paper present
6 | Guide HP Sensor | PI13 | 1: HP
5 | Crescent Roller Phase Sensor | PI12 | 1: HP
4 | Delivery Sensor | PI11 | 0:Paper present
3 | Lower Right Cover Sensor | PI9 | 1:Open
2 | No.3 Paper Sensor | PI20 | 1:Paper present
1 | No.2 Paper Sensor | PI19 | 1:Paper present
0 | No.1 Paper Sensor | PI18 | 1:Paper present