﻿Network Settings

| Print out this category

Network Settings
1. Connecting to External Network
The method of connecting to external network is similar to a normal network connection method. Refer to user manual of the device for details.
NOTE:
See User Manual for how to connect the device to the external network.
Before using UGW link or User mode, see the sections below to prepare as required.
"Enabling UGW Link"
"Enabling [Update Firmware] Button of User Mode"
"Enabling [Install Application/Options] Button of User Mode"
NOTE:
“External Network” here means the network connecting the device to CDS via Internet.
2. Confirming URL Setting of Distribution Server
This section describes how to confirm the URL setting of the distribution server.
1. Start [Service Mode] at Level 1.
1). Press [Setting/Registration (User Mode)] button on the control panel.
2). Press [2] and [8] buttons at a time on the control panel.
3). Press [Setting/Registration (User Mode)] button on the control panel.
4). [Service Mode] screen is shown.
NOTE:
CDS and RDS are another servers.You need the communication test of CDS by all means even if You succeed in a communication test of the RDS.
2. Press [Updater] button.
3. Press [Software Management Settings] button.
4. Press [Settings] button.
5. Ensure to enter “https://device.c-cdsknn.net/cds_soap/updaterif” in the field beside the [Delivery Server URL] button.
If the URL is not entered or a wrong URL is entered in the field, click [Delivery Server URL] button to show the virtual keypad. Check the URL and enter the correct one.
6. Press [OK] to set the entered items. Now the URL of the distribution server is successfully set.
3. Communication Test
This section describes how to check if the communication is normally done to the distribution server and/or the file server.
1. Start [Service Mode] at Level 1.
1). Press [Setting/Registration (User Mode)] button on the control panel.
2). Press [2] and [8] buttons at a time on the control panel.
3). Press [Setting/Registration (User Mode)] button on the control panel.
4). [Service Mode] screen is shown.
NOTE:
CDS and RDS are another servers.
You need the communication test of CDS by all means even if You succeed in a communication test of the RDS.
2. Press [Updater] button.
3. Press [Software Management Settings] button.
4. Press [Test Communication] button.
5. Press [Yes] button.
Obtain the download file information for communication test from the distribution server
(to execute the communication test to the distribution server).
Using the download file information for communication test, the contents for test are downloaded from the file server (for the communication test to the file server).
6. Upon the communication test completed, the communication test result screen is shown.
Press [OK] button to exit this operation.