ACC

| Print out this category

ACC

COPIER>OPTION>ACC
COIN | Setting of charge management
Lv.1 | Details | To set charging management method.
Use case | At installation of Coin Manager
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.

Caution

Following items are automatically specified when changing the value to 3 (from 0 to 2). The change will not be returned even if changing back the value to 0 to 2 (from 3) once the mode has been changed.
- COPIER> OPTION> USER> CONTROL=1
- COPIER> OPTION> NETWORK> DA-CNCT=1
- COPIER> OPTION> DSPLY-SW> UI-BOX, UI-SEND, UI-FAX=0
- Function Settings > Send > E-Mail/I-Fax Settings > Communication Settings > SMTP Receive, POP=OFF
- Preferences> Network > TCP/IP Settings > DNS Settings > FTP Print Settings > Use FTP Printing=OFF
- Preferences> Network > TCP/IP Settings > DNS Settings > IPP Print Settings > Use IPP Printing=ON

Display/adj/set range

0 to 7
0: No charge
1: Charge with Coin Manager
2: Charge with remote counter
3: Charge with DA (only in Japan)
4: Charge with this machine itself
5: Not used
6: External charge mode 6
7: External charge mode 7

Default value | 0
Related service mode | COPIER> OPTION> USER> CONTROL COPIER> OPTION> FNC-SW> DA-CNCT COPIER> OPTION> DSPLY-SW> UI-BOX, UI-SEND, UI-FAX COPIER> OPTION> ACC> PDL-THR
Related user mode | Function Settings > Send > E-Mail/I-Fax Settings > Communication Settings Preferences> Network > TCP/IP Settings > DNS Settings > FTP Print Settings Preferences> Network > TCP/IP Settings > DNS Settings > IPP Print Settings
Supplement/memo | Control card can be used with ""0: No charge"". DA: Digital Accessory
DK-P | Setting of Paper Deck paper size
Lv.1 | Details | To set the paper size used in the Paper Deck.
Display/adj/set range | 0 to 2 0: A4, 1: B5, 2: LTR
Default value | 0
CC-SPSW | Support setting of control card I/F
Lv.2 | Details | To set support level for control card (CCIV/CCV) interface.
Use case | Upon user's request (when connecting to the external counter management system using the control card interface)
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: No support, 1: Support
Default value | 0
UNIT-PRC | Setting of Coin Manager currency unit
Lv.2 | Details | To set currency unit to be handled with Coin Manager
Use case | At installation of Coin Manager
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 6 0: Japanese yen, 1: Euro, 2: Pound, 3: Swiss Franc, 4: Dollar, 5: No currency unit (no fractional unit), 6: No currency unit (with fractional unit)
Default value | 0
IN-TRAY | Presence/absence of inner 2 way tray
Lv.1 | Details | Set the presence/absence of the inner 2 way tray.
Use case | When the inner 2 way tray is installed
Display/adj/set range | 0: The inner 2 way tray is absent 1: The inner 2 way tray is present.
Default value | 0
MIN-PRC | Set of Coin Manager minimum price
Lv.1 | Details | To set the minimum amount to be handled with Coin Manager. Enter 10 when specifying 10 Japanese yen as the minimum amount to be handled with the Coin Manager that supports Japanese yen. In the case to specify 1 to 4 (Euro/Pound/Swiss Franc/Dollar) by going through the following: COPIER> OPTION> ACC > UNIT-PRC, entry is in fractional unit. Entry of 50 indicates 50 cents ($ 0.50).
Use case | At installation of Coin Manager
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | This mode is enabled when selecting 4 for the following: COPIER > OPTION > ACC > COIN.
Display/adj/set range | 0 to 9999
Default value | 10
Related service mode | COPIER> OPTION> ACC> COIN, UNIT-PRC
Supplement/memo | As for the charging amount, it causes an error if specifying the value that is smaller than the minimum currency unit with Settings/Registration mode.
MAX-PRC | Set of Coin Manager maximum price
Lv.1 | Details | To set the maximum amount to be handled with Coin Manager. Enter 8800 when specifying 8800 Japanese yen as the maximum amount to be handled with the Coin Manager that supports Japanese yen. In the case to specify 1 to 4 (Euro/Pound/Swiss Franc/Dollar) by going through the following: COPIER> OPTION> ACC > UNIT-PRC, entry is in fractional unit. Entry of 50 indicates 50 cents ($ 0.50).
Use case | At installation of Coin Manager
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | This mode is enabled when selecting 4 for the following: COPIER > OPTION > ACC > COIN.
Display/adj/set range | 0 to 9999
Default value | 8800
Related service mode | COPIER> OPTION> ACC> COIN, UNIT-PRC
Supplement/memo | As for charging amount, it causes an error if specifying the value that is larger than the maximum currency unit with Settings/Registration mode.
MIC-TUN | Manual adj of voice recognize microphone
Lv.1 | Details | To manually adjust the voice receiving level (sensitivity) of the connected voice recognition microphone. Microphone sensitivity is automatically tuned in user mode; however, adjust it manually as needed.
Use case | When the sensitivity of microphone is not improved by auto tuning
Display/adj/set range | 0 to 255
Default value | 128
Related user mode | Preferences > Accessibility > Voice Navigation Settings > Tune Microphone
Supplement/memo |
PDL-THR | Norm PDL pnt set:External charge mode6/7
Lv.2 | Details | To set normal PDL print job processing at external charge mode 6/7. When 1 is set and external charge mode 6/7 is set with COIN, normal PDL print job is executed without being cancelled.
Use case | When setting the normal PDL print processing in external charge mode 6/7
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: Cancel, 1: Execute
Default value | 0
Related service mode | COPIER> OPTION> ACC> COIN
CR-TYPE | Setting of Card Reader
Lv.1 | Details | To set the model of the Card Reader. Set 1 in the case of connecting the Card Reader-C1. It operates even 0 is set, but recognition rate decreases.
Use case | When connecting the Card Reader-C1
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: Card Reader-F1, 1: Card Reader-C1
Default value | 0