In case of Cassette Feeding Unit

| Print out this category

In case of Cassette Feeding Unit
1) Remove the cassette.
2) Remove the Heater Connector Cover using a flat-blade screwdriver.
1 Claw
2 Protrusions
NOTE:
When performing this procedure, it is not necessary to remove the Host Machine. However, the figure shows the picture without the Host Machine to show easily.
3) Fit the 3 claws on the Cassette Heater Unit into the holes on the Base Plate, and then move it toward the front.
CAIUTION:
Be sure that the claws are fit into the holes of the Base Plate properly.
4) Tighten the removed screw (W Sems Round End;M3x6) with the stubby driver to connect the connector.
5) Install the heater Connector Cover.
6) Install the removed Cassettes.
7) Turn ON the Environment Heater Switch.
8) Connect the power plug of the host machine to the power outlet.
9) Turn ON the main power switch.