Installation Procedure

| Print out this category

Installation Procedure
1) Remove the Rear Cover.
4 Screws
4 Claws
2) Remove the Controller Box Cover.
6 Hooks
3) Install the Expansion RAM.
4) Install the removed cover.
Controller Box Cover
Rear Cover (4 Screws) (Tighten the screws in the following order: upper left, lower left, upper right, and then lower right.)
5) Connect the power plug of the host machine to the power outlet.
6) Turn ON the main power switch.