Boot sequence

| Print out this category

Boot/Shutdown sequence
Boot sequence
NOTE:
Due to the high speed startup, the progress bar and the activating PCB are not synchronized.
For this reason, the progress bar cannot be utilized for troubleshooting.
See the following error code list for the troubleshooting.
Related error codes (major error codes):

Error code | Detail Code | Description | Remedy
E602 | Hard disk error
| 0001 | HDD detection error. Unable to detect HDD, not become Ready, return an error. | 1. Connection of the HDD cable. 2. Reinstall the system. 3. HDD. 4. Main Controller PCB.
0002 | There is no startup file. There is no program for main CPU in /BOOTDEV/BOOT/ on HDD. | 1. Reinstall the system. 2. HDD.
0006 | There is no SubBootable for the PDL type in /BOOTDEV/BOOT. | 1. Reinstall the system. 2. HDD.
4000 | Unable to install OS. | 1. Cable connection error. 2. After HDD All Format, reinstall the system software. 3. HDD.
4001 | No OS startup script. | 1. Cable connection error. 2. After HDD All Format, reinstall the system software. 3. HDD.
E604 | Insufficient memory
| 0000 | Insufficient memory (require 1024 MB). | DDR2-SDRAM

NOTE:
When the following errors occur, the system of the host machine has not been started normally. Therefore the error code is not recorded in the log.
E602-0001, 0002, 0006, 4000, 4001