Error at starting up the MEAP application/Setting to hide JAM screen (level 2)

| Print out this category

Error at starting up the MEAP application/Setting to hide JAM screen (level 2)
In the case that operation is restricted by MEAP application, hide the warning screen of error/ JAM (such as JAM screen, door opening, no-toner). In the case that these errors occur, there will be a display indicating 'call the service personnel' etc.
Note:
Part of the warning screens is displayed if shifting to the device screen.
As for the screens for jam and no-toner, the warning screen (animation) can be displayed by pressing the followings: [Device Screen] > [Recovery Procedure]
As for the screen for door opening, the warning screen cannot be displayed because there is no display for [[Device Screen] > [Recovery Procedure]
Default value
1: No activation of warning display
Setting range, item
0: display warning screen 1: hide warning screen
Setting Procedure
1) Start [ SERVICE MODE ] in Level 2.
2) Press [ COPIER ] > [ Option ] > [ DSPLY-SW ].
3) Press [ ANIM-SW ].
4) Press either 0 (display warning screen) or 1 (hide warning screen) on control panel (the numerical value input in the field is displayed), and press [ OK ] button.
5) Check to see that it is reflected in setting field, and restart the device.