HV-TR

| Print out this category

HV-TR

COPIER>ADJUST>HV-TR
TR-OFST | Adj transfer target current offset
Lv.1 | Details | Single print and the 2-sided print (first sided) with the thick paper
Use case | When replacing the DC Controller PCB/clearing RAM data
Adj/set/operate method | 1) Enter the setting value (switch negative/positive by -/+ key) and press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | -128 to 127
Title | Output adj of the transfer bias for Hvy
Use case | When clearing RAM of the DC Controller PCB or replacing the PCB
Adj/set/operate method | 1) Enter the setting value (switch negative/positive by -/+ key) and press OK key. 2) Turn OFF/ON the main power switch.
Caution | Enter the value of the service label. As the value is increased, the effect becomes larger.
Display/adj/set range | -128 to 127