﻿Image Transfer Wrong/Text Void

| Print out this category

Image Transfer Wrong/Text Void
[Occurrence area]
Transfer roller (circumference: 50mm)
[Cause]
Resistance of paper increases due to reduction in paper water content, resulting in insufficient transfer output.
Resistance of paper decreases due to increase in paper water content, resulting in excessive transfer output.
[Occurrence condition]
Paper left alone in a low-humidity environment
Paper left alone in a high-humidity environment
[Remedy]
Service mode (Lv.2)> COPIER> OPTION> IMG-TR> TROPT-SW> -2 to 1
-2: Transfer output voltage moreover decreases.
-1: Transfer output voltage decreases.
0: OFF
1: Transfer output voltage increases.