﻿Removing the Fixing Main Unit

| Print out this category

Removing the Fixing Main Unit
CAUTION:
There are two kinds of film units for the fixing unit. One is for the 51 ppm machine and another one is for the 45/35/25 ppm machine. Attach the right fixing main unit.
1)Remove the fixing unit. (Reference)
2)Open the fixing outer delivery unit and remove the fixing outer delivery unit.
1 screw
2 claws
3)Remove the positioning guide.
1 screw
4)Remove the fixing inner delivery unit.
1 screw