HV-STS

| Print out this category

HV-STS

COPIER>DISPLAY>HV-STS
PRIMARY | Display of primary charging current
Lv.1 | Details | To display the current that is applied to the Primacy Charging Assembly at the latest.
Use case | When checking ON/OFF of potential control
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 0 to 1600
Unit | micro A
TR | Display of transfer current: Plain, 1st side
Lv.1 | Details | To display the current that is applied to plain paper (1st side) in the Pre-transfer Charging Assembly at the latest.
Use case | For checking
Adj/set/operate method | N/A (Display only)
Unit | micro A
BIAS | Display of developing DC bias setting value
Lv.1 | Details | To display the setting value of developing DC bias.
Use case | For checking
Adj/set/operate method | N/A (Display only)
Unit | V