Points to Note at Installation

| Print out this category

﻿﻿Printer Model (for Europe)
Points to Note at Installation
If the machine is used as a copier model, "Image Reader Unit-E1" is required. Follow the Installation Procedure included in the package of the Image Reader Unit to install it, and then install from the "Installing the Toner Bottle".
If the machine is used as a printer model, "Printer Cover-E1" is required. Follow the this installation procedure to install the Printer Cover, and then install from the "Installing the Toner Bottle".

Items of Installation Procedure | Reference
Making Pre-Checks | Procedure reference of the Copier model
Points to Make Before Installation
Table of Options Combination
Checking the Contents | Reference of this procedure
Unpacking and Installation Procedure | Unpacking the Machine and Removing the Packaging Materials
Insatallation of "Printer Cover-E1" or "Image Reader Unit-E1"
Installing the Toner Bottle | Procedure reference of the Copier model
Installing the Drum Unit
Installing the Filter
Connecting the cord
Setting the Environment Heater Switch
Turning ON the Main Power | Reference of this procedure
Stirring Toner | Procedure reference of the Copier model
Installing Trays
Setting the Cassettes
Installing the Other Parts
Securing the Host Machine
Auto Adjust Gradation
Checking the Print Image
Image Position Adjustment
Checking the Network Connection
Network Troubleshooting
Checking the Network Setting of the Host Machine
Checking Network Function on the Main Controller
Turning OFF the Main Power