IMG-SPD

| Print out this category

IMG-SPD

COPIER>OPTION>IMG-SPD
CPMKP-SW | ON/OFF of sequence to decrease the copy speed
Lv.2 | Details | Decrease the copy speed to maintain fixing performance.
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 : OFF 1 : ON
Default value | 0
PSP-PR1 | Set productivity priority mode
Lv.2 | Details | To lower the fixing temperature for the paper feed start at the paper size change. The priority is given to the productivity so that the fixing offset may occur.
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0: OFF 1: ON (Productivity priority mode)
Default value | 0
PSP-PR2 | Productivity priority mode: post card
Lv.2 | Details | To improve the productivity and to reduce the fixing grade
Use case | To improve the productivity and to reduce the fixing grade in printing the post card
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0: OFF 1: ON (Productivity priority)
Default value | 0
PSP-PR3 | Productivity priority mode: Thick
Lv.2 | Details | To improve the productivity and to reduce the fixing grade
Use case | To improve the productivity and to reduce the fixing grade in printing the thick paper
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0: OFF (Productivity priority) 1: ON (Fixing grade priority) 2: Auto (Fixing grade priority only in the low humidity environment)
Default value | 2
PSP-PR4 | Set prdctvty priority in rotation collation mode
Lv.2 | Details | To set the productivity priority in the rotation collation mode by lowering the fixing temperature for the paper feed start
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0: OFF 1: Productivity priority 1 (fixing temp: -40 degC) 2: Productivity priority 2 (fixing temp: -60 degC) 3: Fixing grade priority (fixing temp: -20 degC)
Default value | 0