Host machine + Cassette Feeding Unit-AF1

| Print out this category

Host machine + Cassette Feeding Unit-AF1

ACC ID | Jam Code | Type | Sensor ID | Sensor Name/Description
00 | 0101 | DELAY | S1 | Cassette 1 pickup sensor
00 | 0102 | DELAY | S33 | Cassette 2 pickup sensor
00 | 0103 | DELAY | PS108 | Cassette 3 pickup sensor
00 | 0104 | DELAY | PS109 | Cassette 4 pickup sensor
00 | 0105 | DELAY | S5 | Pre-registration sensor
00 | 0107 | DELAY | S19 | Fixing outlet sensor
00 | 0108 | DELAY | S21 | No.1 delivery sensor
00 | 0109 | DELAY | S22 | No.2 delivery sensor
00 | 010A | DELAY | S24 | Reversal sensor
00 | 010D | DELAY | S7 | Duplex feed sensor
00 | 0201 | STNRY | S1 | Cassette 1 pickup sensor
00 | 0202 | STNRY | S33 | Cassette 2 pickup sensor
00 | 0203 | STNRY | PS108 | Cassette 3 pickup sensor
00 | 0204 | STNRY | PS109 | Cassette 4 pickup sensor
00 | 0205 | STNRY | S5 | Pre-registration sensor
00 | 0207 | STNRY | S19 | Fixing outlet sensor
00 | 0208 | STNRY | S21 | No.1 delivery sensor
00 | 0209 | STNRY | S22 | No.2 delivery sensor
00 | 020A | STNRY | S24 | Reversal sensor
00 | 020D | STNRY | S7 | Duplex feed sensor
00 | 0A01 | POWER ON | S1 | Cassette 1 pickup sensor
00 | 0A02 | POWER ON | S33 | Cassette 2 pickup sensor
00 | 0A03 | POWER ON | PS108 | Cassette 3 pickup sensor
00 | 0A04 | POWER ON | PS109 | Cassette 4 pickup sensor
00 | 0A05 | POWER ON | S5 | Pre-registration sensor
00 | 0A07 | POWER ON | S19 | Fixing outlet sensor
00 | 0A08 | POWER ON | S21 | No.1 delivery sensor
00 | 0A09 | POWER ON | S22 | No.2 delivery sensor
00 | 0A0A | POWER ON | S24 | Reversal sensor
00 | 0A0D | POWER ON | S7 | Duplex feed sensor
00 | 0B00 | DOOR OP | - | Door open jam
00 | FF01 | SEQ NG*1 | S1 | Cassette 1 pickup sensor
00 | FF02 | SEQ NG*1 | S33 | Cassette 2 pickup sensor
00 | FF03 | SEQ NG*1 | PS108 | Cassette 3 pickup sensor
00 | FF04 | SEQ NG*1 | PS109 | Cassette 4 pickup sensor
00 | FF05 | SEQ NG*1 | S5 | Pre-registration sensor
00 | FF06 | SEQ NG*1 | S19 | Fixing outlet sensor
00 | FF07 | SEQ NG*1 | S21 | No.1 delivery sensor
00 | FF08 | SEQ NG*1 | S22 | No.2 delivery sensor
00 | FF09 | SEQ NG*1 | S24 | Reversal sensor
00 | FF0A | SEQ NG*1 | S24 | Reversal sensor
00 | FF0D | SEQ NG*1 | S7 | Duplex feed sensor

*1: The state is recovered by opening and closing the Door, or turning OFF and then ON the power supply.
If it is not recovered by the above operation, it is considered an error near the target sensor.
Disconnect and then connect the connectors around the target sensor, check if the cable is open circuit, and replace the sensor.