LCNS-TR

| Print out this category

LCNS-TR

COPIER>OPTION>LCNS-TR
ST-SEND | Installation state dis of SEND function
Lv.2 | Details | To display installation state of SEND function when transfer is disabled.
Use case | When checking whether SEND function is installed
Adj/set/operate method | 1) Select ST-SEND. 2) Enter 0, and then press OK key. When installation has been completed, the transfer license key is displayed under TR-SEND.
Display/adj/set range | When operation finished normally: OK!
Default value | 0
TR-SEND | transfer license key dis of SEND function
Lv.2 | Details | To display transfer license key to use SEND function when transfer is disabled.
Use case | - When replacing HDD - When replacing the device
Adj/set/operate method | 1) Select ST-SEND. 2) Enter 0, and then press OK key. The transfer license key is displayed under TR-SEND.
Display/adj/set range | 24 digits
ST-ENPDF | Installation state dis of Encryption PDF
Lv.2 | Details | To display installation state of Encryption PDF when transfer is disabled.
Use case | When checking whether Encryption PDF is installed
Adj/set/operate method | 1) Select ST-ENPDF. 2) Enter 0, and then press OK key. When installation has been completed, the transfer license key is displayed under TR-ENPDF.
Caution |
Display/adj/set range | When operation finished normally: OK!
Default value | 0
TR-ENPDF | transfer license key dis of Encryption PDF
Lv.2 | Details | To display transfer license key to use Encryption PDF when transfer is disabled.
Use case | - When replacing HDD - When replacing the device
Adj/set/operate method | 1) Select ST-ENPDF. 2) Enter 0, and then press OK key. The transfer license key is displayed under TR-ENPDF.
Caution | This mode is enabled when SEND function is installed.
Display/adj/set range | 24 digits
ST-SPDF | Installation state dis of Searchable PDF
Lv.2 | Details | To display installation state of Searchable PDF when transfer is disabled.
Use case | When checking whether Searchable PDF is installed
Adj/set/operate method | 1) Select ST-SPDF. 2) Enter 0, and then press OK key. When installation has been completed, the transfer license key is displayed under TR-SPDF.
Display/adj/set range | When operation finished normally: OK!
Default value | 0
TR-SPDF | Transfer license key dis of Searchable PDF
Lv.2 | Details | To display transfer license key to use Searchable PDF when transfer is disabled.
Use case | - When replacing HDD - When replacing the device
Adj/set/operate method | 1) Select ST-SPDF. 2) Enter 0, and then press OK key. The transfer license key is displayed under TR-SPDF.
Caution | This mode is enabled when SEND function is installed.
Display/adj/set range | 24 digits
ST-EXPDF | Instal state of Encryption PDF + Searchbl PDF
Lv.2 | Details | To display installation state of Encryption PDF + Searchable PDF when transfer is disabled.
Use case | When checking whether Encryption PDF + Searchable PDF is installed
Adj/set/operate method | 1) Select ST-EXPDF. 2) Enter 0, and then press OK key. When installation has been completed, the transfer license key is displayed under TR-EXPDF.
Display/adj/set range | When operation finished normally: OK!
Default value | 0
TR-EXPDF | Transfer license key of Encryption PDF+Searchbl PDF
Lv.2 | Details | To display transfer license key to use Encryption PDF + Searchable PDF when transfer is disabled.
Use case | - When replacing HDD - When replacing the device
Adj/set/operate method | 1) Select ST-EXPDF. 2) Enter 0, and then press OK key. The transfer license key is displayed under TR-EXPDF.
Caution | This mode is enabled when SEND function is installed for Japan.
Display/adj/set range | 24 digits
ST-PDFDR | Install state display of Direct Print PDF
Lv.2 | Details | To display installation state of Direct Print PDF when transfer is disabled.
Use case | When checking whether Direct Print PDF is installed
Adj/set/operate method | 1) Select ST-PDFDR. 2) Enter 0, and then press OK key. When installation has been completed, the transfer license key is displayed under TR-PDFDR.
Display/adj/set range | When operation finished normally: OK!
Default value | 0
TR-PDFDR | Transfer licensekey display of Direct Print PDF
Lv.2 | Details | To display transfer license key to use Direct Print PDF when transfer is disabled.
Use case | - When replacing HDD - When replacing the device
Adj/set/operate method | 1) Select ST-PDFDR. 2) Enter 0, and then press OK key. The transfer license key is displayed under TR-PDFDR.
Display/adj/set range | 24 digits
ST-SCR | Install state display of Encrypted Secure Print
Lv.2 | Details | To display installation state of Encrypted Secure Print when transfer is disabled.
Use case | When checking whether Encrypted Secure Print is installed
Adj/set/operate method | 1) Select ST-SCR. 2) Enter 0, and then press OK key. When installation has been completed, the transfer license key is displayed under TR-SCR.
Display/adj/set range | When operation finished normally: OK!
Default value | 0
TR-SCR | Transfer license key display of Encrypted Secure Print
Lv.2 | Details | To display transfer license key to use Encrypted Secure Print when transfer is disabled.
Use case | - When replacing HDD - When replacing the device
Adj/set/operate method | 1) Select ST-SCR. 2) Enter 0, and then press OK key. The transfer license key is displayed under TR-SCR.
Caution | This mode is enabled when there is "3DES+USH-H" Board.
Display/adj/set range | 24 digits
ST-BRDIM | Installation status of the BarDIMM upon the transfer invalidation
Lv.2 | Details | Display the installation status of the BarDIMM.
Adj/set/operate method | 1) Select ST-BRDIM. 2) Enter 0, and then press OK key. When installation has been completed, the transfer license key is displayed under TR-BRDIM.
Display/adj/set range | When operation finished normally: OK!
Default value | 0
TR-BRDIM | Transfer license key of the BarDIMM upon the transfer invalidation
Lv.2 | Details | This item is used when replacing the HDD, or when changing the machine. Display the transfer license key of the BarDIMM.
Use case | - When replacing HDD - When replacing the device
Adj/set/operate method | 1) Select ST-BRDIM. 2) Enter 0, and then press OK key. The transfer license key is displayed under TR-BRDIM.
Display/adj/set range | 24 digits
ST-VNC | Install state display of Remote Operators Software
Lv.2 | Details | To display installation state of Remote Operators Software when transfer is disabled.
Use case | When checking whether Remote Operators Software is installed
Adj/set/operate method | 1) Select ST-VNC. 2) Enter 0, and then press OK key. When installation has been completed, the transfer license key is displayed under TR-VNC.
Display/adj/set range | When operation finished normally: OK!
Default value | 0
TR-VNC | Transfer license key display of Remote Operators Soft
Lv.2 | Details | To display transfer license key to use Remote Operators Software when transfer is disabled.
Use case | - When replacing HDD - When replacing the device
Adj/set/operate method | 1) Select ST-VNC. 2) Enter 0, and then press OK key. The transfer license key is displayed under TR-VNC.
Display/adj/set range | 24 digits
ST-WEB | Install state display of Web Access Software
Lv.2 | Details | To display installation state of Web Access Software when transfer is disabled.
Use case | When checking whether Web Access Software is installed
Adj/set/operate method | 1) Select ST-WEB. 2) Enter 0, and then press OK key. When installation has been completed, the transfer license key is displayed under TR-WEB.
Display/adj/set range | When operation finished normally: OK!
Default value | 0
TR-WEB | Transfer license key display of Web Access Soft
Lv.2 | Details | To display transfer license key to use Web Access Software when transfer is disabled.
Use case | "- When replacing HDD - When replacing the device"
Adj/set/operate method | 1) Select ST-WEB. 2) Enter 0, and then press OK key. The transfer license key is displayed under TR-WEB.
Display/adj/set range | 24 digits
ST-HRPDF | Install state display of High Compress PDF
Lv.2 | Details | To display installation state of High Compression PDF when transfer is disabled.
Use case | When checking whether High Compression PDF is installed
Adj/set/operate method | 1) Select ST-HRPDF. 2) Enter 0, and then press OK key. When installation has been completed, the transfer license key is displayed under TR-HRPDF.
Display/adj/set range | When operation finished normally: OK!
Default value | 0
TR-HRPDF | Transfer licens key display of High Compress PDF
Lv.2 | Details | To display transfer license key to use High Compression PDF when transfer is disabled.
Use case | - When replacing HDD - When replacing the device
Adj/set/operate method | 1) Select ST-HRPDF. 2) Enter 0, and then press OK key. The transfer license key is displayed under TR-HRPDF.
Display/adj/set range | 24 digits
ST-TRSND | Install state display of Trial SEND function
Lv.2 | Details | To display installation state of Trial SEND function when transfer is disabled.
Use case | When checking whether Trial SEND function is installed
Adj/set/operate method | 1) Select ST-TRSND. 2) Enter 0, and then press OK key. When installation has been completed, the transfer license key is displayed under TR-TRSND.
Display/adj/set range | When operation finished normally: OK!
Default value | 0
TR-TRSND | Transfer licensekey display of Trial SEND function
Lv.2 | Details | To display transfer license key to use Trial SEND function when transfer is disabled.
Use case | "- When replacing HDD - When replacing the device"
Adj/set/operate method | 1) Select ST-TRSND. 2) Enter 0, and then press OK key. The transfer license key is displayed under TR-TRSND.
Display/adj/set range | 24 digits
ST-WTMRK | Install state display of Secure Watermark
Lv.2 | Details | To display installation state of Secure Watermark when transfer is disabled.
Use case | When checking whether Secure Watermark is installed
Adj/set/operate method | 1) Select ST-WTMRK. 2) Enter 0, and then press OK key. When installation has been completed, the transfer license key is displayed under TR-WTMRK.
Display/adj/set range | When operation finished normally: OK!
Default value | 0
TR-WTMRK | Trns license key dis of Secure Watermark
Lv.2 | Details | To display transfer license key to use Secure Watermark when transfer is disabled.
Use case | - When replacing HDD - When replacing the device
Adj/set/operate method | 1) Select ST-WTMRK. 2) Enter 0, and then press OK key. The transfer license key is displayed under TR-WTMRK.
Display/adj/set range | 24 digits
ST-TSPDF | Install state display of Time Stamp PDF: JP
Lv.2 | Details | To display installation state of Time Stamp PDF (JP only) when transfer is disabled.
Use case | When checking whether Time Stamp PDF (JP only) is installed
Adj/set/operate method | 1) Select ST-TSPDF. 2) Enter 0, and then press OK key. When installation has been completed, the transfer license key is displayed under TR-TSPDF.
Display/adj/set range | When operation finished normally: OK!
Default value | 0
TR-TSPDF | Transfer license key display of Time Stamp PDF: JP
Lv.2 | Details | To display transfer license key to use Time Stamp PDF (JP only) when transfer is disabled.
Use case | - When replacing HDD - When replacing the device
Adj/set/operate method | 1) Select ST-TSPDF. 2) Enter 0, and then press OK key. The transfer license key is displayed under TR-TSPDF.
Caution | This mode is enabled when SEND function is installed.
Display/adj/set range | 24 digits
ST-USPDF | Install state display of Digital User Sign PDF
Lv.2 | Details | To display installation state of Digital User Signature PDF when transfer is disabled.
Use case | When checking whether Digital User Signature PDF is installed
Adj/set/operate method | 1) Select ST-USPDF. 2) Enter 0, and then press OK key. When installation has been completed, the transfer license key is displayed under TR-USPDF.
Display/adj/set range | When operation finished normally: OK!
Default value | 0
TR-USPDF | Transfer license key display of Digital User Sign PDF
Lv.2 | Details | To display transfer license key to use Digital User Signature PDF when transfer is disabled.
Use case | - When replacing HDD - When replacing the device
Adj/set/operate method | 1) Select ST-USPDF. 2) Enter 0, and then press OK key. The transfer license key is displayed under TR-USPDF.
Caution | This mode is enabled when SEND function is installed.
Display/adj/set range | 24 digits
ST-DVPDF | Install state display of Device Sign PDF
Lv.2 | Details | To display installation state of Device Signature PDF when transfer is disabled.
Use case | When checking whether Device Signature PDF is installed
Adj/set/operate method | 1) Select ST-DVPDF. 2) Enter 0, and then press OK key. When installation has been completed, the transfer license key is displayed under TR-DVPDF.
Display/adj/set range | When operation finished normally: OK!
Default value | 0
TR-DVPDF | Transfer license key display of Device Sign PDF
Lv.2 | Details | To display transfer license key to use Device Signature PDF when transfer is disabled.
Use case | - When replacing HDD - When replacing the device
Adj/set/operate method | 1) Select ST-DVPDF. 2) Enter 0, and then press OK key. The transfer license key is displayed under TR-DVPDF.
Caution | This mode is enabled when SEND function is installed.
Display/adj/set range | 24 digits
ST-SCPDF | Install state display of Trace & Smooth PDF
Lv.2 | Details | To display installation state of Trace & Smooth PDF when transfer is disabled.
Use case | When checking whether Trace & Smooth PDF is installed
Adj/set/operate method | 1) Select ST-SCPDF. 2) Enter 0, and then press OK key. When installation has been completed, the transfer license key is displayed under TR-SCPDF.
Display/adj/set range | When operation finished normally: OK!
Default value | 0
TR-SCPDF | Transfer licensekey display of Trace & Smooth PDF
Lv.2 | Details | To display transfer license key to use Trace & Smooth PDF when transfer is disabled.
Use case | - When replacing HDD - When replacing the device
Adj/set/operate method | 1) Select ST-SCPDF. 2) Enter 0, and then press OK key. The transfer license key is displayed under TR-SCPDF.
Caution | This mode is enabled when SEND function is installed.
Display/adj/set range | 24 digits
ST-AMS | Install state display of Access Management System
Lv.2 | Details | To display installation state of Access Management System when transfer is disabled.
Use case | When checking whether Access Management System is installed
Adj/set/operate method | 1) Select ST-AMS. 2) Enter 0, and then press OK key. When installation has been completed, the transfer license key is displayed under TR-AMS.
Display/adj/set range | When operation finished normally: OK!
Default value | 0
TR-AMS | Transfer license key display of Access Management System
Lv.2 | Details | To display transfer license key to use Access Management System when transfer is disabled.
Use case | - When replacing HDD - When replacing the device
Adj/set/operate method | 1) Select ST-AMS. 2) Enter 0, and then press OK key. The transfer license key is displayed under TR-AMS.
Display/adj/set range | 24 digits
ST-ERDS | Install state dis: E-RDS 3rd Pty Expnsn
Lv.2 | Details | To display installation state of E-RDS 3rd Party Expansion when transfer is disabled.
Use case | When checking whether E-RDS 3rd Party Expansion is installed
Adj/set/operate method | 1) Select ST-ERDS. 2) Enter 0, and then press OK key. When installation has been completed, the transfer license key is displayed under TR-ERDS.
Display/adj/set range | When operation finished normally: OK!
Default value | 0
Supplement/memo | E-RDS 3rd Party Expansion: A function to send charge counter to the third party's charge server.
TR-ERDS | Trns lcns key dis: E-RDS 3rd Pty Expnsn
Lv.2 | Details | To display transfer license key to use E-RDS 3rd Party Expansion when transfer is disabled.
Use case | - When replacing HDD - When replacing the device
Adj/set/operate method | 1) Select ST-ERDS. 2) Enter 0, and then press OK key. The transfer license key is displayed under TR-ERDS.
Display/adj/set range | 24 digits
Supplement/memo | E-RDS 3rd Party Expansion: A function to send charge counter to the third party's charge server.
ST-PS | Install state display of PS function
Lv.2 | Details | To display installation state of PS function when transfer is disabled.
Use case | When checking whether PS function is installed
Adj/set/operate method | 1) Select ST-PS. 2) Enter 0, and then press OK key. When installation has been completed, the transfer license key is displayed under TR-PS.
Display/adj/set range | When operation finished normally: OK!
Default value | 0
TR-PS | Transfer license key display of PS function
Lv.2 | Details | To display transfer license key to use PS function when transfer is disabled.
Use case | - When replacing HDD - When replacing the device
Adj/set/operate method | 1) Select ST-PS. 2) Enter 0, and then press OK key. The transfer license key is displayed under TR-PS.
Display/adj/set range | 24 digits
ST-PCL | Install state display of PCL function
Lv.2 | Details | To display installation state of PCL function when transfer is disabled.
Use case | When checking whether PCL function is installed
Adj/set/operate method | 1) Select ST-PCL. 2) Enter 0, and then press OK key. When installation has been completed, the transfer license key is displayed under TR-PCL.
Display/adj/set range | When operation finished normally: OK!
Default value | 0
TR-PCL | Transfer license key display of PCL function
Lv.2 | Details | To display transfer license key to use PCL function when transfer is disabled.
Use case | - When replacing HDD - When replacing the device
Adj/set/operate method | 1) Select ST-PCL. 2) Enter 0, and then press OK key. The transfer license key is displayed under TR-PCL.
Display/adj/set range | 24 digits
ST-PSLI5 | Install state display:PS/LIPS4/LIPS LX: JP
Lv.2 | Details | To display installation state of PS/LIPS4/LIPS LX function (JP only) when transfer is disabled.
Use case | When checking whether PS/LIPS4/LIPS LX function (JP only) is installed
Adj/set/operate method | 1) Select ST-PSLI5. 2) Enter 0, and then press OK key. When installation has been completed, the transfer license key is displayed under TR-PSLI5.
Display/adj/set range | When operation finished normally: OK!
Default value | 0
TR-PSLI5 | Transfer license key dis:PS/LIPS4/LIPS LX: JP
Lv.2 | Details | To display transfer license key to use PS/LIPS4/LIPS LX function (JP only) when transfer is disabled.
Use case | - When replacing HDD - When replacing the device
Adj/set/operate method | 1) Select ST-PSLI5. 2) Enter 0, and then press OK key. The transfer license key is displayed under TR-PSLI5.
Display/adj/set range | 24 digits
ST-LIPS5 | Install state display:LIPS LX/LIPS4 func: JP
Lv.2 | Details | To display installation state of LIPS LX/LIPS4 function (JP only) when transfer is disabled.
Use case | When checking whether LIPS LX/LIPS4 function (JP only) is installed
Adj/set/operate method | "1) Select ST-LIPS5. 2) Enter 0, and then press OK key. When installation has been completed, the transfer license key is displayed under TR-LIPS5."
Display/adj/set range | When operation finished normally: OK!
Default value | 0
TR-LIPS5 | Transfer license key display:LIPS LX/LIPS4 func: JP
Lv.2 | Details | To display transfer license key to use LIPS LX/LIPS4 function (JP only) when transfer is disabled.
Use case | - When replacing HDD - When replacing the device
Adj/set/operate method | 1) Select ST-LIPS5. 2) Enter 0, and then press OK key. The transfer license key is displayed under TR-LIPS5.
Display/adj/set range | 24 digits
ST-LIPS4 | Install state display of LIPS4 func: JP
Lv.2 | Details | To display installation state of LIPS4 function (JP only) when transfer is disabled.
Use case | When checking whether LIPS4 function (JP only) is installed
Adj/set/operate method | 1) Select ST-LIPS4. 2) Enter 0, and then press OK key. When installation has been completed, the transfer license key is displayed under TR-LIPS4.
Display/adj/set range | When operation finished normally: OK!
Default value | 0
TR-LIPS4 | Trns license key display of LIPS4 func: JP
Lv.2 | Details | To display transfer license key to use LIPS4 function (JP only) when transfer is disabled.
Use case | - When replacing HDD - When replacing the device
Adj/set/operate method | 1) Select ST-LIPS4. 2) Enter 0, and then press OK key. The transfer license key is displayed under TR-LIPS4.
Display/adj/set range | 24 digits
ST-PSPCL | Install state dis of PS/PCL function
Lv.2 | Details | To display installation state of PS/PCL function when transfer is disabled.
Use case | When checking whether PS/PCL function is installed
Adj/set/operate method | 1) Select ST-PSPCL. 2) Enter 0, and then press OK key. When installation has been completed, the transfer license key is displayed under TR-PSPCL.
Display/adj/set range | When operation finished normally: OK!
Default value | 0
TR-PSPCL | Transfer license key dis of PS/PCL func
Lv.2 | Details | To display transfer license key to use PS/PCL function when transfer is disabled.
Use case | - When replacing HDD - When replacing the device
Adj/set/operate method | 1) Select ST-PSPCL. 2) Enter 0, and then press OK key. The transfer license key is displayed under TR-PSPCL.
Display/adj/set range | 24 digits
ST-PCLUF | Install state dis of PCL/UFR II function
Lv.2 | Details | To display installation state of PCL/UFR II function when transfer is disabled.
Use case | When checking whether PCL/UFR II function is installed
Adj/set/operate method | 1) Select ST-PCLUF. 2) Enter 0, and then press OK key. When installation has been completed, the transfer license key is displayed under TR-PCLUF.
Display/adj/set range | When operation finished normally: OK!
Default value | 0
TR-PCLUF | Trns license key dis of PCL/UFR II func
Lv.2 | Details | To display transfer license key to use PCL/UFR II function when transfer is disabled.
Use case | - When replacing HDD - When replacing the device
Adj/set/operate method | 1) Select ST-PCLUF. 2) Enter 0, and then press OK key. The transfer license key is displayed under TR-PCLUF.
Display/adj/set range | 24 digits
ST-PSLIP | Install state dis of PS/LIPS4 func: JP
Lv.2 | Details | To display installation state of PS/LIPS4 function (JP only) when transfer is disabled.
Use case | When checking whether PS/LIPS4 function (JP only) is installed
Adj/set/operate method | 1) Select ST-PSLIP. 2) Enter 0, and then press OK key. When installation has been completed, the transfer license key is displayed under TR-PSLIP.
Display/adj/set range | When operation finished normally: OK!
Default value | 0
TR-PSLIP | Trns license key dis of PS/LIPS4 func:JP
Lv.2 | Details | To display transfer license key to use PS/LIPS4 function (JP only) when transfer is disabled.
Use case | - When replacing HDD - When replacing the device
Adj/set/operate method | 1) Select ST-PSLIP. 2) Enter 0, and then press OK key. The transfer license key is displayed under TR-PSLIP.
Display/adj/set range | 24 digits
ST-PSPCU | Install state dis of PS/PCL/UFR II func
Lv.2 | Details | To display installation state of PS/PCL/UFR II function when transfer is disabled.
Use case | When checking whether PS/PCL/UFR II function is installed
Adj/set/operate method | 1) Select ST-PSPCU. 2) Enter 0, and then press OK key. When installation has been completed, the transfer license key is displayed under TR-PSPCU.
Display/adj/set range | When operation finished normally: OK!
Default value | 0
TR-PSPCU | Trns lcns key dis of PS/PCL/UFR II func
Lv.2 | Details | To display transfer license key to use PS/PCL/UFR II function when transfer is disabled.
Use case | - When replacing HDD - When replacing the device
Adj/set/operate method | 1) Select ST-PSPCU. 2) Enter 0, and then press OK key. The transfer license key is displayed under TR-PSPCU.
Display/adj/set range | 24 digits
ST-LXUFR | Install state dis of UFR II function
Lv.2 | Details | To display installation state of UFR II function when transfer is disabled.
Use case | When checking whether UFR II function is installed
Adj/set/operate method | 1) Select ST-LXUFR. 2) Enter 0, and then press OK key. When installation has been completed, the transfer license key is displayed under TR-LXUFR.
Display/adj/set range | When operation finished normally: OK!
Default value | 0
TR-LXUFR | Trns license key dis of UFR II function
Lv.2 | Details | To display transfer license key to use UFR II function when transfer is disabled.
Use case | - When replacing HDD - When replacing the device
Adj/set/operate method | 1) Select ST-LXUFR. 2) Enter 0, and then press OK key. The transfer license key is displayed under TR-LXUFR.
Display/adj/set range | 24 digits
ST-HDCR2 | Install state dis:HDD Init All Data/Set
Lv.2 | Details | To display installation state of HDD Initialize All Data/Settings when transfer is disabled.
Use case | When checking whether HDD Initialize All Data/Settings is installed
Adj/set/operate method | 1) Select ST-HDCR2. 2) Enter 0, and then press OK key. When installation has been completed, the transfer license key is displayed under TR-HDCR2.
Display/adj/set range | When operation finished normally: OK!
Default value | 0
TR-HDCR2 | Trns lcns key dis:HDD Init All Data/Set
Lv.2 | Details | To display transfer license key to use HDD Initialize All Data/Settings when transfer is disabled.
Use case | - When replacing HDD - When replacing the device
Adj/set/operate method | 1) Select ST-HDCR2. 2) Enter 0, and then press OK key. The transfer license key is displayed under TR-HDCR2.
Display/adj/set range | 24 digits
ST-MOBIL | Install state dis of Mobile Link func:JP
Lv.2 | Details | To display installation state of Mobile Link function (JP only) when transfer is disabled.
Use case | When checking whether Mobile Link function (JP only) is installed
Adj/set/operate method | 1) Select ST-MOBIL. 2) Enter 0, and then press OK key. When installation has been completed, the transfer license key is displayed under TR-MOBIL.
Display/adj/set range | When operation finished normally: OK!
Default value | 0
TR-MOBIL | Trns lcns key dis of Mobile Link func:JP
Lv.2 | Details | To display transfer license key to use Mobile Link function (JP only) when transfer is disabled.
Use case | - When replacing HDD - When replacing the device
Adj/set/operate method | 1) Select ST-MOBIL. 2) Enter 0, and then press OK key. The transfer license key is displayed under TR-MOBIL.
Display/adj/set range | 24 digits
ST-JBLK | Install state dis of Document Scan Lock
Lv.2 | Details | To display installation state of Document Scan Lock when transfer is disabled.
Use case | When checking whether Document Scan Lock is installed
Adj/set/operate method | 1) Select ST-JBLK. 2) Enter 0, and then press OK key. When installation has been completed, the transfer license key is displayed under TR-JBLK.
Display/adj/set range | When operation finished normally: OK!
Default value | 0
TR-JBLK | Trns lcns key dis of Document Scan Lock
Lv.2 | Details | To display transfer license key to use Document Scan Lock when transfer is disabled.
Use case | - When replacing HDD - When replacing the device
Adj/set/operate method | 1) Select ST-JBLK. 2) Enter 0, and then press OK key. The transfer license key is displayed under TR-JBLK.
Display/adj/set range | 24 digits
ST-AFAX | Installation state dis of Remote Fax
Lv.2 | Details | To display installation state of Remote Fax when transfer is disabled.
Use case | When checking whether Remote Fax is installed
Adj/set/operate method | 1) Select ST-AFAX. 2) Enter 0, and then press OK key. When installation has been completed, the transfer license key is displayed under TR-AFAX.
Display/adj/set range | When operation finished normally: OK!
Default value | 0
TR-AFAX | Transfer license key dis of Remote Fax
Lv.2 | Details | To display transfer license key to use Remote Fax when transfer is disabled.
Use case | - When replacing HDD - When replacing the device
Adj/set/operate method | 1) Select ST-AFAX. 2) Enter 0, and then press OK key. The transfer license key is displayed under TR-AFAX.
Display/adj/set range | 24 digits
ST-REPDF | Install state dis:Reader Extensions PDF
Lv.2 | Details | To display installation state of Reader Extensions PDF when transfer is disabled.
Use case | When checking whether Reader Extensions PDF is installed
Adj/set/operate method | 1) Select ST-REPDF. 2) Enter 0, and then press OK key. When installation has been completed, the transfer license key is displayed under TR-REPDF.
Display/adj/set range | When operation finished normally: OK!
Default value | 0
TR-REPDF | Trns lcns key dis:Reader Extensions PDF
Lv.2 | Details | To display transfer license key to use Reader Extensions PDF when transfer is disabled.
Use case | - When replacing HDD - When replacing the device
Adj/set/operate method | 1) Select ST-REPDF. 2) Enter 0, and then press OK key. The transfer license key is displayed under TR-REPDF.
Display/adj/set range | 24 digits
ST-OOXML |  | Install state dis of Office Open XML
Lv.2 | Details | To display installation state of Office Open XML when transfer is disabled.
Use case | When checking whether Office Open XML is installed
Adj/set/operate method | 1) Select ST-OOXML. 2) Enter 0, and then press OK key. When installation has been completed, the transfer license key is displayed under TR-OOXML.
Display/adj/set range | When operation finished normally: OK!
Default value | 0
TR-OOXML | Trns lcns key dis of Office Open XML
Lv.2 | Details | To display transfer license key to use Office Open XML when transfer is disabled.
Use case | - When replacing HDD - When replacing the device
Adj/set/operate method | 1) Select ST-OOXML. 2) Enter 0, and then press OK key. The transfer license key is displayed under TR-OOXML.
Display/adj/set range | 24 digits
ST-XPS | Install state dis of Direct Print XPS
Lv.2 | Details | To display installation state of Direct Print XPS when transfer is disabled.
Use case | When checking whether Direct Print XPS is installed
Adj/set/operate method | 1) Select ST-XPS. 2) Enter 0, and then press OK key. When installation has been completed, the transfer license key is displayed under TR-XPS.
Display/adj/set range | When operation finished normally: OK!
Default value | 0
TR-XPS | Trns lcns key dis of Direct Print XPS
Lv.2 | Details | To display transfer license key to use Direct Print XPS when transfer is disabled.
Use case | - When replacing HDD - When replacing the device
Adj/set/operate method | 1) Select ST-XPS. 2) Enter 0, and then press OK key. The transfer license key is displayed under TR-XPS.
Display/adj/set range | 24 digits
ST-2600 | Instal state dis:HDD data encrypt/mirror
Lv.2 | Details | To display installation state of the HDD data encryption/mirroring kit when transfer is disabled.
Use case | When checking whether the HDD data encryption/mirroring kit is installed
Adj/set/operate method | 1) Select ST-2600. 2) Enter 0, and then press OK key. When installation has been completed, the transfer license key is displayed under TR-2600.
Display/adj/set range | When operation finished normally: OK!
Default value | 0
TR-2600 |  | Trn lcns key dis:HDD data encrypt/mirror
Lv.2 | Details | To display transfer license key of the HDD data encryption/mirroring kit when transfer is disabled.
Use case | - When replacing HDD - When replacing the device
Adj/set/operate method | 1) Select ST-2600. 2) Enter 0, and then press OK key. The transfer license key is displayed under TR-2600.
Display/adj/set range | 24 digits
ST-OPFNT | Install status display of PCL option font
Lv.2 | Details | To display the installation status of PCL option font when transfer is disabled
Use case | When checking whether PCL option font is installed
Adj/set/operate method | 1) Select ST-OPFNT. 2) Enter 0, and then press OK key. The transfer license key is displayed under ST-OPFNT.
Display/adj/set range | 0: Not installed 1: Installed
TR-OPFNT | Trns lcns key display of PCL option font
Lv.2 | Details | To display transfer license key to use PCL option font function with Policy when transfer is disabled.
Use case | - When replacing HDD - When replacing the device
Adj/set/operate method | 1) Select TR-OPFNT. 2) Enter 0, and then press OK key. The transfer license key is displayed under TR-OPFNT.
Display/adj/set range | 24 digits