Installing the System Software Using the SST (Only when installing HDD Data Encryption & Mirroring Kit)

| Print out this category

Installing the System Software Using the SST (Only when installing HDD Data Encryption & Mirroring Kit)
The system data stored on the HDD and used to control the host machine will be lost when the machine is first started up after installing this product.
It is important to install the system software used to control the host machine so that the machine may start up properly after installation of this product.
Details follow.
1. Requirements
1) PC
Service support tool in the version that supports this host machine must be installed.
2) Cross Ethernet Cable
2. Preparing for the Installation of the System Software of Host machine
1) If both PC and the machine are on, turn them off.
2) Connect the PC and the machine using an Cross Ethernet cable.
3) Turn on the PC.
4) Start up the machine in download mode (safe mode).
3. Selecting the System Software
1) Set the CD containing the latest system software in the PC on which the SST is used.
2) Start up the SST.
3) Click Register Firmware.
4) Select the drive in which the System Software CD has been set, and click search.
5) Click REGISTER.
6) Click OK.
4. Downloading the System Software
1) Click "Start Assist Mode" and click "Initialize" according to the instruction on the screen.
2) When initialization is completed, the machine is automatically restarted and it enters download mode.
3) Select the version to be downloaded and click “Start”.
4) When download is completed, the machine is automatically restarted.
5) When writing of the firmware is completed, the machine is automatically restarted.
6) Perform upgrading according to the instruction on the screen. When it is completed, it is automatically restarted.
7) Terminate the SST.
8) Check the version of the downloaded firmware in service mode.