IMG-TR

| Print out this category

IMG-TR

COPIER>OPTION>IMG-TR
HUM-SW | Selection of the level of transfer current output
Lv.2 | Details | Use this item when a failure occurs to the environment sensor. The output level of transfer current is controlled in accordance with the specified environment.
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.

Display/adj/set range

0: Automatic control by the environment sensor
1: Low humidity
2: Rather low humidity
3: Normal humidity
4: Rather high humidity
5: High humidity
Make the setting in accordance with the installation environment.
The transfer current output level is controlled in accordance with the specified environment.
Low-humidity environment: The transfer current output level increases.
High-humidity environment: The transfer current output level decreases.

Default value | 0
TRANS-SW | Switching of the transfer high-voltage control mode
Lv.1 | Details | Switch the transfer high-voltage control mode from fixed current control mode to fixed voltage control mode.
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0: Do not switch the mode. 1: Fixed voltage mode 1 2: Fixed voltage mode 2
Default value | 0
TROPT-SW | Adj of transfer output
Lv.2 | Details | To adjust the transfer roller voltage
Use case | - When the print is executed with the thick paper, index paper or thin paper or of the out-of-specification - When the second page is printed in 2-sided mode with the manual feed table
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | -2: Transfer output voltage moreover decreases. -1: Transfer output voltage decreases. 0: OFF 1: Transfer output voltage increases.
Default value | 0
TR-BS-SW | Set transfer bias highland ev mode
Lv.2 | Details | To control the transfer bias in printing so that it does not exceed a specified level
Use case | When the black spots appear on the image (caused by leak occurs at high latitude)
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: Normal, 1: Voltage reduction mode
Default value | 0