Sharing the authentication information

| Print out this category

Authentication Information Sharing Function
Sharing the authentication information
Authentication information at login and authentication information for MEAP application were managed separately, so it was very inconvenient because authentication was executed many times.
In the MEAP environment, the unified authentication function which authentication information can be shared even between MEAP applications was added.
Supported MEAP Specifications is Ver.59 and both device and MEAP application need to support this version in order to use this function.
There are 2 types for authentication information sharing: Volatile Credential which the registered information is discarded at logout or shutdown of the device, and Persistent Credential which the registered information is not discarded even at logout.