Assembling the Option HDD

| Print out this category

Assembling the Option HDD
1) Remove the HDD from the HDD Fixation Plate Unit. (The removed HDD and the screws will not be used.)
2 Screws
2) Assemble the option HDD.
CAUTION:
Be sure to use the Anti-vibration Damper included in HDD Data Encryption & Mirroring Kit-C4.
Never use the parts included in 2.5inch/250GB HDD-D1.
NOTE:
When tightening the screen, be sure to align the screw holes by lifting the HDD.
1 HDD Support Pate (enclosed with option HDD)
4 Anti-vibration Damper (enclosed with HDD Data Encryption & Mirroring Kit.)
4 Spacers (enclosed with option HDD)
1 Option HDD (enclosed with option HDD)
4 Screws (binding with flat washer; M3X14) (enclosed with option HDD)
CAUTION:
Assembling the option HDD, be careful of the installation direction.
Make sure that the label on the option HDD is facing up.
Make sure that [A] part of HDD Support Plate is placed at the opposite side of connector.