Installation Procedure

| Print out this category

Installation Procedure
1) Open the ADF and remove the Reader Front Cover while pushing the claw at the bottom of the cover.
2 Screws (The removed screws will be used in step 12.)
1 Claw
2) Remove the 2 screws, and shift the Control Panel out of the way of the work.
(The removed screws will be used in step 11.)
2 Bosses
CAUTION:
Be careful not to let the harness come in contact with the plate to prevent the Control Panel or the harness from being damaged.
Be careful not to pull the Control Panel because it is connected with the Control Panel Cable and the Power Supply Cable.
3) Remove the DP Upper Cover.
1 Screw (The removed screw will be used in step 10.)
1 Claw
4) Install the Multimedia Card Slot and the Grounding Plate to the DP Lower Cover Unit.
4 Screws (TP; M3x6)
5) Connect the USB Cable.
6) Remove the Transparent Cover and the DP Sheet of the DP Upper Cover Unit.
2 Screws (The removed screws will be used in step 8.)
7) Affix the Multimedia Label to the DP Sheet.
8) Install the DP Sheet and the Transparent Cover to the DP Upper Cover.
2 Screws (Use the screws removed in step 6.)
9) Remove the Card Slot (closed) from the DP Upper Cover Unit and attach the Card Insertion Slot.
10) Return the DP Upper Cover Unit to its original position. (1 Screw)
11) Return the Control Panel to its original position. (2 Screws)
12) Return the Reader Front Cover to its original position. (2 Screws)
13) Close the DADF.
14) Connect the power plug of the host machine to the outlet.
15) Turn ON the main power switch.