HV-PRI

| Print out this category

HV-PRI

COPIER>ADJUST>HV-PRI
OFST1-DC | Adj primary charge DC offset 1
Lv.1 | Use case | When replacing the DC Controller PCB/clearing RAM data, enter the value of service label.
Adj/set/operate method | Enter the setting value (switch negative/positive by -/+ key) and press OK key.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | -128 to 127
Default value | 0
Use case | When replacing the DC Controller PCB/clearing RAM data, enter the value of service label.
Adj/set/operate method | Enter the setting value (switch negative/positive by -/+ key) and press OK key.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | -128 to 127
Default value | 0